sys=PROCEDURES



devstack=PowerUP

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=electrical power up procedure

&&

[SYSTEMS.ELEC.ACBusAvail]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,electrical power up procedure,-1.000000,

execute=1,Electrical power up procedure,0.000000,

logic:

instring=electrical power up procedure

&&

[SYSTEMS.ELEC.ACBusAvail]!=[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,electrical power up procedure,-1.000000,

execute=1,Captain! AC bus already powered,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Battery,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.BatterySW]==[0.000000]

calc=[0.000000]

execute=2,bat-off,-1.000000,

execute=4,laminar/B738/button_switch_cover02,0.000000,

execute=8,laminar/B738/electric/battery_pos,1.000000,

execute=2,bat-on,0.000000,

logic:

[SYSTEMS.ELEC.BatterySW]==[1.000000]

calc=[0.000000]

execute=2,ovhd-1,-1.000000,

execute=2,bat,-1.000000,

logic:

calc=[0.000000]

out=DomeLight,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_DomeSW]==[0.000000]

&&

[SYSTEMS.TIME.Night_Day]==[1.000000]

calc=[0.000000]

execute=2,domewhite,-1.000000,

execute=4,laminar/B738/toggle_switch/cockpit_dome_dn,0.000000,

execute=2,rest01,-1.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=StandbyPower,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.StanddyPowerCover]!=[0.000000]

calc=[0.000000]

execute=2,stndpower,-1.000000,

execute=2,stby-off,-1.000000,

execute=8,laminar/B738/electric/standby_bat_pos,1.000000,

execute=4,laminar/B738/button_switch_cover03,0.000000,

execute=2,stby-on,0.000000,

logic:

[SYSTEMS.ELEC.StanddyPowerCover]==[0.000000]

calc=[0.000000]

execute=2,stndpower,-1.000000,

logic:

calc=[0.000000]

out=AltFlaps,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.AltFlapCover]==[1.000000]

calc=[0.000000]

execute=2,alterflaps,-1.000000,

execute=4,laminar/B738/toggle_switch/alt_flaps_cover,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.AltFlapCover]==[0.000000]

calc=[0.000000]

execute=2,altflap,-1.000000,

logic:

calc=[0.000000]

out=Wiper1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WiperL]!=[0.000000]

calc=[0.000000]

execute=2,wiper1-low,-1.000000,

execute=4,laminar/B738/knob/left_wiper_dn,0.000000,

execute=4,laminar/B738/knob/left_wiper_dn,0.000000,

execute=4,laminar/B738/knob/left_wiper_dn,0.000000,

execute=2,wiper1-off,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.WiperL]==[0.000000]

calc=[0.000000]

execute=2,wiper1,-1.000000,

logic:

calc=[0.000000]

out=Wiper2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WiperR]!=[0.000000]

calc=[0.000000]

execute=2,wiper2-low,-1.000000,

execute=4,laminar/B738/knob/right_wiper_dn,0.000000,

execute=4,laminar/B738/knob/right_wiper_dn,0.000000,

execute=4,laminar/B738/knob/right_wiper_dn,0.000000,

execute=2,wiper2-off,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.WiperR]==[0.000000]

calc=[0.000000]

execute=2,wiper2,-1.000000,

logic:

calc=[0.000000]

out=Elec2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.ElecPump2]!=[0.000000]

calc=[0.000000]

execute=2,helec2on,-1.000000,

execute=8,laminar/B738/toggle_switch/electric_hydro_pumps1_pos,0.000000,

execute=2,helec2off,0.000000,

logic:

[SYSTEMS.HYD.ElecPump2]==[0.000000]

calc=[0.000000]

execute=2,elec,-1.000000,

logic:

calc=[0.000000]

out=Elec1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.ElecPump1]!=[0.000000]

calc=[0.000000]

execute=2,helec1on,-1.000000,

execute=8,laminar/B738/toggle_switch/electric_hydro_pumps2_pos,0.000000,

execute=2,helec1off,0.000000,

logic:

[SYSTEMS.HYD.ElecPump1]==[0.000000]

calc=[0.000000]

execute=2,elec,-1.000000,

logic:

calc=[0.000000]

out=LgLever,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LG.LG_Lever]!=[1.000000]

calc=[0.000000]

execute=2,lg-off,-1.000000,

execute=8,laminar/B738/controls/gear_handle_down,1.000000,

execute=2,lg-down,0.000000,

logic:

[SYSTEMS.LG.LG_Lever]==[1.000000]

calc=[0.000000]

execute=2,lg,-1.000000,

logic:

calc=[0.000000]

out=GrdPower,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.ExtPwrConnect]==[1.000000]

||

[SYSTEMS.ELEC.JetwayPower]==[1.000000]

&&

[SYSTEMS.ELEC.ExtPwrSW]==[0.000000]

calc=[2.000000]

execute=2,grd-ctrl,-1.000000,

execute=8,sim/cockpit/electrical/gpu_on,1.000000,

execute=8,laminar/B738/electrical/gpu_pos,1.000000,

execute=4,laminar/B738/toggle_switch/gpu_dn,0.000000,

execute=2,grd-on,0.000000,

execute=1,Electrical power up procedure complete,0.000000,

execute=3,,0.000000,

logic:

[SYSTEMS.ELEC.ExtPwrConnect]==[1.000000]

||

[SYSTEMS.ELEC.JetwayPower]==[1.000000]

&&

[SYSTEMS.ELEC.ExtPwrSW]==[1.000000]

calc=[0.000000]

execute=2,gndpower,-1.000000,

logic:

[SYSTEMS.ELEC.ExtPwrConnect]==[0.000000]

||

[SYSTEMS.ELEC.JetwayPower]<=[0.000000]

calc=[0.000000]

execute=10,not_define,0.000000,

logic:

calc=[0.000000]

out=FireIn,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FIRE.Eng1FirePB]==[1.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

execute=1,Sir; engine one fire switch is not in,0.000000,

execute=1,Electrical power up procedure is not complete,0.000000,

execute=3,,0.000000,

logic:

[SYSTEMS.FIRE.Eng2FirePB]==[1.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

execute=1,Sir; engine two fire switch is not in,0.000000,

execute=1,Electrical power up procedure is not complete,0.000000,

execute=3,,0.000000,

logic:

[SYSTEMS.FIRE.APUFirePB]==[1.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

execute=1,Sir; APU fire switch is not in,0.000000,

execute=1,Electrical power up procedure is not complete,0.000000,

execute=3,,0.000000,

logic:

[SYSTEMS.FIRE.Eng1FirePB]==[0.000000]

&&

[SYSTEMS.FIRE.Eng2FirePB]==[0.000000]

&&

[SYSTEMS.FIRE.APUFirePB]==[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[0.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

execute=0,A P U Fire test,0.000000,

execute=2,apu-fire,-1.000000,

execute=5,laminar/B738/toggle_switch/fire_test_lft,0.000000,

execute=7,,1.000000,

execute=2,apu-fire1,-1.000000,

execute=7,,1.000000,

execute=2,apu-fire,-1.000000,

execute=7,,1.000000,

execute=6,laminar/B738/toggle_switch/fire_test_lft,0.000000,

execute=2,apu-fire,-1.000000,

execute=5,laminar/B738/toggle_switch/fire_test_rgt,0.000000,

execute=7,,2.000000,

execute=2,apu-fire1,-1.000000,

execute=7,,1.000000,

execute=2,apu-fire2,-1.000000,

execute=5,laminar/B738/push_button/fire_bell_light2,0.000000,

execute=8,laminar/B738/push_button/fire_bell_cutout2,0.000000,

execute=7,,1.000000,

execute=6,laminar/B738/push_button/fire_bell_light2,0.000000,

execute=2,apu-fire,-1.000000,

execute=7,,1.000000,

execute=6,laminar/B738/toggle_switch/fire_test_rgt,0.000000,

execute=2,ext-test,-1.000000,

execute=5,laminar/B738/toggle_switch/exting_test_lft,0.000000,

execute=7,,1.000000,

execute=6,laminar/B738/toggle_switch/exting_test_lft,0.000000,

execute=5,laminar/B738/toggle_switch/exting_test_rgt,0.000000,

execute=7,,1.000000,

execute=6,laminar/B738/toggle_switch/exting_test_rgt,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=ApuStart,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.APU.AvailAPU]==[1.000000]

calc=[0.000000]

execute=2,apu,-1.000000,

logic:

[SYSTEMS.APU.AvailAPU]==[0.000000]

&&

[SYSTEMS.APU.StartSW]==[0.000000]

calc=[0.000000]

execute=2,apu-off,-1.000000,

execute=4,laminar/B738/spring_toggle_switch/APU_start_pos_dn,0.000000,

execute=2,apu-cntr,0.000000,

execute=2,ovhd-dn,-1.000000,

execute=7,,10.000000,

execute=2,apu-cntr,-1.000000,

execute=8,laminar/B738/spring_toggle_switch/APU_start_pos,2.000000,

execute=4,laminar/B738/spring_toggle_switch/APU_start_pos_dn,0.000000,

execute=2,apu-start,0.000000,

execute=0,Waiting for start A P U!,0.000000,

execute=2,ovhd-dn,-1.000000,

logic:

[SYSTEMS.APU.AvailAPU]==[0.000000]

&&

[SYSTEMS.APU.StartSW]==[1.000000]

calc=[0.000000]

execute=2,apu-cntr,-1.000000,

execute=4,laminar/B738/spring_toggle_switch/APU_start_pos_dn,0.000000,

execute=2,apu-start,0.000000,

execute=0,Waiting for start A P U!,0.000000,

execute=2,ovhd-dn,-1.000000,

logic:

calc=[0.000000]

out=ApuGenOffAnn,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.APU.ApuGenOff_Ann]!=[0.000000]

||

[SYSTEMS.ELEC.ACBusAvail]!=[0.000000]

calc=[0.000000]

execute=10,not_define,0.000000,

logic:

calc=[0.000000]

out=ApuGen1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.APU.ApuGenOff_Ann]!=[0.000000]

||

[SYSTEMS.ELEC.SourceIndLeft]!=[0.000000]

calc=[0.000000]

execute=2,apu1-cntr,-1.000000,

execute=4,laminar/B738/toggle_switch/apu_gen1_dn,0.000000,

execute=8,laminar/B738/electrical/apu_gen1_pos,1.000000,

execute=2,apu1-on,0.000000,

execute=7,,0.300000,

execute=8,laminar/B738/electrical/apu_gen1_pos,0.000000,

logic:

[SYSTEMS.ELEC.APUGen1Bus]==[1.000000]

&&

[SYSTEMS.ELEC.SourceIndLeft]==[0.000000]

calc=[0.000000]

execute=2,gencheck,-1.000000,

logic:

calc=[0.000000]

out=ApuGen2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.APU.ApuGenOff_Ann]!=[0.000000]

||

[SYSTEMS.ELEC.SourceIndRight]!=[0.000000]

calc=[0.000000]

execute=2,apu2-cntr,-1.000000,

execute=4,laminar/B738/toggle_switch/apu_gen2_dn,0.000000,

execute=8,laminar/B738/electrical/apu_gen2_pos,1.000000,

execute=2,apu2-on,0.000000,

execute=7,,0.300000,

execute=8,laminar/B738/electrical/apu_gen2_pos,0.000000,

logic:

[SYSTEMS.ELEC.APUGen2Bus]==[1.000000]

&&

[SYSTEMS.ELEC.SourceIndRight]==[0.000000]

calc=[0.000000]

execute=2,gencheck,-1.000000,

logic:

calc=[0.000000]

out=Pump1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LAftPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,aft-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft1,0.000000,

execute=2,aft-l-off,0.000000,

logic:

calc=[0.000000]

execute=2,f-aft-l,-1.000000,

out=Pump2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]!=[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[0.000000]

calc=[0.000000]

execute=2,fwd-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft2,0.000000,

execute=2,fwd-l-off,0.000000,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]==[1.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]<[200.000000]

calc=[0.000000]

execute=2,f-fwd-l,-1.000000,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]==[1.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]>[200.000000]

calc=[0.000000]

execute=2,fwd-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft2,0.000000,

execute=2,fwd-l-off,0.000000,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]==[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]<[200.000000]

calc=[0.000000]

execute=2,fwd-l-off,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft2,1.000000,

execute=2,fwd-l-on,0.000000,

logic:

calc=[0.000000]

execute=2,f-fwd-l,-1.000000,

out=Pump3,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RFwdPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,fwd-r-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_rgt2,0.000000,

execute=2,fwd-r-off,0.000000,

logic:

calc=[0.000000]

execute=2,f-fwd-r,-1.000000,

out=Pump4,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RAftPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,aft-r-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_rgt1,0.000000,

execute=2,aft-r-off,0.000000,

logic:

calc=[0.000000]

execute=2,f-aft-r,-1.000000,

out=Pump5,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LCtrPumpSW]!=[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[0.000000]

calc=[0.000000]

execute=2,ctr-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr1,0.000000,

execute=2,ctr-l-off,0.000000,

logic:

[SYSTEMS.FUEL.LCtrPumpSW]==[1.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]>[200.000000]

calc=[0.000000]

execute=2,f-ctr-l,-1.000000,

logic:

[SYSTEMS.FUEL.LCtrPumpSW]==[1.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]<[200.000000]

calc=[0.000000]

execute=2,ctr-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr1,0.000000,

execute=2,ctr-l-off,0.000000,

logic:

[SYSTEMS.FUEL.LCtrPumpSW]==[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]>[200.000000]

calc=[0.000000]

execute=2,ctr-l-off,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr1,1.000000,

execute=2,ctr-l-on,0.000000,

logic:

calc=[0.000000]

execute=2,f-ctr-l,-1.000000,

out=Pump6,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RCtrPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,ctr-r-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr2,0.000000,

execute=2,ctr-r-off,0.000000,

logic:

calc=[0.000000]

execute=2,f-ctr-r,-1.000000,

out=BusTrans,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.BasTransCover]==[0.000000]

&&

[SYSTEMS.ELEC.BusTransSW]==[1.000000]

calc=[0.000000]

execute=2,elec,-1.000000,

logic:

[SYSTEMS.ELEC.BasTransCover]==[0.000000]

&&

[SYSTEMS.ELEC.BusTransSW]==[0.000000]

calc=[0.000000]

execute=2,busoff,-1.000000,

execute=4,laminar/B738/button_switch_cover06,0.000000,

execute=8,sim/cockpit2/electrical/cross_tie,1.000000,

execute=7,,1.000000,

execute=4,laminar/B738/button_switch_cover06,0.000000,

execute=2,buson,-1.000000,

logic:

[SYSTEMS.ELEC.BasTransCover]==[1.000000]

&&

[0.000000]==[1.000000]

calc=[0.000000]

execute=2,bus-off,-1.000000,

execute=4,laminar/B738/button_switch_cover06,0.000000,

execute=2,bus-on,0.000000,

logic:

[SYSTEMS.ELEC.BasTransCover]==[1.000000]

&&

[SYSTEMS.ELEC.BusTransSW]==[0.000000]

calc=[0.000000]

execute=2,bus-off,-1.000000,

execute=8,sim/cockpit2/electrical/cross_tie,1.000000,

execute=4,laminar/B738/button_switch_cover06,0.000000,

execute=2,bus-on,0.000000,

logic:

calc=[0.000000]

out=TestInop,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

execute=2,apu-fire,-1.000000,

execute=5,laminar/B738/toggle_switch/fire_test_rgt,0.000000,

execute=7,,1.000000,

execute=2,apu-fire1,-1.000000,

execute=7,,2.000000,

execute=2,apu-fire,-1.000000,

execute=7,,1.000000,

execute=5,laminar/B738/toggle_switch/fire_test_rgt,0.000000,

execute=6,laminar/B738/toggle_switch/fire_test_rgt,0.000000,

logic:

calc=[0.000000]

out=NavLight,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_NavSW]==[0.000000]

calc=[0.000000]

execute=2,strobe-off,-1.000000,

execute=4,laminar/B738/toggle_switch/position_light_down,0.000000,

execute=2,strobe-nav,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_NavSW]==[1.000000]

calc=[0.000000]

execute=2,strobe-on,-1.000000,

execute=4,laminar/B738/toggle_switch/position_light_down,0.000000,

execute=4,laminar/B738/toggle_switch/position_light_down,0.000000,

execute=2,strobe-nav,0.000000,

logic:

calc=[0.000000]

execute=2,nav,-1.000000,

out=Logo,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_LogoSW]!=[1.000000]

&&

[SYSTEMS.TIME.Night_Day]==[1.000000]

calc=[0.000000]

execute=2,logo-off,-1.000000,

execute=8,laminar/B738/toggle_switch/logo_light,1.000000,

execute=2,logo-on,0.000000,

logic:

calc=[0.000000]

execute=2,logolight,-1.000000,

out=BrightPanelOvhd,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.TIME.Night_Day]==[1.000000]

&&

[SYSTEMS.LIGHTS.OVHD_Panel]<[0.800000]

calc=[0.000000]

execute=2,panel-off,-1.000000,

execute=8,laminar/B738/electric/panel_brightness[2],0.300000,

execute=7,,0.100000,

execute=8,laminar/B738/electric/panel_brightness[2],0.500000,

execute=7,,0.100000,

execute=8,laminar/B738/electric/panel_brightness[2],1.000000,

execute=2,panel-on,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=ManPanelLight,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.PFD_Panel]==[0.000000]

&&

[SYSTEMS.TIME.Night_Day]==[1.000000]

calc=[0.000000]

execute=2,main-l-off,-1.000000,

execute=8,laminar/B738/electric/panel_brightness[1],0.000000,

execute=7,,0.200000,

execute=8,laminar/B738/electric/panel_brightness[1],0.500000,

execute=7,,0.200000,

execute=8,laminar/B738/electric/panel_brightness[1],1.000000,

execute=2,main-l-on,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=PedPanelLight,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.TIME.Night_Day]==[1.000000]

&&

[SYSTEMS.LIGHTS.PED_Panel]<[0.800000]

calc=[0.000000]

execute=2,ped-l-off,-1.000000,

execute=8,laminar/B738/electric/panel_brightness[3],0.000000,

execute=7,,0.100000,

execute=8,laminar/B738/electric/panel_brightness[3],0.500000,

execute=7,,0.100000,

execute=8,laminar/B738/electric/panel_brightness[3],1.000000,

execute=2,ped-l-on,-1.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=WHeat1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WHeatLSide]!=[1.000000]

&&

[SYSTEMS.WEATHER.SAT]<=[10.000000]

calc=[0.000000]

execute=2,wh1-off,0.500000,

execute=4,laminar/B738/toggle_switch/window_heat_l_side,0.000000,

execute=2,wh1-on,0.000000,

logic:

calc=[0.000000]

execute=2,wh1,-1.000000,

out=WHeat2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WHeatLFwd]!=[1.000000]

&&

[SYSTEMS.WEATHER.SAT]<=[10.000000]

calc=[0.000000]

execute=2,wh2-off,0.500000,

execute=4,laminar/B738/toggle_switch/window_heat_l_fwd,0.000000,

execute=2,wh2-on,0.000000,

logic:

calc=[0.000000]

execute=2,wh2,-1.000000,

out=WHeat3,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WHeatRFwd]!=[1.000000]

&&

[SYSTEMS.WEATHER.SAT]<=[10.000000]

calc=[0.000000]

execute=2,wh3-off,0.500000,

execute=4,laminar/B738/toggle_switch/window_heat_r_fwd,0.000000,

execute=2,wh3-on,0.000000,

logic:

calc=[0.000000]

execute=2,wh3,-1.000000,

out=WHeat4,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WHeatRSide]!=[1.000000]

&&

[SYSTEMS.WEATHER.SAT]<=[10.000000]

calc=[0.000000]

execute=2,wh4-off,0.500000,

execute=4,laminar/B738/toggle_switch/window_heat_r_side,0.000000,

execute=2,wh4-on,0.000000,

logic:

calc=[0.000000]

execute=2,wh4,-1.000000,

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,electrical power up procedure,-1.000000,

execute=1,Electrical power up procedure complete,0.000000,

logic:

calc=[0.000000]



devstack=PrelimPreflight

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDUP.IRS_L]!=[2.000000]

||

[SYSTEMS.OVHDUP.IRS_R]!=[2.000000]

&&

[SYSTEMS.POSITION.onGround]==[1.000000]

&&

[SYSTEMS.MISC.PowerPlus4Min]>=[8550.000000]

&&

[SYSTEMS.ELEC.ACBusAvail]==[2.000000]

&&

[SYSTEMS.POSITION.WasInAir]==[0.000000]

&&

[SYSTEMS.COPILOT.doPM_JobOnly]==[0.000000]

&&

[SYSOLD.Procedure.Preliminary]==[0.000000]

calc=[0.000000]

execute=12,preliminary preflight procedure,-1.000000,

execute=2,answer01,-1.000000,

execute=0,Preliminary preflight procedure,0.000000,

execute=2,ovhd-up,-1.000000,

logic:

instring=preliminary preflight procedure

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,electrical power up procedure,-1.000000,

execute=12,preliminary preflight procedure,-1.000000,

execute=0,Preliminary preflight procedure,0.000000,

execute=2,ovhd-up,-1.000000,

logic:

calc=[0.000000]

out=Irs1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDUP.IRS_L]==[0.000000]

calc=[0.000000]

execute=2,irs-l-off,-1.000000,

execute=4,laminar/B738/toggle_switch/irs_L_right,0.000000,

execute=4,laminar/B738/toggle_switch/irs_L_right,0.000000,

execute=2,irs-l-nav,0.000000,

logic:

[SYSTEMS.OVHDUP.IRS_L]==[1.000000]

calc=[0.000000]

execute=2,irs-l-off,-1.000000,

execute=4,laminar/B738/toggle_switch/irs_L_right,0.000000,

execute=2,irs-l-nav,0.000000,

logic:

[SYSTEMS.OVHDUP.IRS_L]==[2.000000]

calc=[0.000000]

execute=2,idrs,-1.000000,

logic:

[SYSTEMS.OVHDUP.IRS_L]==[3.000000]

calc=[0.000000]

execute=2,irs-l-nav,-1.000000,

execute=4,laminar/B738/toggle_switch/irs_L_left,0.000000,

execute=2,irs-l-off,0.000000,

logic:

calc=[0.000000]

out=Irs2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDUP.IRS_R]==[0.000000]

calc=[0.000000]

execute=2,irs-r-off,-1.000000,

execute=4,laminar/B738/toggle_switch/irs_R_right,0.000000,

execute=4,laminar/B738/toggle_switch/irs_R_right,0.000000,

execute=2,irs-r-nav,0.000000,

logic:

[SYSTEMS.OVHDUP.IRS_R]==[1.000000]

calc=[0.000000]

execute=2,irs-r-off,-1.000000,

execute=4,laminar/B738/toggle_switch/irs_R_right,0.000000,

execute=2,irs-r-nav,0.000000,

logic:

[SYSTEMS.OVHDUP.IRS_R]==[2.000000]

calc=[0.000000]

execute=2,idrs,-1.000000,

logic:

[SYSTEMS.OVHDUP.IRS_R]==[3.000000]

calc=[0.000000]

execute=2,irs-r-nav,-1.000000,

execute=4,laminar/B738/toggle_switch/irs_R_left,0.000000,

execute=2,irs-r-off,0.000000,

logic:

calc=[0.000000]

out=VoiceRecorder,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDER.VoiceRecorder]==[1.000000]

calc=[0.000000]

execute=2,ovhd-5,-1.000000,

logic:

[SYSTEMS.OVHDSIDER.VoiceRecorder]==[0.000000]

calc=[0.000000]

execute=2,voice-off,-1.000000,

execute=4,laminar/B738/toggle_switch/vcr_on,0.000000,

execute=2,voice-on,0.000000,

logic:

calc=[0.000000]

out=HydQtySys,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FRONTPANEL.SysPage]==[0.000000]

calc=[0.000000]

execute=2,look-cdu,-1.000000,

execute=2,sys-page,-1.000000,

execute=4,laminar/B738/LDU_control/push_button/MFD_SYS,0.000000,

execute=2,look-cdu,-1.000000,

execute=7,,2.000000,

logic:

[SYSTEMS.FRONTPANEL.SysPage]==[1.000000]

calc=[0.000000]

execute=2,look-cdu,-1.000000,

execute=7,,2.000000,

logic:

calc=[0.000000]

out=HydQty,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.HydQty_A]<[65.000000]

&&

[SYSTEMS.FRONTPANEL.SysPage]==[0.000000]

calc=[0.000000]

execute=2,look-cdu,-1.000000,

execute=2,sys-page,-1.000000,

execute=4,laminar/B738/LDU_control/push_button/MFD_SYS,0.000000,

execute=2,look-cdu,-1.000000,

execute=1,Sir; hydraulic quantity is to low,0.000000,

logic:

[SYSTEMS.HYD.HydQty_A]<[65.000000]

&&

[SYSTEMS.FRONTPANEL.SysPage]==[1.000000]

calc=[0.000000]

execute=2,look-cdu,-1.000000,

execute=1,Sir; hydraulic quantity is to low,0.000000,

logic:

[SYSTEMS.HYD.HydQty_B]<[65.000000]

&&

[SYSTEMS.FRONTPANEL.SysPage]==[0.000000]

calc=[0.000000]

execute=2,look-cdu,-1.000000,

execute=2,sys-page,-1.000000,

execute=4,laminar/B738/LDU_control/push_button/MFD_SYS,0.000000,

execute=2,look-cdu,-1.000000,

execute=1,Sir; hydraulic quantity is to low,0.000000,

logic:

[SYSTEMS.HYD.HydQty_B]<[65.000000]

&&

[SYSTEMS.FRONTPANEL.SysPage]==[1.000000]

calc=[0.000000]

execute=2,look-cdu,-1.000000,

execute=1,Sir; hydraulic quantity is to low,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=EmerEquip,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,look-back,-1.000000,

execute=7,,2.000000,

execute=2,look-back1,-1.000000,

execute=7,,2.000000,

execute=2,look-frd,-1.000000,

logic:

calc=[0.000000]

out=EltSW,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDUP.EltCover]!=[0.000000]

calc=[0.000000]

execute=2,elt,-1.000000,

execute=4,laminar/B738/button_switch_cover08,0.000000,

logic:

[SYSTEMS.OVHDUP.EltCover]==[0.000000]

calc=[0.000000]

execute=2,elt-arm,-1.000000,

logic:

calc=[0.000000]

out=ServInter,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDUP.ServiceInter]==[1.000000]

calc=[0.000000]

execute=2,interphone,-1.000000,

execute=8,laminar/B738/toggle_switch/service_interphone,0.000000,

logic:

[SYSTEMS.OVHDUP.ServiceInter]==[0.000000]

calc=[0.000000]

execute=2,interphon,-1.000000,

logic:

calc=[0.000000]

out=ReversAnn,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Revers1annunc]==[1.000000]

calc=[0.000000]

execute=2,ovhd-up,-1.000000,

execute=1,Sir; we have a problem with the reverse,0.000000,

logic:

[SYSTEMS.ENGINE.Revers2annunc]==[1.000000]

calc=[0.000000]

execute=2,ovhd-up,-1.000000,

execute=1,Sir; we have a problem with the reverse,0.000000,

logic:

[SYSTEMS.ENGINE.Revers1annunc]==[1.000000]

&&

[SYSTEMS.ENGINE.Revers2annunc]==[1.000000]

calc=[0.000000]

execute=2,ovhd-up,-1.000000,

execute=1,Sir; we have a problem with the reverse,0.000000,

logic:

[SYSTEMS.ENGINE.Revers1annunc]==[0.000000]

&&

[SYSTEMS.ENGINE.Revers2annunc]==[0.000000]

calc=[0.000000]

execute=2,eec,-1.000000,

logic:

calc=[0.000000]

out=EEC1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.EEC1]==[0.000000]

&&

[SYSTEMS.ENGINE.EEC1Cover]==[0.000000]

calc=[0.000000]

execute=2,eec-1,-1.000000,

execute=4,laminar/B738/button_switch_cover00,0.000000,

execute=7,,1.000000,

execute=8,sim/cockpit2/engine/actuators/fadec_on[0],1.000000,

execute=4,laminar/B738/button_switch_cover00,0.000000,

logic:

[SYSTEMS.ENGINE.EEC1]==[0.000000]

&&

[SYSTEMS.ENGINE.EEC1Cover]==[1.000000]

calc=[0.000000]

execute=2,eec-1,-1.000000,

execute=8,sim/cockpit2/engine/actuators/fadec_on[0],1.000000,

execute=4,laminar/B738/button_switch_cover00,0.000000,

logic:

[SYSTEMS.ENGINE.EEC1]==[1.000000]

&&

[SYSTEMS.ENGINE.EEC1Cover]==[0.000000]

calc=[0.000000]

execute=2,eec,-1.000000,

logic:

[SYSTEMS.ENGINE.EEC1]==[1.000000]

&&

[SYSTEMS.ENGINE.EEC1Cover]==[1.000000]

calc=[0.000000]

execute=2,eec-1,-1.000000,

execute=4,laminar/B738/button_switch_cover00,0.000000,

logic:

calc=[0.000000]

out=EEC2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.EEC2]==[0.000000]

&&

[SYSTEMS.ENGINE.EEC2Cover]==[0.000000]

calc=[0.000000]

execute=2,eec-2,-1.000000,

execute=4,laminar/B738/button_switch_cover01,0.000000,

execute=7,,1.000000,

execute=8,sim/cockpit2/engine/actuators/fadec_on[1],1.000000,

execute=4,laminar/B738/button_switch_cover01,0.000000,

logic:

[SYSTEMS.ENGINE.EEC2]==[0.000000]

&&

[SYSTEMS.ENGINE.EEC2Cover]==[1.000000]

calc=[0.000000]

execute=2,eec-2,-1.000000,

execute=8,sim/cockpit2/engine/actuators/fadec_on[1],1.000000,

execute=4,laminar/B738/button_switch_cover01,0.000000,

logic:

[SYSTEMS.ENGINE.EEC2]==[1.000000]

&&

[SYSTEMS.ENGINE.EEC2Cover]==[0.000000]

calc=[0.000000]

execute=2,eec,-1.000000,

logic:

[SYSTEMS.ENGINE.EEC2]==[1.000000]

&&

[SYSTEMS.ENGINE.EEC2Cover]==[1.000000]

calc=[0.000000]

execute=2,eec-2,-1.000000,

execute=4,laminar/B738/button_switch_cover01,0.000000,

logic:

calc=[0.000000]

out=PassOxy,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDUP.PassOxyCover]==[0.000000]

calc=[0.000000]

execute=2,oxy-check,-1.000000,

logic:

[SYSTEMS.OVHDUP.PassOxyCover]==[1.000000]

calc=[0.000000]

execute=2,pass-oxy,-1.000000,

execute=4,laminar/B738/button_switch_cover07,0.000000,

logic:

calc=[0.000000]

out=FlightRecor,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDUP.FlightRecorCover]==[1.000000]

&&

[SYSTEMS.OVHDUP.FlightRecor]==[0.000000]

calc=[0.000000]

execute=2,recordtest,-1.000000,

execute=4,laminar/B738/toggle_switch/fdr,0.000000,

execute=7,,1.000000,

execute=2,flrecorder,-1.000000,

execute=4,laminar/B738/toggle_switch/fdr_cover,0.000000,

logic:

[SYSTEMS.OVHDUP.FlightRecorCover]==[0.000000]

calc=[0.000000]

execute=2,flrecorder,-1.000000,

execute=4,laminar/B738/toggle_switch/fdr_cover,0.000000,

execute=2,recordtest,-1.000000,

execute=4,laminar/B738/toggle_switch/fdr,0.000000,

execute=7,,1.000000,

execute=2,flrecorder,-1.000000,

execute=4,laminar/B738/toggle_switch/fdr_cover,0.000000,

logic:

[SYSTEMS.OVHDUP.FlightRecorCover]==[1.000000]

&&

[SYSTEMS.OVHDUP.FlightRecor]==[1.000000]

calc=[0.000000]

execute=2,flrecorder,-1.000000,

execute=4,laminar/B738/toggle_switch/fdr_cover,0.000000,

logic:

calc=[0.000000]

out=MachAir,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,airspeed1,-1.000000,

execute=5,laminar/B738/push_button/mach_warn1_test,0.000000,

execute=7,,3.000000,

execute=6,laminar/B738/push_button/mach_warn1_test,0.000000,

execute=2,airspeed2,-1.000000,

execute=5,laminar/B738/push_button/mach_warn2_test,0.000000,

execute=7,,3.000000,

execute=6,laminar/B738/push_button/mach_warn2_test,0.000000,

logic:

calc=[0.000000]

out=Stall,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,stall-1,-1.000000,

execute=5,laminar/B738/push_button/stall_test1_press,0.000000,

execute=7,,3.000000,

execute=6,laminar/B738/push_button/stall_test1_press,0.000000,

execute=2,stall-2,-1.000000,

execute=5,laminar/B738/push_button/stall_test2_press,0.000000,

execute=7,,3.000000,

execute=6,laminar/B738/push_button/stall_test2_press,0.000000,

logic:

calc=[0.000000]

out=ParkBrake,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.BRAKES.ParkBrakeHandlePos]==[0.000000]

calc=[0.000000]

execute=2,parkb-off,-1.000000,

execute=8,sim/flightmodel/controls/parkbrake,1.000000,

execute=8,laminar/B738/parking_brake_pos,1.000000,

execute=2,parkb-on,0.000000,

execute=0,Parking brake Set!,0.000000,

logic:

[SYSTEMS.BRAKES.ParkBrakeHandlePos]==[1.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

execute=0,Park Brake Set!,0.000000,

logic:

calc=[0.000000]

out=FlightDeck,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MISC.DeckDoor]>[0.000000]

calc=[0.000000]

execute=2,look-back,-1.000000,

execute=7,,0.200000,

execute=4,laminar/B738/toggle_switch/flt_dk_door_open,0.000000,

execute=7,,1.500000,

execute=2,look-ped,-1.000000,

execute=7,,1.000000,

logic:

[SYSTEMS.MISC.DeckDoor]==[0.000000]

calc=[0.000000]

execute=2,look-back,-1.000000,

execute=7,,0.200000,

execute=2,look-ped,-1.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,preliminary preflight procedure,-1.000000,

execute=1,Preliminary preflight procedure complete,0.000000,

execute=2,look-front,-1.000000,

execute=0,Enter the data in the C D U!,0.000000,

logic:

calc=[0.000000]



devstack=Preflight

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FMS.GWCDU]>[0.000000]

||

[SYSTEMS.FMS.FlightPlane]>[0.000000]

&&

[SYSTEMS.OVHDUP.IRS_L]==[2.000000]

&&

[SYSTEMS.OVHDUP.IRS_R]==[2.000000]

&&

[SYSTEMS.POSITION.onGround]==[1.000000]

&&

[SYSTEMS.ENGINE.EngsRun]==[0.000000]

&&

[SYSTEMS.COPILOT.doPM_JobOnly]==[0.000000]

&&

[SYSTEMS.FMS.V1]>[100.000000]

&&

[SYSTEMS.FMS.VR]>[100.000000]

&&

[SYSTEMS.FMS.V2]>[100.000000]

&&

[SYSOLD.Procedure.PreflightStart]==[0.000000]

calc=[1.000000]

execute=12,preflight procedure,-1.000000,

execute=0,Preflight procedure,0.000000,

logic:

instring=preflight procedure

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=1,Preflight procedure,0.000000,

execute=12,preflight procedure,-1.000000,

logic:

calc=[0.000000]

out=FltContrA,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.FltContrA]==[1.000000]

calc=[0.000000]

execute=2,flt-cont-a,-1.000000,

execute=4,laminar/B738/toggle_switch/flt_ctr_A_cover,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.FltContrA]==[0.000000]

calc=[0.000000]

execute=2,fltcontrol,-1.000000,

logic:

calc=[0.000000]

out=FlControlB,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.FltContrB]==[1.000000]

calc=[0.000000]

execute=2,flt-cont-b,-1.000000,

execute=4,laminar/B738/toggle_switch/flt_ctr_B_cover,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.SpoilerB]==[0.000000]

calc=[0.000000]

execute=2,fltcontrol,-1.000000,

logic:

calc=[0.000000]

out=AltFlaps,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.AltFlapCover]==[1.000000]

calc=[0.000000]

execute=2,alterflaps,-1.000000,

execute=4,laminar/B738/toggle_switch/alt_flaps_cover,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.AltFlapCover]==[0.000000]

calc=[0.000000]

execute=2,altflap,-1.000000,

logic:

calc=[0.000000]

out=SpoilerA,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.SpoilerA]==[1.000000]

calc=[0.000000]

execute=2,spoiler-a,-1.000000,

execute=4,laminar/B738/toggle_switch/spoiler_A_cover,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.SpoilerA]==[0.000000]

calc=[0.000000]

execute=2,spoiler-ab,-1.000000,

logic:

calc=[0.000000]

out=SpoilerB,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.SpoilerB]==[1.000000]

calc=[0.000000]

execute=2,spoiler-b,-1.000000,

execute=4,laminar/B738/toggle_switch/spoiler_B_cover,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.SpoilerB]==[0.000000]

calc=[0.000000]

execute=2,spoiler-ab,-1.000000,

logic:

calc=[0.000000]

out=YawDamper,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.YawDamper]==[0.000000]

calc=[0.000000]

execute=2,yaw-off,-1.000000,

execute=4,laminar/B738/toggle_switch/yaw_dumper,0.000000,

execute=2,yaw-on,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.YawDamper]==[1.000000]

calc=[0.000000]

execute=2,yawdamper,-1.000000,

logic:

calc=[0.000000]

out=VhfNav,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.VhfNavSource]>[0.000000]

calc=[0.000000]

execute=2,vhf-nav,-1.000000,

execute=4,laminar/B738/toggle_switch/vhf_nav_source_lft,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.VhfNavSource]<[0.000000]

calc=[0.000000]

execute=2,vhf-nav,-1.000000,

execute=4,laminar/B738/toggle_switch/vhf_nav_source_rgt,0.000000,

logic:

calc=[0.000000]

execute=2,vhf-disp,-1.000000,

out=Irs,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.IrsSource]>[0.000000]

calc=[0.000000]

execute=2,irs,-1.000000,

execute=4,laminar/B738/toggle_switch/irs_source_left,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.IrsSource]<[0.000000]

calc=[0.000000]

execute=2,irs,-1.000000,

execute=4,laminar/B738/toggle_switch/irs_source_right,0.000000,

logic:

calc=[0.000000]

execute=2,irs-disp,-1.000000,

out=Fmc,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.FmcSource]>[0.000000]

calc=[0.000000]

execute=2,fmc,-1.000000,

execute=4,laminar/B738/toggle_switch/fmc_source_left,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.FmcSource]<[0.000000]

calc=[0.000000]

execute=2,fmc,-1.000000,

execute=4,laminar/B738/toggle_switch/fmc_source_right,0.000000,

logic:

calc=[0.000000]

execute=2,irs-disp,-1.000000,

out=Source,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.SourceAuto]>[0.000000]

calc=[0.000000]

execute=2,source,-1.000000,

execute=4,laminar/B738/toggle_switch/dspl_source_left,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.SourceAuto]<[0.000000]

calc=[0.000000]

execute=2,source,-1.000000,

execute=4,laminar/B738/toggle_switch/dspl_source_right,0.000000,

logic:

calc=[0.000000]

execute=2,cp-disp,-1.000000,

out=CtrPanel,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.ControlSource]>[0.000000]

calc=[0.000000]

execute=2,ctr-panel,-1.000000,

execute=4,laminar/B738/toggle_switch/dspl_ctrl_pnl_left,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.ControlSource]<[0.000000]

calc=[0.000000]

execute=2,ctr-panel,-1.000000,

execute=4,laminar/B738/toggle_switch/dspl_ctrl_pnl_right,0.000000,

logic:

calc=[0.000000]

execute=2,cp-disp,-1.000000,

out=CrossFeed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.CrossFeedSW]>[0.000000]

calc=[0.000000]

execute=2,crossfeed,-1.000000,

execute=4,laminar/B738/toggle_switch/crossfeed_valve_off,0.000000,

logic:

[SYSTEMS.FUEL.CrossFeedSW]==[0.000000]

calc=[0.000000]

execute=2,cr-feed,-1.000000,

logic:

calc=[0.000000]

out=Pump1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LAftPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,aft-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft1,0.000000,

execute=2,aft-l-off,0.000000,

logic:

calc=[0.000000]

execute=2,f-aft-l,-1.000000,

out=Pump2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]!=[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[0.000000]

calc=[0.000000]

execute=2,fwd-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft2,0.000000,

execute=2,fwd-l-off,0.000000,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]==[1.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]<[200.000000]

calc=[0.000000]

execute=2,f-fwd-l,-1.000000,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]==[1.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]>[200.000000]

calc=[0.000000]

execute=2,fwd-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft2,0.000000,

execute=2,fwd-l-off,0.000000,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]==[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]<[200.000000]

calc=[0.000000]

execute=2,fwd-l-off,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft2,1.000000,

execute=2,fwd-l-on,0.000000,

logic:

calc=[0.000000]

execute=2,f-fwd-l,-1.000000,

out=Pump3,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RFwdPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,fwd-r-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_rgt2,0.000000,

execute=2,fwd-r-off,0.000000,

logic:

calc=[0.000000]

execute=2,f-fwd-r,-1.000000,

out=Pump4,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RAftPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,aft-r-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_rgt1,0.000000,

execute=2,aft-r-off,0.000000,

logic:

calc=[0.000000]

execute=2,f-aft-r,-1.000000,

out=Pump5,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LCtrPumpSW]!=[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[0.000000]

calc=[0.000000]

execute=2,ctr-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr1,0.000000,

execute=2,ctr-l-off,0.000000,

logic:

[SYSTEMS.FUEL.LCtrPumpSW]==[1.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]>[200.000000]

calc=[0.000000]

execute=2,f-ctr-l,-1.000000,

logic:

[SYSTEMS.FUEL.LCtrPumpSW]==[1.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]<[200.000000]

calc=[0.000000]

execute=2,ctr-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr1,0.000000,

execute=2,ctr-l-off,0.000000,

logic:

[SYSTEMS.FUEL.LCtrPumpSW]==[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]>[200.000000]

calc=[0.000000]

execute=2,ctr-l-off,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr1,1.000000,

execute=2,ctr-l-on,0.000000,

logic:

calc=[0.000000]

execute=2,f-ctr-l,-1.000000,

out=Pump6,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RCtrPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,ctr-r-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr2,0.000000,

execute=2,ctr-r-off,0.000000,

logic:

calc=[0.000000]

execute=2,f-ctr-r,-1.000000,

out=Bat,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.BatterySW]==[0.000000]

calc=[0.000000]

execute=2,bat-off,-1.000000,

execute=4,laminar/B738/button_switch_cover02,0.000000,

execute=8,laminar/B738/electric/battery_pos,1.000000,

execute=2,bat-on,0.000000,

logic:

[SYSTEMS.ELEC.BatterySW]==[1.000000]

calc=[0.000000]

execute=2,bat,-1.000000,

logic:

calc=[0.000000]

out=Util,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.CabUtil]==[0.000000]

calc=[0.000000]

execute=2,util-off,-1.000000,

execute=8,laminar/B738/toggle_switch/cab_util_pos,1.000000,

execute=2,util-on,-1.000000,

logic:

[SYSTEMS.ELEC.CabUtil]==[1.000000]

calc=[0.000000]

execute=2,utilcab,-1.000000,

logic:

calc=[0.000000]

out=Pass,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.IfePass]==[0.000000]

calc=[0.000000]

execute=2,ife-off,-1.000000,

execute=8,laminar/B738/toggle_switch/ife_pass_seat_pos,1.000000,

execute=2,ife-on,0.000000,

logic:

[SYSTEMS.ELEC.IfePass]==[1.000000]

calc=[0.000000]

execute=2,utilcab,-1.000000,

logic:

calc=[0.000000]

out=StbyPower,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.StanddyPowerCover]!=[0.000000]

calc=[0.000000]

execute=2,stby-off,-1.000000,

execute=8,laminar/B738/electric/standby_bat_pos,1.000000,

execute=4,laminar/B738/button_switch_cover03,0.000000,

execute=2,stby-on,0.000000,

logic:

[SYSTEMS.ELEC.StanddyPowerCover]==[0.000000]

calc=[0.000000]

execute=2,stndpower,-1.000000,

logic:

calc=[0.000000]

out=Drive1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.Gen1DiscCover]==[1.000000]

&&

[SYSTEMS.ELEC.Gen1Disc]==[0.000000]

calc=[0.000000]

execute=2,drive1,-1.000000,

execute=4,laminar/B738/button_switch_cover04,0.000000,

logic:

[SYSTEMS.ELEC.Gen1DiscCover]==[1.000000]

&&

[SYSTEMS.ELEC.Gen1Disc]==[1.000000]

calc=[0.000000]

execute=2,drive1,-1.000000,

execute=4,laminar/B738/one_way_switch/drive_disconnect1_off,0.000000,

execute=7,,0.300000,

execute=4,laminar/B738/button_switch_cover04,0.000000,

logic:

[SYSTEMS.ELEC.Gen1DiscCover]==[0.000000]

&&

[SYSTEMS.ELEC.Gen1Disc]==[1.000000]

calc=[0.000000]

execute=2,drive1,-1.000000,

execute=4,laminar/B738/button_switch_cover04,0.000000,

execute=7,,0.300000,

execute=4,laminar/B738/one_way_switch/drive_disconnect1_off,0.000000,

execute=4,laminar/B738/button_switch_cover04,0.000000,

logic:

[SYSTEMS.ELEC.Gen1DiscCover]==[0.000000]

&&

[SYSTEMS.ELEC.Gen1Disc]==[0.000000]

calc=[0.000000]

execute=2,stndpower,-1.000000,

logic:

calc=[0.000000]

out=Drive2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.Gen2DiscCover]==[1.000000]

&&

[SYSTEMS.ELEC.Gen2Disc]==[0.000000]

calc=[0.000000]

execute=2,drive2,-1.000000,

execute=4,laminar/B738/button_switch_cover05,0.000000,

logic:

[SYSTEMS.ELEC.Gen2DiscCover]==[1.000000]

&&

[SYSTEMS.ELEC.Gen2Disc]==[1.000000]

calc=[0.000000]

execute=2,drive2,-1.000000,

execute=4,laminar/B738/one_way_switch/drive_disconnect2_off,0.000000,

execute=7,,0.300000,

execute=4,laminar/B738/button_switch_cover05,0.000000,

logic:

[SYSTEMS.ELEC.Gen2DiscCover]==[0.000000]

&&

[SYSTEMS.ELEC.Gen2Disc]==[1.000000]

calc=[0.000000]

execute=2,drive2,-1.000000,

execute=4,laminar/B738/button_switch_cover05,0.000000,

execute=7,,0.300000,

execute=4,laminar/B738/one_way_switch/drive_disconnect2_off,0.000000,

execute=4,laminar/B738/button_switch_cover05,0.000000,

logic:

[SYSTEMS.ELEC.Gen2DiscCover]==[0.000000]

&&

[SYSTEMS.ELEC.Gen2Disc]==[0.000000]

calc=[0.000000]

execute=2,stndpower,-1.000000,

logic:

calc=[0.000000]

out=BusTrans,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.BasTransCover]==[0.000000]

&&

[SYSTEMS.ELEC.BusTransSW]==[1.000000]

calc=[0.000000]

execute=2,bustransf,-1.000000,

logic:

[SYSTEMS.ELEC.BasTransCover]==[0.000000]

&&

[SYSTEMS.ELEC.BusTransSW]==[0.000000]

calc=[0.000000]

execute=2,busoff,-1.000000,

execute=4,laminar/B738/button_switch_cover06,0.000000,

execute=8,sim/cockpit2/electrical/cross_tie,1.000000,

execute=7,,1.000000,

execute=4,laminar/B738/button_switch_cover06,0.000000,

execute=2,buson,-1.000000,

logic:

[SYSTEMS.ELEC.BasTransCover]==[1.000000]

&&

[0.000000]==[1.000000]

calc=[0.000000]

execute=2,bus-off,-1.000000,

execute=4,laminar/B738/button_switch_cover06,0.000000,

execute=2,bus-on,0.000000,

logic:

[SYSTEMS.ELEC.BasTransCover]==[1.000000]

&&

[SYSTEMS.ELEC.BusTransSW]==[0.000000]

calc=[0.000000]

execute=2,bus-off,-1.000000,

execute=8,sim/cockpit2/electrical/cross_tie,1.000000,

execute=4,laminar/B738/button_switch_cover06,0.000000,

execute=2,bus-on,0.000000,

logic:

calc=[0.000000]

out=TestApu,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FIRE.Eng1FirePB]==[1.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

execute=1,Sir; engine one fire switch is not in,0.000000,

execute=1,Electrical power up procedure is not complete,0.000000,

execute=3,,0.000000,

logic:

[SYSTEMS.FIRE.Eng2FirePB]==[1.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

execute=1,Sir; engine two fire switch is not in,0.000000,

execute=1,Electrical power up procedure is not complete,0.000000,

execute=3,,0.000000,

logic:

[SYSTEMS.FIRE.APUFirePB]==[1.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

execute=1,Sir; APU fire switch is not in,0.000000,

execute=1,Electrical power up procedure is not complete,0.000000,

execute=3,,0.000000,

logic:

[SYSTEMS.APU.AvailAPU]==[0.000000]

&&

[SYSTEMS.FIRE.Eng1FirePB]==[0.000000]

&&

[SYSTEMS.FIRE.Eng2FirePB]==[0.000000]

&&

[SYSTEMS.FIRE.APUFirePB]==[0.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

execute=2,apu-fire,-1.000000,

execute=5,laminar/B738/toggle_switch/fire_test_lft,0.000000,

execute=7,,1.000000,

execute=2,apu-fire1,-1.000000,

execute=7,,1.000000,

execute=2,apu-fire,-1.000000,

execute=7,,1.000000,

execute=6,laminar/B738/toggle_switch/fire_test_lft,0.000000,

execute=2,apu-fire,-1.000000,

execute=5,laminar/B738/toggle_switch/fire_test_rgt,0.000000,

execute=7,,2.000000,

execute=2,apu-fire1,-1.000000,

execute=7,,1.000000,

execute=2,apu-fire2,-1.000000,

execute=5,laminar/B738/push_button/fire_bell_light2,0.000000,

execute=7,,1.000000,

execute=6,laminar/B738/push_button/fire_bell_light2,0.000000,

execute=2,apu-fire,-1.000000,

execute=7,,1.000000,

execute=6,laminar/B738/toggle_switch/fire_test_rgt,0.000000,

execute=2,ext-test,-1.000000,

execute=5,laminar/B738/toggle_switch/exting_test_lft,0.000000,

execute=7,,1.000000,

execute=6,laminar/B738/toggle_switch/exting_test_lft,0.000000,

execute=5,laminar/B738/toggle_switch/exting_test_rgt,0.000000,

execute=7,,1.000000,

execute=6,laminar/B738/toggle_switch/exting_test_rgt,0.000000,

logic:

calc=[0.000000]

execute=2,apu,-1.000000,

out=ApuStart,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.APU.AvailAPU]==[1.000000]

calc=[0.000000]

execute=2,apu,-1.000000,

logic:

[SYSTEMS.APU.AvailAPU]==[0.000000]

&&

[SYSTEMS.APU.StartSW]==[0.000000]

calc=[2.000000]

execute=2,ovhd-dn,-1.000000,

execute=2,apu-off,-1.000000,

execute=4,laminar/B738/spring_toggle_switch/APU_start_pos_dn,0.000000,

execute=2,apu-cntr,0.000000,

execute=2,ovhd-dn,-1.000000,

execute=7,,10.000000,

execute=2,apu-cntr,-1.000000,

execute=4,laminar/B738/spring_toggle_switch/APU_start_pos_dn,0.000000,

execute=2,apu-start,0.000000,

execute=2,ovhd-dn,-1.000000,

logic:

[SYSTEMS.APU.AvailAPU]==[0.000000]

&&

[SYSTEMS.APU.StartSW]==[1.000000]

calc=[2.000000]

execute=2,apu-cntr,-1.000000,

execute=4,laminar/B738/spring_toggle_switch/APU_start_pos_dn,0.000000,

execute=2,apu-start,0.000000,

execute=2,ovhd-dn,-1.000000,

logic:

calc=[0.000000]

out=ApuGenOffAnn,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.APU.ApuGenOff_Ann]!=[0.000000]

||

[SYSTEMS.ELEC.ACBusAvail]!=[0.000000]

calc=[0.000000]

execute=10,not_define,0.000000,

logic:

calc=[0.000000]

out=ApuGen1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.APU.ApuGenOff_Ann]!=[0.000000]

||

[SYSTEMS.ELEC.SourceIndLeft]!=[0.000000]

calc=[0.000000]

execute=2,apu1-cntr,-1.000000,

execute=4,laminar/B738/toggle_switch/apu_gen1_dn,0.000000,

execute=8,laminar/B738/electrical/apu_gen1_pos,1.000000,

execute=2,apu1-on,0.000000,

execute=7,,0.300000,

execute=8,laminar/B738/electrical/apu_gen1_pos,0.000000,

logic:

[SYSTEMS.ELEC.APUGen1Bus]==[1.000000]

&&

[SYSTEMS.ELEC.SourceIndLeft]==[0.000000]

calc=[0.000000]

execute=2,gencheck,-1.000000,

logic:

calc=[0.000000]

out=ApuGen2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.APU.ApuGenOff_Ann]!=[0.000000]

||

[SYSTEMS.ELEC.SourceIndRight]!=[0.000000]

calc=[0.000000]

execute=2,apu2-cntr,-1.000000,

execute=4,laminar/B738/toggle_switch/apu_gen2_dn,0.000000,

execute=8,laminar/B738/electrical/apu_gen2_pos,1.000000,

execute=2,apu2-on,0.000000,

execute=7,,0.300000,

execute=8,laminar/B738/electrical/apu_gen2_pos,0.000000,

logic:

[SYSTEMS.ELEC.APUGen2Bus]==[1.000000]

&&

[SYSTEMS.ELEC.SourceIndRight]==[0.000000]

calc=[0.000000]

execute=2,gencheck,-1.000000,

logic:

calc=[0.000000]

out=FuelPump2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]!=[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[0.000000]

calc=[0.000000]

execute=2,fwd-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft2,0.000000,

execute=2,fwd-l-off,0.000000,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]==[1.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]<[200.000000]

calc=[0.000000]

execute=2,f-fwd-l,-1.000000,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]==[1.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]>[200.000000]

calc=[0.000000]

execute=2,fwd-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft2,0.000000,

execute=2,fwd-l-off,0.000000,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]==[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]<[200.000000]

calc=[0.000000]

execute=2,fwd-l-off,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft2,1.000000,

execute=2,fwd-l-on,0.000000,

logic:

calc=[0.000000]

execute=2,f-fwd-l,-1.000000,

out=Wiper1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WiperL]!=[0.000000]

calc=[0.000000]

execute=2,wiper1-low,-1.000000,

execute=4,laminar/B738/knob/left_wiper_dn,0.000000,

execute=4,laminar/B738/knob/left_wiper_dn,0.000000,

execute=4,laminar/B738/knob/left_wiper_dn,0.000000,

execute=2,wiper1-off,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.WiperL]==[0.000000]

calc=[0.000000]

execute=2,wiper1,-1.000000,

logic:

calc=[0.000000]

out=Wiper2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WiperR]!=[0.000000]

calc=[0.000000]

execute=2,wiper2-low,-1.000000,

execute=4,laminar/B738/knob/right_wiper_dn,0.000000,

execute=4,laminar/B738/knob/right_wiper_dn,0.000000,

execute=4,laminar/B738/knob/right_wiper_dn,0.000000,

execute=2,wiper2-off,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.WiperR]==[0.000000]

calc=[0.000000]

execute=2,wiper2,-1.000000,

logic:

calc=[0.000000]

out=EquipCool_S,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.EquipCool_S]==[1.000000]

calc=[0.000000]

execute=2,sup-altn,-1.000000,

execute=8,laminar/B738/toggle_switch/eq_cool_supply,0.000000,

execute=2,sup-norm,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.EquipCool_S]==[0.000000]

calc=[0.000000]

execute=2,equipcool,-1.000000,

logic:

calc=[0.000000]

out=EquipCool_E,integer,,0.000000,,,,,,,,0,,

logic:

[PROCEDURES.Preflight.EquipCool_E]==[1.000000]

calc=[0.000000]

execute=2,exh-altn,-1.000000,

execute=8,laminar/B738/toggle_switch/eq_cool_exhaust,0.000000,

execute=2,exh-norm,0.000000,

logic:

[PROCEDURES.Preflight.EquipCool_E]==[0.000000]

calc=[0.000000]

execute=2,equipcool,-1.000000,

logic:

calc=[0.000000]

out=EmerExit,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.EmerExitSW]<=[1.000000]

&&

[SYSTEMS.LIGHTS.EmerExitCover]==[1.000000]

calc=[0.000000]

execute=2,exit-off,-1.000000,

execute=4,laminar/B738/button_switch_cover09,0.000000,

execute=2,exit-on,0.000000,

logic:

[SYSTEMS.LIGHTS.EmerExitSW]==[1.000000]

&&

[SYSTEMS.LIGHTS.EmerExitCover]==[2.000000]

calc=[0.000000]

execute=2,exitoff,-1.000000,

execute=4,laminar/B738/toggle_switch/emer_exit_lights_up,0.000000,

execute=2,exit-off,-1.000000,

execute=4,laminar/B738/button_switch_cover09,0.000000,

execute=2,exit-on,0.000000,

logic:

[SYSTEMS.LIGHTS.EmerExitSW]==[0.000000]

&&

[SYSTEMS.LIGHTS.EmerExitCover]==[2.000000]

calc=[0.000000]

execute=2,exiton,-1.000000,

execute=4,laminar/B738/button_switch_cover09,0.000000,

execute=2,exitoff,-1.000000,

execute=4,laminar/B738/toggle_switch/emer_exit_lights_up,0.000000,

execute=2,exit-off,-1.000000,

execute=4,laminar/B738/button_switch_cover09,0.000000,

execute=2,exit-on,0.000000,

logic:

[SYSTEMS.LIGHTS.EmerExitSW]==[1.000000]

&&

[SYSTEMS.LIGHTS.EmerExitCover]<=[0.000000]

calc=[0.000000]

execute=2,emerexit,-1.000000,

logic:

calc=[0.000000]

out=Chimes,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_NoSmokeSW]==[0.000000]

calc=[0.000000]

execute=2,chimes-off,-1.000000,

execute=4,laminar/B738/toggle_switch/no_smoking_dn,0.000000,

execute=2,chimes-on,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_NoSmokeSW]!=[0.000000]

calc=[0.000000]

execute=2,chime,-1.000000,

logic:

calc=[0.000000]

out=FastenBelt,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_SeatBeltsSW]==[0.000000]

calc=[0.000000]

execute=2,belt-off,-1.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_dn,0.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_dn,0.000000,

execute=2,belt-on,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_SeatBeltsSW]==[1.000000]

calc=[0.000000]

execute=2,belt-auto,-1.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_dn,0.000000,

execute=2,belt-on,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_SeatBeltsSW]==[2.000000]

calc=[0.000000]

execute=2,chime,-1.000000,

logic:

calc=[0.000000]

out=HeatTest,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,whtest,-1.000000,

execute=7,,0.500000,

execute=2,ovht-test,-1.000000,

execute=5,laminar/B738/toggle_switch/window_ovht_test_dn,0.000000,

execute=7,,2.000000,

execute=5,laminar/B738/toggle_switch/window_ovht_test_dn,0.000000,

execute=2,ovht-t-up,0.000000,

execute=5,laminar/B738/toggle_switch/window_ovht_test_up,0.000000,

execute=7,,2.000000,

execute=6,laminar/B738/toggle_switch/window_ovht_test_up,0.000000,

execute=2,ovht-test,0.000000,

logic:

calc=[0.000000]

out=Heat1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WHeatLSide]!=[1.000000]

calc=[0.000000]

execute=2,wh1-off,-1.000000,

execute=4,laminar/B738/toggle_switch/window_heat_l_side,0.000000,

execute=2,wh1-on,0.000000,

logic:

calc=[0.000000]

execute=2,wh1-on,-1.000000,

execute=4,laminar/B738/toggle_switch/window_heat_l_side,0.000000,

execute=2,wh1-off,0.000000,

execute=2,wh1-off,-1.000000,

execute=4,laminar/B738/toggle_switch/window_heat_l_side,0.000000,

execute=2,wh1-on,0.000000,

out=Heat2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WHeatLFwd]!=[1.000000]

calc=[0.000000]

execute=2,wh2-off,-1.000000,

execute=4,laminar/B738/toggle_switch/window_heat_l_fwd,0.000000,

execute=2,wh2-on,0.000000,

logic:

calc=[0.000000]

execute=2,wh2-on,-1.000000,

execute=4,laminar/B738/toggle_switch/window_heat_l_fwd,0.000000,

execute=2,wh2-off,0.000000,

execute=2,wh2-off,-1.000000,

execute=4,laminar/B738/toggle_switch/window_heat_l_fwd,0.000000,

execute=2,wh2-on,0.000000,

out=Heat3,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WHeatRFwd]!=[1.000000]

calc=[0.000000]

execute=2,wh3-off,-1.000000,

execute=4,laminar/B738/toggle_switch/window_heat_r_fwd,0.000000,

execute=2,wh3-on,0.000000,

logic:

calc=[0.000000]

execute=2,wh3-on,-1.000000,

execute=4,laminar/B738/toggle_switch/window_heat_r_fwd,0.000000,

execute=2,wh3-off,0.000000,

execute=2,wh3-off,-1.000000,

execute=4,laminar/B738/toggle_switch/window_heat_r_fwd,0.000000,

execute=2,wh3-on,0.000000,

out=Heat4,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WHeatRSide]!=[1.000000]

calc=[0.000000]

execute=2,wh4-off,-1.000000,

execute=4,laminar/B738/toggle_switch/window_heat_r_side,0.000000,

execute=2,wh4-on,0.000000,

logic:

calc=[0.000000]

execute=2,wh4-on,-1.000000,

execute=4,laminar/B738/toggle_switch/window_heat_r_side,0.000000,

execute=2,wh4-off,0.000000,

execute=2,wh4-off,-1.000000,

execute=4,laminar/B738/toggle_switch/window_heat_r_side,0.000000,

execute=2,wh4-on,0.000000,

out=Probe_A,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.ProbeHeatA]!=[0.000000]

calc=[0.000000]

execute=2,probeaon,-1.000000,

execute=8,laminar/B738/toggle_switch/capt_probes_pos,0.000000,

execute=2,probeaoff,0.000000,

logic:

calc=[0.000000]

execute=2,probeheat,-1.000000,

out=Probe_B,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.ProbeHeatB]!=[0.000000]

calc=[0.000000]

execute=2,probebon,-1.000000,

execute=8,laminar/B738/toggle_switch/fo_probes_pos,0.000000,

execute=2,probeboff,0.000000,

logic:

calc=[0.000000]

execute=2,probeheat,-1.000000,

out=WingAntiIce,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.WingPB]==[0.000000]

calc=[0.000000]

execute=2,wing-ice,-1.000000,

logic:

[SYSTEMS.ICE.WingPB]>[0.000000]

calc=[0.000000]

execute=2,wice-on,-1.000000,

execute=4,laminar/B738/toggle_switch/wing_heat,0.000000,

execute=2,wice-off,0.000000,

logic:

calc=[0.000000]

out=Eng1AntiIce,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.ENG1IcePB]==[1.000000]

calc=[0.000000]

execute=2,e1ice-on,-1.000000,

execute=8,laminar/B738/ice/eng1_heat_pos,0.000000,

execute=2,e1ice-off,0.000000,

logic:

[SYSTEMS.ICE.ENG1IcePB]==[0.000000]

calc=[0.000000]

execute=2,eng-ice,-1.000000,

logic:

calc=[0.000000]

out=Eng2AntiIce,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.ENG2IcePB]==[1.000000]

calc=[0.000000]

execute=2,e2ice-on,-1.000000,

execute=8,laminar/B738/ice/eng2_heat_pos,0.000000,

execute=2,e2ice-off,0.000000,

logic:

[SYSTEMS.ICE.ENG2IcePB]==[0.000000]

calc=[0.000000]

execute=2,eng-ice,-1.000000,

logic:

calc=[0.000000]

out=HydEng1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.Eng1PumpSW]!=[1.000000]

calc=[0.000000]

execute=2,hydeng1off,-1.000000,

execute=8,laminar/B738/toggle_switch/hydro_pumps1_pos,1.000000,

execute=2,hydeng1on,0.000000,

logic:

calc=[0.000000]

execute=2,lhydpump,-1.000000,

out=HydElec2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.ElecPump2]!=[0.000000]

calc=[0.000000]

execute=2,helec2on,-1.000000,

execute=8,laminar/B738/toggle_switch/electric_hydro_pumps1_pos,0.000000,

execute=2,helec2off,0.000000,

logic:

calc=[0.000000]

execute=2,2ehydpump,-1.000000,

out=HydElec1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.ElecPump1]!=[0.000000]

calc=[0.000000]

execute=2,helec1on,-1.000000,

execute=8,laminar/B738/toggle_switch/electric_hydro_pumps2_pos,0.000000,

execute=2,helec1off,0.000000,

logic:

calc=[0.000000]

execute=2,1ehydpump,-1.000000,

out=HydEng2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.Eng2PumpSW]!=[1.000000]

calc=[0.000000]

execute=2,hydeng2off,-1.000000,

execute=8,laminar/B738/toggle_switch/hydro_pumps2_pos,1.000000,

execute=2,hydeng2on,0.000000,

logic:

calc=[0.000000]

execute=2,rhydpump,-1.000000,

out=CabPressDiff,integer,,0.000000,,,,,,,,0,,

logic:

calc=[0.000000]

execute=2,cab-press,-1.000000,

out=TrimAir,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.TrimAir]==[0.000000]

calc=[0.000000]

execute=2,trim-off,-1.000000,

execute=8,laminar/B738/air/trim_air_pos,1.000000,

execute=2,trim-on,0.000000,

logic:

[SYSTEMS.AIR.TrimAir]==[1.000000]

calc=[0.000000]

execute=2,condition,-1.000000,

logic:

calc=[0.000000]

out=ContCab,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.ContCabTempSW]!=[0.500000]

calc=[0.000000]

execute=2,cont-cab,-1.000000,

execute=8,laminar/B738/air/cont_cab_temp/rheostat,0.500000,

logic:

[SYSTEMS.AIR.ContCabTempSW]==[0.500000]

calc=[0.000000]

execute=2,tempcont1,-1.000000,

logic:

calc=[0.000000]

out=FwdCab,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.FwdCabinTempSW]!=[0.500000]

calc=[0.000000]

execute=2,fwd-cab,-1.000000,

execute=8,laminar/B738/air/fwd_cab_temp/rheostat,0.500000,

logic:

[SYSTEMS.AIR.FwdCabinTempSW]==[0.500000]

calc=[0.000000]

execute=2,tempcont2,-1.000000,

logic:

calc=[0.000000]

out=AftCab,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.AftCabinTempSW]!=[0.500000]

calc=[0.000000]

execute=2,aft-cab,-1.000000,

execute=8,laminar/B738/air/aft_cab_temp/rheostat,0.500000,

logic:

[SYSTEMS.AIR.AftCabinTempSW]==[0.500000]

calc=[0.000000]

execute=2,tempcont2,-1.000000,

logic:

calc=[0.000000]

out=L_Fan,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.L_Fan]==[0.000000]

calc=[0.000000]

execute=2,fan-l-off,-1.000000,

execute=8,laminar/B738/air/l_recirc_fan_pos,1.000000,

execute=2,fan-l-on,0.000000,

logic:

[SYSTEMS.AIR.L_Fan]==[1.000000]

calc=[0.000000]

execute=2,lecircfan,-1.000000,

logic:

calc=[0.000000]

out=R_Fan,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.R_Fan]==[0.000000]

calc=[0.000000]

execute=2,fan-r-off,-1.000000,

execute=8,laminar/B738/air/r_recirc_fan_pos,1.000000,

execute=2,fan-r-on,0.000000,

logic:

[SYSTEMS.AIR.R_Fan]==[1.000000]

calc=[0.000000]

execute=2,recircfan,-1.000000,

logic:

calc=[0.000000]

out=L_Pack,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Pack1]==[0.000000]

calc=[0.000000]

execute=2,pack-1-off,-1.000000,

execute=8,laminar/B738/air/l_pack_pos,1.000000,

execute=2,pack-1-aut,0.000000,

logic:

[SYSTEMS.AIR.Pack1]==[2.000000]

calc=[0.000000]

execute=2,pack-1-hig,-1.000000,

execute=8,laminar/B738/air/l_pack_pos,1.000000,

execute=2,pack-1-aut,0.000000,

logic:

[SYSTEMS.AIR.Pack1]==[1.000000]

calc=[0.000000]

execute=2,lpack,-1.000000,

logic:

calc=[0.000000]

out=R_Pack,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Pack2]==[0.000000]

calc=[0.000000]

execute=2,pack-2-off,-1.000000,

execute=8,laminar/B738/air/r_pack_pos,1.000000,

execute=2,pack-2-aut,0.000000,

logic:

[SYSTEMS.AIR.Pack2]==[2.000000]

calc=[0.000000]

execute=2,pack-2-hig,-1.000000,

execute=8,laminar/B738/air/r_pack_pos,1.000000,

execute=2,pack-2-aut,0.000000,

logic:

[SYSTEMS.AIR.Pack2]==[1.000000]

calc=[0.000000]

execute=2,rpack,-1.000000,

logic:

calc=[0.000000]

out=IzolValve,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.IsolValve]==[0.000000]

calc=[0.000000]

execute=2,isol-v-off,-1.000000,

execute=8,laminar/B738/air/isolation_valve_pos,2.000000,

execute=2,isol-v-ope,0.000000,

logic:

[SYSTEMS.AIR.IsolValve]==[2.000000]

calc=[0.000000]

execute=2,lsolvalv,-1.000000,

logic:

[SYSTEMS.AIR.IsolValve]==[1.000000]

calc=[0.000000]

execute=2,isol-v-aut,-1.000000,

execute=8,laminar/B738/air/isolation_valve_pos,2.000000,

execute=2,isol-v-ope,0.000000,

logic:

calc=[0.000000]

out=Bleed1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Eng1BleedSW]!=[1.000000]

calc=[0.000000]

execute=2,bleed1-off,-1.000000,

execute=8,laminar/B738/toggle_switch/bleed_air_1_pos,1.000000,

execute=2,bleed1-on,0.000000,

logic:

[SYSTEMS.AIR.Eng1BleedSW]==[1.000000]

calc=[0.000000]

execute=2,lbleed,-1.000000,

logic:

calc=[0.000000]

out=Bleed2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Eng2BleedSW]!=[1.000000]

calc=[0.000000]

execute=2,bleed2-off,-1.000000,

execute=8,laminar/B738/toggle_switch/bleed_air_2_pos,1.000000,

execute=2,bleed2-on,0.000000,

logic:

[SYSTEMS.AIR.Eng2BleedSW]==[1.000000]

calc=[0.000000]

execute=2,rpack,-1.000000,

logic:

calc=[0.000000]

out=ApuBleed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.APUBleedSW]==[0.000000]

calc=[0.000000]

execute=2,apuble-off,-1.000000,

execute=8,laminar/B738/toggle_switch/bleed_air_apu_pos,1.000000,

execute=2,apubleedon,0.000000,

logic:

[SYSTEMS.AIR.APUBleedSW]==[1.000000]

calc=[0.000000]

execute=2,apubleed,-1.000000,

logic:

calc=[0.000000]

out=OvhtTest,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,body-test,-1.000000,

execute=5,laminar/B738/push_button/duct_ovht_test,0.000000,

execute=7,,5.000000,

execute=6,laminar/B738/push_button/duct_ovht_test,0.000000,

logic:

calc=[0.000000]

out=FltAlt,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,alt-off,-1.000000,

execute=8,jd/fo/needsetcrz,1.000000,

execute=8,jd/fo/needsetcrz,0.000000,

execute=2,alt-on,-1.000000,

execute=2,answer01,-1.000000,

execute=0,Please check that the flight level is set correctly,0.000000,

logic:

calc=[0.000000]

out=LandAlt,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,l-alt-off,-1.000000,

execute=8,jd/fo/needsetlandalt,1.000000,

execute=8,jd/fo/needsetlandalt,0.000000,

execute=2,l-alt-on,-1.000000,

execute=2,answer01,-1.000000,

execute=0,Please check that the landing altitude is set correctly,0.000000,

logic:

calc=[0.000000]

out=Altn,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDER.PressModeSel]<=[1.000000]

calc=[0.000000]

execute=2,altnpress,-1.000000,

logic:

[SYSTEMS.OVHDSIDER.PressModeSel]==[2.000000]

calc=[0.000000]

execute=2,altn-man,-1.000000,

execute=4,laminar/B738/toggle_switch/air_valve_ctrl_left,0.000000,

execute=2,altn-auto,0.000000,

logic:

[SYSTEMS.OVHDSIDER.PressModeSel]==[3.000000]

calc=[0.000000]

execute=2,altn-man,-1.000000,

execute=4,laminar/B738/toggle_switch/air_valve_ctrl_left,0.000000,

execute=4,laminar/B738/toggle_switch/air_valve_ctrl_left,0.000000,

execute=2,altn-auto,0.000000,

logic:

calc=[0.000000]

out=Lights1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_LandLSW]!=[0.000000]

||

[SYSTEMS.LIGHTS.OVHD_LandRSW]!=[0.000000]

||

[SYSTEMS.LIGHTS.OVHD_LandLRetr]!=[0.000000]

||

[SYSTEMS.LIGHTS.OVHD_LandRRetr]!=[0.000000]

calc=[0.000000]

execute=2,all-1-on,-1.000000,

execute=4,laminar/B738/switch/land_lights_ret_right_up,0.000000,

execute=4,laminar/B738/switch/land_lights_ret_right_up,0.000000,

execute=4,laminar/B738/switch/land_lights_ret_left_up,0.000000,

execute=4,laminar/B738/switch/land_lights_ret_left_up,0.000000,

execute=8,laminar/B738/switch/land_lights_left_pos,0.000000,

execute=8,laminar/B738/switch/land_lights_right_pos,0.000000,

execute=2,all-1-off,0.000000,

logic:

calc=[0.000000]

execute=2,landlight,-1.000000,

out=Lights2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_RwyLeftSW]==[1.000000]

calc=[0.000000]

execute=2,runwayonl,-1.000000,

execute=4,laminar/B738/switch/rwy_light_left_off,0.000000,

execute=2,runwayoffl,0.000000,

logic:

calc=[0.000000]

execute=2,taxilight,-1.000000,

out=Lights3,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_RwyRightSW]==[1.000000]

calc=[0.000000]

execute=2,runwayonr,-1.000000,

execute=4,laminar/B738/switch/rwy_light_right_off,0.000000,

execute=2,runwayoffr,0.000000,

logic:

calc=[0.000000]

execute=2,taxilight,-1.000000,

out=Lights4,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_TaxiSW]!=[0.000000]

calc=[0.000000]

execute=2,taxi-on,-1.000000,

execute=4,laminar/B738/toggle_switch/taxi_light_brightness_pos_up,0.000000,

execute=4,laminar/B738/toggle_switch/taxi_light_brightness_pos_up,0.000000,

execute=2,taxi-off,0.000000,

logic:

calc=[0.000000]

execute=2,taxilight,-1.000000,

out=Lights5,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_LogoSW]!=[0.000000]

calc=[0.000000]

execute=2,logo-on,-1.000000,

execute=8,laminar/B738/toggle_switch/logo_light,0.000000,

execute=2,logo-off,0.000000,

logic:

calc=[0.000000]

execute=2,logolight,-1.000000,

out=Lights6,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_NavSW]==[0.000000]

calc=[0.000000]

execute=2,strobe-off,-1.000000,

execute=4,laminar/B738/toggle_switch/position_light_down,0.000000,

execute=2,strobe-nav,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_NavSW]==[1.000000]

calc=[0.000000]

execute=2,strobe-on,-1.000000,

execute=4,laminar/B738/toggle_switch/position_light_down,0.000000,

execute=4,laminar/B738/toggle_switch/position_light_down,0.000000,

execute=2,strobe-nav,0.000000,

logic:

calc=[0.000000]

execute=2,nav,-1.000000,

out=Lights7,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_BeaconSW]!=[0.000000]

calc=[0.000000]

execute=2,beacon-on,-1.000000,

execute=8,sim/cockpit/electrical/beacon_lights_on,0.000000,

execute=2,beacon-off,0.000000,

logic:

calc=[0.000000]

execute=2,beacon,-1.000000,

out=Lights8,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_WingSW]!=[0.000000]

calc=[0.000000]

execute=2,wing-on,-1.000000,

execute=4,laminar/B738/switch/wing_light_off,0.000000,

execute=2,wing-off,0.000000,

logic:

calc=[0.000000]

execute=2,winglight,-1.000000,

out=Lights9,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_WheelSW]!=[0.000000]

calc=[0.000000]

execute=2,well-on,-1.000000,

execute=8,sim/cockpit2/switches/generic_lights_switch[5],0.000000,

execute=2,well-off,0.000000,

logic:

calc=[0.000000]

execute=2,welllight,-1.000000,

out=Eng1Start,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng1StartSW]>[1.000000]

calc=[0.000000]

execute=2,start1cont,-1.000000,

execute=4,laminar/B738/rotary/eng1_start_off,0.000000,

execute=2,start1auto,0.000000,

logic:

[SYSTEMS.ENGINE.EngMasterSW_1]<[1.000000]

calc=[0.000000]

execute=2,start1grd,-1.000000,

execute=4,laminar/B738/rotary/eng1_start_off,0.000000,

execute=2,start1auto,0.000000,

logic:

calc=[0.000000]

execute=2,lengstart,-1.000000,

out=Eng2Start,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng2StartSW]<[1.000000]

calc=[0.000000]

execute=2,start2grd,-1.000000,

execute=4,laminar/B738/rotary/eng2_start_off,0.000000,

execute=2,start2auto,0.000000,

logic:

[SYSTEMS.ENGINE.EngMasterSW_2]>[1.000000]

calc=[0.000000]

execute=2,start2cont,-1.000000,

execute=4,laminar/B738/rotary/eng2_start_off,0.000000,

execute=2,start2auto,0.000000,

logic:

calc=[0.000000]

execute=2,rengstart,-1.000000,

out=Course,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,look-frd,-1.000000,

execute=2,course-off,-1.000000,

execute=8,jd/fo/rwyneedhdg,1.000000,

execute=8,jd/fo/rwyneedhdg,0.000000,

execute=2,course-on,-1.000000,

logic:

calc=[0.000000]

out=FD,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MCP.FD2]==[0.000000]

calc=[0.000000]

execute=2,look-frd,-1.000000,

execute=2,fd-on,-1.000000,

execute=4,laminar/B738/autopilot/flight_director_fo_toggle,0.000000,

logic:

[SYSTEMS.MCP.FD2]==[1.000000]

calc=[0.000000]

execute=2,look-frd,-1.000000,

logic:

calc=[0.000000]

out=Baro,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MCP.ChangeHPA_Cap]==[0.000000]

calc=[0.000000]

execute=2,baro-off,-1.000000,

execute=4,laminar/B738/EFIS_control/fo/baro_in_hpa_dn,0.000000,

execute=8,jd/fo/needsetbaro,0.000000,

execute=8,jd/fo/needsetbaro1,0.000000,

execute=8,jd/fo/needsetbaro,1.000000,

execute=2,baro-on,-1.000000,

logic:

[SYSTEMS.MCP.ChangeHPA_Cap]==[1.000000]

calc=[0.000000]

execute=2,baro-off,-1.000000,

execute=4,laminar/B738/EFIS_control/fo/baro_in_hpa_up,0.000000,

execute=8,jd/fo/needsetbaro,0.000000,

execute=8,jd/fo/needsetbaro1,0.000000,

execute=8,jd/fo/needsetbaro,1.000000,

execute=2,baro-on,-1.000000,

logic:

calc=[0.000000]

out=RW,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.PEDESTAL.RadarSWFo]==[1.000000]

calc=[0.000000]

execute=2,wxr,-1.000000,

execute=4,laminar/B738/EFIS_control/fo/push_button/wxr_press,0.000000,

logic:

[SYSTEMS.PEDESTAL.RadarSWFo]==[0.000000]

calc=[0.000000]

execute=2,look-frd,-1.000000,

logic:

calc=[0.000000]

out=OxyTest,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,oxy-test,-1.000000,

execute=5,laminar/B738/push_button/oxy_test_fo,0.000000,

execute=7,,5.000000,

execute=6,laminar/B738/push_button/oxy_test_fo,0.000000,

logic:

calc=[0.000000]

out=ClockFO,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FRONTPANEL.ClockFO]<=[1.000000]

calc=[0.000000]

execute=2,look-pfd,-1.000000,

logic:

[SYSTEMS.FRONTPANEL.ClockFO]==[2.000000]

calc=[0.000000]

execute=2,clock-utc,-1.000000,

execute=4,laminar/B738/push_button/chrono_disp_mode_fo,0.000000,

execute=7,,1.000000,

execute=4,laminar/B738/push_button/chrono_disp_mode_fo,0.000000,

logic:

[SYSTEMS.FRONTPANEL.ClockFO]==[3.000000]

calc=[0.000000]

execute=2,clock-utc,-1.000000,

execute=4,laminar/B738/push_button/chrono_disp_mode_fo,0.000000,

execute=4,laminar/B738/push_button/chrono_disp_mode_fo,0.000000,

logic:

[SYSTEMS.FRONTPANEL.ClockFO]==[4.000000]

calc=[0.000000]

execute=2,clock-utc,-1.000000,

execute=4,laminar/B738/push_button/chrono_disp_mode_fo,0.000000,

logic:

calc=[0.000000]

out=MPDisplay,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FRONTPANEL.MainPanelDisplay]==[-1.000000]

calc=[0.000000]

execute=2,dus-norm,-1.000000,

execute=4,laminar/B738/toggle_switch/main_pnl_du_fo_left,0.000000,

logic:

[SYSTEMS.FRONTPANEL.MainPanelDisplay]==[0.000000]

calc=[0.000000]

execute=2,look-pfd,-1.000000,

logic:

[SYSTEMS.FRONTPANEL.MainPanelDisplay]==[1.000000]

calc=[0.000000]

execute=2,dus-norm,-1.000000,

execute=4,laminar/B738/toggle_switch/main_pnl_du_fo_right,0.000000,

logic:

calc=[0.000000]

out=LDisplay,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FRONTPANEL.LowerDisplay]==[1.000000]

calc=[0.000000]

execute=2,du-norm,-1.000000,

execute=4,laminar/B738/toggle_switch/lower_du_fo_right,0.000000,

logic:

[SYSTEMS.FRONTPANEL.LowerDisplay]==[0.000000]

calc=[0.000000]

execute=2,look-pfd,-1.000000,

logic:

[SYSTEMS.FRONTPANEL.LowerDisplay]==[2.000000]

calc=[0.000000]

execute=2,du-norm,-1.000000,

execute=4,laminar/B738/toggle_switch/lower_du_fo_left,0.000000,

logic:

calc=[0.000000]

out=TestSW,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,prst-test,-1.000000,

execute=5,laminar/B738/toggle_switch/ap_disconnect_test2_up,0.000000,

execute=7,,2.000000,

execute=6,laminar/B738/toggle_switch/ap_disconnect_test2_up,0.000000,

execute=2,prst-test,-1.000000,

execute=5,laminar/B738/toggle_switch/ap_disconnect_test2_dn,0.000000,

execute=7,,2.000000,

execute=6,laminar/B738/toggle_switch/ap_disconnect_test2_dn,0.000000,

logic:

calc=[0.000000]

out=GPWS,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FRONTPANEL.GPWSFlap]!=[0.000000]

calc=[0.000000]

execute=2,look-cdu,-1.000000,

execute=2,gpws-on,-1.000000,

execute=4,laminar/B738/toggle_switch/gpws_flap_cover,0.000000,

execute=2,gpws-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=GPWS1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FRONTPANEL.GPWSGear]!=[0.000000]

calc=[0.000000]

execute=2,look-cdu,-1.000000,

execute=2,gpws-on,-1.000000,

execute=4,laminar/B738/toggle_switch/gpws_gear_cover,0.000000,

execute=2,gpws-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=GPWS2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FRONTPANEL.GPWSTerr]!=[0.000000]

calc=[0.000000]

execute=2,look-cdu,-1.000000,

execute=2,gpws-on,-1.000000,

execute=4,laminar/B738/toggle_switch/gpws_terr_cover,0.000000,

execute=2,gpws-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=GPWSTest,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,gpws-test,-1.000000,

execute=4,laminar/B738/push_button/gpws_test,0.000000,

logic:

calc=[0.000000]

out=LG,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LG.LG_Lever]!=[1.000000]

calc=[0.000000]

execute=2,look-front,-1.000000,

execute=2,lg-off,-1.000000,

execute=8,laminar/B738/controls/gear_handle_down,1.000000,

execute=2,lg-down,0.000000,

logic:

[SYSTEMS.LG.LG_Lever]==[1.000000]

calc=[0.000000]

execute=2,look-front,-1.000000,

logic:

calc=[0.000000]

out=AutoBrake,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.BRAKES.AutoBrakeSW]>[1.000000]

calc=[0.000000]

execute=2,brake-1,-1.000000,

execute=4,laminar/B738/knob/autobrake_rto,0.000000,

execute=2,brake-rto,0.000000,

logic:

[SYSTEMS.BRAKES.AutoBrakeSW]==[1.000000]

calc=[0.000000]

execute=2,brake-off,-1.000000,

execute=4,laminar/B738/knob/autobrake_rto,0.000000,

execute=2,brake-rto,0.000000,

logic:

[SYSTEMS.BRAKES.AutoBrakeSW]==[0.000000]

calc=[0.000000]

execute=2,look-front,-1.000000,

logic:

calc=[0.000000]

out=Vspeeds,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FRONTPANEL.VrefSet]!=[0.000000]

calc=[0.000000]

execute=2,spd-ref,-1.000000,

execute=8,laminar/B738/toggle_switch/spd_ref,0.000000,

logic:

[SYSTEMS.FRONTPANEL.VrefSet]==[0.000000]

calc=[0.000000]

execute=2,look-front,-1.000000,

logic:

calc=[0.000000]

out=N1Set,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FRONTPANEL.N1Set]!=[0.000000]

calc=[0.000000]

execute=2,n1-set,-1.000000,

execute=8,laminar/B738/toggle_switch/n1_set_source,0.000000,

logic:

[SYSTEMS.FRONTPANEL.N1Set]==[0.000000]

calc=[0.000000]

execute=2,look-front,-1.000000,

logic:

calc=[0.000000]

out=FuelFlow,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,flow-off,-1.000000,

execute=8,laminar/B738/toggle_switch/fuel_flow_pos,-1.000000,

execute=2,flow-reset,0.000000,

execute=7,,1.000000,

execute=2,flow-off,0.000000,

execute=8,laminar/B738/toggle_switch/fuel_flow_pos,0.000000,

logic:

calc=[0.000000]

out=SysPage,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FRONTPANEL.SysPage]!=[1.000000]

calc=[0.000000]

execute=2,sys-page,-1.000000,

execute=4,laminar/B738/LDU_control/push_button/MFD_SYS,0.000000,

execute=2,look-cdu,-1.000000,

execute=7,,2.000000,

execute=2,sys-page,-1.000000,

execute=4,laminar/B738/LDU_control/push_button/MFD_SYS,0.000000,

logic:

[SYSTEMS.FRONTPANEL.SysPage]==[1.000000]

calc=[0.000000]

execute=2,look-cdu,-1.000000,

execute=7,,2.000000,

execute=2,sys-page,-1.000000,

execute=4,laminar/B738/LDU_control/push_button/MFD_SYS,0.000000,

logic:

calc=[0.000000]

out=CargoFireTest,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

execute=2,cargo-test,-1.000000,

execute=5,laminar/B738/push_button/cargo_fire_test_push,0.000000,

execute=7,,4.000000,

execute=6,laminar/B738/push_button/cargo_fire_test_push,0.000000,

logic:

calc=[0.000000]

out=Transponder,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.PEDESTAL.Transponder]!=[1.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

execute=2,tcas-tara,-1.000000,

execute=4,laminar/B738/knob/transponder_stby,0.000000,

execute=2,tcas-test,-1.000000,

execute=5,laminar/B738/knob/transponder_test,0.000000,

execute=7,,2.000000,

execute=6,laminar/B738/knob/transponder_test,0.000000,

logic:

[SYSTEMS.PEDESTAL.Transponder]==[1.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

execute=2,tcas-tara,-1.000000,

execute=5,laminar/B738/knob/transponder_test,0.000000,

execute=2,tcas-test,-1.000000,

execute=7,,2.000000,

execute=6,laminar/B738/knob/transponder_test,0.000000,

logic:

calc=[0.000000]

out=Audio,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ACP.Com1On]!=[1.000000]

calc=[0.000000]

execute=2,vhf-1on,-1.000000,

execute=4,laminar/B738/comm/fo_com1_audio_sel,0.000000,

execute=8,laminar/B738/comm/fo_audio_vol_com1,1.000000,

logic:

[SYSTEMS.ACP.Com1On]==[1.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

logic:

calc=[0.000000]

out=Audio1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ACP.Com2On]!=[1.000000]

calc=[0.000000]

execute=2,vhf-2on,-1.000000,

execute=4,laminar/B738/comm/fo_com2_audio_sel,0.000000,

execute=8,laminar/B738/comm/fo_audio_vol_com2,1.000000,

logic:

[SYSTEMS.ACP.Com2On]==[1.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

logic:

calc=[0.000000]

out=Audio2,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,vhf-2,-1.000000,

execute=4,laminar/B738/audio/fo/mic_push2,0.000000,

logic:

calc=[0.000000]

out=TrimLock1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.PEDESTAL.TrimLock1]==[0.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

logic:

[SYSTEMS.PEDESTAL.TrimLock1]!=[0.000000]

calc=[0.000000]

execute=2,trimlock1,-1.000000,

execute=4,laminar/B738/toggle_switch/el_trim_lock,0.000000,

logic:

calc=[0.000000]

out=TrimLock2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.PEDESTAL.TrimLock2]==[0.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

logic:

[SYSTEMS.PEDESTAL.TrimLock2]!=[0.000000]

calc=[0.000000]

execute=2,trimlock2,-1.000000,

execute=4,laminar/B738/toggle_switch/ap_trim_lock,0.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDUP.IrsAlignment]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,preflight procedure,-1.000000,

execute=1,Preflight procedure complete,0.000000,

logic:

[SYSTEMS.OVHDUP.IrsAlignment]!=[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,preflight procedure,-1.000000,

execute=1,Preflight procedure complete,0.000000,

execute=0,We are waiting for the approval of the inertial system,0.000000,

logic:

calc=[0.000000]



devstack=BeforeStart

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=before start procedure

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,before start procedure,-1.000000,

execute=1,Before start procedure,0.000000,

logic:

calc=[0.000000]

out=DeckDoor,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MISC.DeckDoor]>[0.000000]

calc=[0.000000]

execute=2,look-back,-1.000000,

execute=7,,0.200000,

execute=4,laminar/B738/toggle_switch/flt_dk_door_open,0.000000,

execute=7,,1.500000,

execute=2,look-ped,-1.000000,

execute=7,,1.000000,

logic:

[SYSTEMS.MISC.DeckDoor]==[0.000000]

calc=[0.000000]

execute=2,look-back,-1.000000,

execute=7,,0.200000,

execute=2,look-ped,-1.000000,

logic:

calc=[0.000000]

out=CDU,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,look-cdu,-1.000000,

execute=2,init,-1.000000,

execute=4,laminar/B738/button/fmc2_init_ref,0.000000,

execute=2,legs,-1.000000,

execute=4,laminar/B738/button/fmc2_legs,0.000000,

logic:

calc=[0.000000]

out=ExDoors,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MISC.DoorsClosed]!=[1.000000]

calc=[0.000000]

execute=2,ovhd-4,-1.000000,

execute=7,,1.000000,

execute=2,tab-home,-1.000000,

execute=4,laminar/B738/tab/home,0.000000,

execute=2,tab-grnd,-1.000000,

execute=4,laminar/B738/tab/menu6,0.000000,

execute=2,tab-door,-1.000000,

execute=4,laminar/B738/tab/menu7,0.000000,

execute=4,sim/flight_controls/door_close_1,0.000000,

execute=4,sim/flight_controls/door_close_2,0.000000,

execute=4,sim/flight_controls/door_close_3,0.000000,

execute=4,sim/flight_controls/door_close_4,0.000000,

execute=4,sim/flight_controls/door_close_5,0.000000,

execute=4,sim/flight_controls/door_close_6,0.000000,

execute=4,sim/flight_controls/door_close_7,0.000000,

execute=4,sim/flight_controls/door_close_8,0.000000,

execute=4,sim/flight_controls/door_close_9,0.000000,

execute=4,sim/flight_controls/door_close_10,0.000000,

execute=2,tab-home,-1.000000,

execute=4,laminar/B738/tab/home,0.000000,

logic:

[SYSTEMS.MISC.DoorsClosed]==[1.000000]

calc=[0.000000]

execute=2,ovhd-4,-1.000000,

logic:

calc=[0.000000]

out=Pump1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LAftPumpSW]!=[1.000000]

calc=[0.000000]

execute=2,aft-l-off,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft1,1.000000,

execute=2,aft-l-on,0.000000,

logic:

calc=[0.000000]

execute=2,f-aft-l,-1.000000,

out=Pump2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]!=[1.000000]

calc=[0.000000]

execute=2,ovhd-2,-1.000000,

execute=2,fwd-l-off,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft2,1.000000,

execute=2,fwd-l-on,0.000000,

logic:

calc=[0.000000]

execute=2,f-fwd-l,-1.000000,

out=Pump3,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RFwdPumpSW]!=[1.000000]

calc=[0.000000]

execute=2,fwd-r-off,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_rgt2,1.000000,

execute=2,fwd-r-on,0.000000,

logic:

calc=[0.000000]

execute=2,f-fwd-r,-1.000000,

out=Pump4,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RAftPumpSW]!=[1.000000]

calc=[0.000000]

execute=2,aft-r-off,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_rgt1,1.000000,

execute=2,aft-r-on,0.000000,

logic:

calc=[0.000000]

execute=2,f-aft-r,-1.000000,

out=Pump5,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.CenterTank]>[460.000000]

&&

[SYSTEMS.FUEL.LCtrPumpSW]!=[1.000000]

calc=[0.000000]

execute=2,ctr-l-off,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr1,1.000000,

execute=2,ctr-l-on,0.000000,

logic:

[SYSTEMS.FUEL.CenterTank]<[460.000000]

&&

[SYSTEMS.FUEL.LCtrPumpSW]==[1.000000]

calc=[0.000000]

execute=2,ctr-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr1,0.000000,

execute=2,ctr-l-off,0.000000,

logic:

calc=[0.000000]

execute=2,f-ctr-l,-1.000000,

out=Pump6,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.CenterTank]>[460.000000]

&&

[SYSTEMS.FUEL.RCtrPumpSW]!=[1.000000]

calc=[0.000000]

execute=2,ctr-r-off,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr2,1.000000,

execute=2,ctr-r-on,0.000000,

logic:

[SYSTEMS.FUEL.CenterTank]<[460.000000]

&&

[SYSTEMS.FUEL.RCtrPumpSW]==[1.000000]

calc=[0.000000]

execute=2,ctr-r-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr2,0.000000,

execute=2,ctr-r-off,0.000000,

logic:

calc=[0.000000]

execute=2,f-ctr-r,-1.000000,

out=HydEng1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.Eng1PumpSW]!=[1.000000]

calc=[0.000000]

execute=2,hydeng1off,-1.000000,

execute=8,laminar/B738/toggle_switch/hydro_pumps1_pos,1.000000,

execute=2,hydeng1on,0.000000,

logic:

calc=[0.000000]

execute=2,lhydpump,-1.000000,

out=HydEng2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.Eng2PumpSW]!=[1.000000]

calc=[0.000000]

execute=2,hydeng2off,-1.000000,

execute=8,laminar/B738/toggle_switch/hydro_pumps2_pos,1.000000,

execute=2,hydeng2on,0.000000,

logic:

calc=[0.000000]

execute=2,rhydpump,-1.000000,

out=HydElec1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.ElecPump1]!=[1.000000]

calc=[0.000000]

execute=2,helec1off,-1.000000,

execute=8,laminar/B738/toggle_switch/electric_hydro_pumps2_pos,1.000000,

execute=2,helec1on,0.000000,

logic:

calc=[0.000000]

execute=2,1ehydpump,-1.000000,

out=HydElec2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.ElecPump2]!=[1.000000]

calc=[0.000000]

execute=2,helec2off,-1.000000,

execute=8,laminar/B738/toggle_switch/electric_hydro_pumps1_pos,1.000000,

execute=2,helec2on,0.000000,

logic:

calc=[0.000000]

execute=2,2ehydpump,-1.000000,

out=AntiColl,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_BeaconSW]==[1.000000]

calc=[0.000000]

execute=2,beacon,-1.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_BeaconSW]==[0.000000]

calc=[0.000000]

execute=2,beacon-off,-1.000000,

execute=8,sim/cockpit/electrical/beacon_lights_on,1.000000,

execute=2,beacon-on,0.000000,

logic:

calc=[0.000000]

out=Transponder,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.PEDESTAL.Transponder]!=[2.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

execute=2,tcas-test,-1.000000,

execute=4,laminar/B738/knob/transponder_altoff,0.000000,

execute=2,tcas-tara,-1.000000,

logic:

[SYSTEMS.PEDESTAL.Transponder]==[2.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,before start procedure,-1.000000,

execute=1,Before start procedure complete,0.000000,

logic:

calc=[0.000000]



devstack=EngStart

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=engine start procedure

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,start up clearance obtained,-1.000000,

execute=1,Engine start procedure,0.000000,

execute=2,rest01,-1.000000,

logic:

instring=start up clearance obtained

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,start up clearance obtained,-1.000000,

execute=1,Engine start procedure,0.000000,

execute=2,rest01,-1.000000,

logic:

calc=[0.000000]

out=CheckBus,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.APU.AvailAPU]==[0.000000]

calc=[0.000000]

execute=2,ovhd-2,-1.000000,

execute=2,answer01,-1.000000,

execute=1,Sir; APU is not started,0.000000,

execute=1,Engine start procedure is not complete,0.000000,

execute=3,,0.000000,

logic:

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.ELEC.APUGen1Bus]==[0.000000]

calc=[0.000000]

execute=2,apu1-cntr,-1.000000,

execute=4,laminar/B738/toggle_switch/apu_gen1_dn,0.000000,

execute=2,apu1-on,0.000000,

logic:

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.ELEC.APUGen2Bus]==[0.000000]

calc=[0.000000]

execute=2,apu2-cntr,-1.000000,

execute=4,laminar/B738/toggle_switch/apu_gen2_dn,0.000000,

execute=2,apu2-on,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=ApuGen1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.SourceIndLeft]!=[0.000000]

||

[SYSTEMS.APU.ApuGenOff_Ann]!=[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

calc=[0.000000]

execute=2,apu1-cntr,-1.000000,

execute=4,laminar/B738/toggle_switch/apu_gen1_dn,0.000000,

execute=8,laminar/B738/electrical/apu_gen1_pos,1.000000,

execute=2,apu1-on,0.000000,

execute=7,,0.300000,

execute=8,laminar/B738/electrical/apu_gen1_pos,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=ApuGen2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.SourceIndLeft]!=[0.000000]

||

[SYSTEMS.APU.ApuGenOff_Ann]!=[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

calc=[0.000000]

execute=2,apu2-cntr,-1.000000,

execute=4,laminar/B738/toggle_switch/apu_gen2_dn,0.000000,

execute=8,laminar/B738/electrical/apu_gen2_pos,1.000000,

execute=2,apu2-on,0.000000,

execute=7,,0.300000,

execute=8,laminar/B738/electrical/apu_gen2_pos,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pack1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Pack1]==[1.000000]

calc=[0.000000]

execute=2,pack-1-aut,-1.000000,

execute=8,laminar/B738/air/l_pack_pos,0.000000,

execute=2,pack-1-off,0.000000,

logic:

[SYSTEMS.AIR.Pack1]==[2.000000]

calc=[0.000000]

execute=2,pack-1-hig,-1.000000,

execute=8,laminar/B738/air/l_pack_pos,0.000000,

execute=2,pack-1-off,0.000000,

logic:

calc=[0.000000]

execute=2,ovhd-6,-1.000000,

out=Pack2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Pack2]==[1.000000]

calc=[0.000000]

execute=2,pack-2-aut,-1.000000,

execute=8,laminar/B738/air/r_pack_pos,0.000000,

execute=2,pack-2-off,0.000000,

logic:

[SYSTEMS.AIR.Pack2]==[2.000000]

calc=[0.000000]

execute=2,pack-2-hig,-1.000000,

execute=8,laminar/B738/air/r_pack_pos,0.000000,

execute=2,pack-2-off,0.000000,

logic:

calc=[0.000000]

execute=2,ovhd-6,-1.000000,

out=ApuBleed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.APUBleedSW]==[0.000000]

calc=[0.000000]

execute=2,ovhd-6,-1.000000,

execute=2,apuble-off,0.000000,

execute=8,laminar/B738/toggle_switch/bleed_air_apu_pos,1.000000,

execute=2,apubleedon,0.000000,

logic:

[SYSTEMS.AIR.APUBleedSW]==[1.000000]

calc=[0.000000]

execute=2,ovhd-6,-1.000000,

logic:

calc=[0.000000]

out=CheckPM,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.COPILOT.doPM_JobOnly]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=1,Waiting for the command to start sequence,0.000000,

execute=12,start number one engine,120.000000,

execute=12,start number two engine,120.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=DispEng,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FRONTPANEL.EngPag]==[0.000000]

calc=[0.000000]

execute=2,eng-page,-1.000000,

execute=4,laminar/B738/LDU_control/push_button/MFD_ENG,0.000000,

logic:

[SYSTEMS.FRONTPANEL.EngPag]==[1.000000]

calc=[0.000000]

execute=2,look-front,-1.000000,

logic:

[SYSTEMS.FRONTPANEL.EngPag]==[2.000000]

calc=[0.000000]

execute=2,eng-page,-1.000000,

execute=4,laminar/B738/LDU_control/push_button/MFD_ENG,0.000000,

execute=4,laminar/B738/LDU_control/push_button/MFD_ENG,0.000000,

logic:

calc=[0.000000]

out=StartEng1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng1StartSW]<=[1.000000]

&&

[SYSTEMS.ENGINE.Eng1N2]<[55.000000]

calc=[1.000000]

execute=2,look-front,-1.000000,

execute=2,start1auto,-1.000000,

execute=4,laminar/B738/rotary/eng1_start_grd,0.000000,

execute=2,start1grd,0.000000,

execute=2,look-front,-1.000000,

execute=8,jd/fo/starter1,1.000000,

logic:

[SYSTEMS.ENGINE.Eng1StartSW]>[1.000000]

&&

[SYSTEMS.ENGINE.Eng1N2]<[55.000000]

calc=[1.000000]

execute=2,look-front,-1.000000,

execute=2,start1cont,-1.000000,

execute=4,laminar/B738/rotary/eng1_start_grd,0.000000,

execute=2,start1grd,0.000000,

execute=2,look-front,-1.000000,

execute=8,jd/fo/starter1,1.000000,

logic:

[SYSTEMS.ENGINE.Eng1StartSW]==[1.000000]

&&

[SYSTEMS.ENGINE.Eng1N2]>[56.000000]

calc=[0.000000]

execute=2,look-front,-1.000000,

execute=0,Already started,0.000000,

logic:

calc=[COMMANDS.Eng1Start.Title]

out=StartLever1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng1N2]>=[24.000000]

calc=[0.000000]

execute=2,look-front,-1.000000,

execute=0,twenty five N two,0.000000,

execute=0,Fuel flow!,0.000000,

execute=2,fuel1-off,-1.000000,

execute=8,laminar/B738/engine/mixture_ratio1,1.000000,

execute=2,fuel1-on,0.000000,

execute=2,look-front,-1.000000,

logic:

calc=[0.000000]

out=Starter1Cutout,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng1StartSW]==[1.000000]

calc=[0.000000]

execute=2,ovhd-4,-1.000000,

execute=0,Starter cutout,0.000000,

execute=2,rest01,-1.000000,

logic:

calc=[0.000000]

out=StartEng2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng2StartSW]<=[1.000000]

&&

[SYSTEMS.ENGINE.Eng2N2]<[55.000000]

calc=[1.000000]

execute=2,start2auto,-1.000000,

execute=4,laminar/B738/rotary/eng2_start_grd,0.000000,

execute=2,start2grd,0.000000,

execute=2,look-front,-1.000000,

execute=8,jd/fo/starter2,1.000000,

logic:

[SYSTEMS.ENGINE.Eng2StartSW]>[1.000000]

&&

[SYSTEMS.ENGINE.Eng2N2]<[55.000000]

calc=[1.000000]

execute=2,start2cont,-1.000000,

execute=4,laminar/B738/rotary/eng2_start_grd,0.000000,

execute=2,start2grd,0.000000,

execute=2,look-front,-1.000000,

execute=8,jd/fo/starter2,1.000000,

logic:

[SYSTEMS.ENGINE.Eng2StartSW]==[1.000000]

&&

[SYSTEMS.ENGINE.Eng2N2]>[56.000000]

calc=[0.000000]

execute=2,look-front,-1.000000,

execute=0,Already started,0.000000,

logic:

calc=[COMMANDS.Eng1Start.Title]

out=StartLever2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng2N2]>=[24.000000]

calc=[0.000000]

execute=2,look-front,-1.000000,

execute=0,twenty five N two,0.000000,

execute=0,Fuel flow!,0.000000,

execute=2,fuel2-off,-1.000000,

execute=8,laminar/B738/engine/mixture_ratio2,1.000000,

execute=2,fuel2-on,0.000000,

execute=2,look-front,-1.000000,

logic:

calc=[0.000000]

out=Starter2Cutout,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng2StartSW]==[1.000000]

calc=[0.000000]

execute=2,ovhd-4,-1.000000,

execute=0,Starter cutout,0.000000,

execute=2,rest01,-1.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,look-front,-1.000000,

execute=12,start up clearance obtained,-1.000000,

execute=1,Engine start procedure complete,0.000000,

logic:

calc=[0.000000]



devstack=BeforeTaxi

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

[SYSOLD.Procedure.EngStart]==[1.000000]

&&

[SYSOLD.Procedure.BeforeTaxi]==[0.000000]

&&

[SYSTEMS.CDU.CDUPreflight]==[1.000000]

&&

[SYSTEMS.TIME.TFT]>=[30.000000]

&&

[SYSTEMS.FLAPS.FlapCompCDU]==[0.000000]

&&

[SYSTEMS.COPILOT.doPM_JobOnly]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,before taxi procedure,-1.000000,

execute=1,Before taxi procedure,0.000000,

logic:

instring=before taxi procedure

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,before taxi procedure,-1.000000,

execute=1,Before taxi procedure,0.000000,

logic:

calc=[0.000000]

out=Gen1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.GenON]==[1.000000]

calc=[0.000000]

execute=2,gen1-ctrl,-1.000000,

execute=4,laminar/B738/toggle_switch/gen1_dn,0.000000,

execute=8,laminar/B738/electrical/gen1_pos,1.000000,

execute=2,gen1-on,0.000000,

execute=7,,1.000000,

execute=8,laminar/B738/electrical/gen1_pos,0.000000,

logic:

[SYSTEMS.ELEC.GenON]==[3.000000]

calc=[0.000000]

execute=2,gen1-ctrl,-1.000000,

execute=4,laminar/B738/toggle_switch/gen1_dn,0.000000,

execute=2,gen1-on,0.000000,

logic:

calc=[0.000000]

execute=2,elec,-1.000000,

out=Gen2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.GenON]==[2.000000]

calc=[0.000000]

execute=2,gen2-ctrl,-1.000000,

execute=4,laminar/B738/toggle_switch/gen2_dn,0.000000,

execute=8,laminar/B738/electrical/gen2_pos,1.000000,

execute=2,gen2-on,0.000000,

execute=7,,0.300000,

execute=8,laminar/B738/electrical/gen2_pos,0.000000,

logic:

[SYSTEMS.ELEC.GenON]==[3.000000]

calc=[0.000000]

execute=2,gen2-ctrl,-1.000000,

execute=4,laminar/B738/toggle_switch/gen2_dn,0.000000,

execute=2,gen2-on,0.000000,

logic:

calc=[0.000000]

execute=2,elec,-1.000000,

out=ProbeHeat_A,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.ProbeHeatA]==[0.000000]

calc=[0.000000]

execute=2,ovhd-5,-1.000000,

execute=2,probeaoff,-1.000000,

execute=8,laminar/B738/toggle_switch/capt_probes_pos,1.000000,

execute=2,probeaon,0.000000,

logic:

calc=[0.000000]

execute=2,ovhd-5,-1.000000,

out=ProbeHeat_B,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.ProbeHeatB]==[0.000000]

calc=[0.000000]

execute=2,probeboff,-1.000000,

execute=8,laminar/B738/toggle_switch/fo_probes_pos,1.000000,

execute=2,probebon,0.000000,

logic:

calc=[0.000000]

execute=2,probeheat,-1.000000,

out=AntiAce,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.WEATHER.TAT]<[10.000000]

&&

[SYSTEMS.WEATHER.TAT]>[-5.000000]

&&

[SYSTEMS.WEATHER.Rain]>[0.300000]

calc=[0.000000]

execute=2,look-front,-1.000000,

execute=2,answer01,-1.000000,

execute=1,Sir; we have the conditions for icing,0.000000,

logic:

calc=[0.000000]

execute=2,eng-ice,-1.000000,

out=Pack1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Pack1]==[0.000000]

calc=[0.000000]

execute=2,pack-1-off,-1.000000,

execute=8,laminar/B738/air/l_pack_pos,1.000000,

execute=2,pack-1-aut,0.000000,

logic:

[SYSTEMS.AIR.Pack1]==[2.000000]

calc=[0.000000]

execute=2,pack-1-hig,-1.000000,

execute=8,laminar/B738/air/l_pack_pos,1.000000,

execute=2,pack-1-aut,0.000000,

logic:

calc=[0.000000]

execute=2,lpack,-1.000000,

out=Pack2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Pack2]==[0.000000]

calc=[0.000000]

execute=2,pack-2-off,-1.000000,

execute=8,laminar/B738/air/r_pack_pos,1.000000,

execute=2,pack-2-aut,0.000000,

logic:

[SYSTEMS.AIR.Pack2]==[2.000000]

calc=[0.000000]

execute=2,pack-2-hig,-1.000000,

execute=8,laminar/B738/air/r_pack_pos,1.000000,

execute=2,pack-2-aut,0.000000,

logic:

calc=[0.000000]

execute=2,rpack,-1.000000,

out=IsolValve,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.IsolValve]==[0.000000]

calc=[0.000000]

execute=2,isol-v-off,-1.000000,

execute=8,laminar/B738/air/isolation_valve_pos,1.000000,

execute=2,isol-v-aut,0.000000,

logic:

[SYSTEMS.AIR.IsolValve]==[1.000000]

calc=[0.000000]

execute=2,lsolvalv,-1.000000,

logic:

[SYSTEMS.AIR.IsolValve]==[2.000000]

calc=[0.000000]

execute=2,isol-v-ope,-1.000000,

execute=8,laminar/B738/air/isolation_valve_pos,1.000000,

execute=2,isol-v-aut,0.000000,

logic:

calc=[0.000000]

out=APUBleed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.APUBleedSW]==[1.000000]

calc=[0.000000]

execute=2,apubleedon,-1.000000,

execute=8,laminar/B738/toggle_switch/bleed_air_apu_pos,0.000000,

execute=2,apuble-off,0.000000,

logic:

[SYSTEMS.AIR.APUBleedSW]==[0.000000]

calc=[0.000000]

execute=2,apubleed,-1.000000,

logic:

calc=[0.000000]

out=APU,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.APU.StartSW]>[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

calc=[0.000000]

execute=2,ovhd-2,-1.000000,

execute=2,apu-start,-1.000000,

execute=4,laminar/B738/spring_toggle_switch/APU_start_pos_up,0.000000,

execute=4,laminar/B738/spring_toggle_switch/APU_start_pos_up,0.000000,

execute=2,apu-off,0.000000,

logic:

[SYSTEMS.APU.StartSW]==[1.000000]

&&

[SYSTEMS.APU.AvailAPU]==[0.000000]

calc=[0.000000]

execute=2,ovhd-2,-1.000000,

execute=2,apu-start,-1.000000,

execute=4,laminar/B738/spring_toggle_switch/APU_start_pos_up,0.000000,

execute=4,laminar/B738/spring_toggle_switch/APU_start_pos_up,0.000000,

execute=2,apu-off,0.000000,

execute=1,Battery switch?,0.000000,

logic:

[SYSTEMS.APU.StartSW]==[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[0.000000]

calc=[0.000000]

execute=2,ovhd-2,-1.000000,

logic:

calc=[0.000000]

out=Eng1StartSW,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng1StartSW]!=[2.000000]

calc=[0.000000]

execute=2,start1auto,-1.000000,

execute=4,laminar/B738/knob/eng1_start_right,0.000000,

execute=2,start1cont,0.000000,

logic:

calc=[0.000000]

execute=2,lengstart,-1.000000,

out=Eng2StartSW,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng2StartSW]!=[2.000000]

calc=[0.000000]

execute=2,start2auto,-1.000000,

execute=4,laminar/B738/knob/eng2_start_right,0.000000,

execute=2,start2cont,0.000000,

logic:

calc=[0.000000]

execute=2,rengstart,-1.000000,

out=Recall,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,masterwarn,-1.000000,

execute=5,laminar/B738/push_button/fo_six_pack,0.000000,

execute=7,,1.000000,

execute=6,laminar/B738/push_button/fo_six_pack,0.000000,

execute=2,rest01,-1.000000,

logic:

calc=[0.000000]

out=Baro,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MCP.ChangeHPA_Cap]==[0.000000]

&&

[SYSTEMS.MISC.StartEngRunning]==[1.000000]

calc=[0.000000]

execute=2,baro-off,-1.000000,

execute=4,laminar/B738/EFIS_control/fo/baro_in_hpa_dn,0.000000,

execute=8,jd/fo/needsetbaro,0.000000,

execute=8,jd/fo/needsetbaro1,0.000000,

execute=8,jd/fo/needsetbaro,1.000000,

execute=2,baro-on,-1.000000,

logic:

[SYSTEMS.MCP.ChangeHPA_Cap]==[1.000000]

&&

[SYSTEMS.MISC.StartEngRunning]==[1.000000]

calc=[0.000000]

execute=2,baro-off,-1.000000,

execute=4,laminar/B738/EFIS_control/fo/baro_in_hpa_up,0.000000,

execute=8,jd/fo/needsetbaro,0.000000,

execute=8,jd/fo/needsetbaro1,0.000000,

execute=8,jd/fo/needsetbaro,1.000000,

execute=2,baro-on,-1.000000,

logic:

[SYSTEMS.MISC.StartEngRunning]==[0.000000]

calc=[0.000000]

execute=10,not_define,0.000000,

logic:

calc=[0.000000]

out=Fd,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MCP.FD2]==[0.000000]

&&

[SYSTEMS.MISC.StartEngRunning]==[1.000000]

calc=[0.000000]

execute=2,look-frd,-1.000000,

execute=2,fd-on,-1.000000,

execute=4,laminar/B738/autopilot/flight_director_fo_toggle,0.000000,

logic:

[SYSTEMS.MCP.FD2]==[1.000000]

&&

[SYSTEMS.MISC.StartEngRunning]==[1.000000]

calc=[0.000000]

execute=2,look-frd,-1.000000,

logic:

[SYSTEMS.MISC.StartEngRunning]==[0.000000]

calc=[0.000000]

execute=10,not_define,0.000000,

logic:

calc=[0.000000]

out=AutoBrakes,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.BRAKES.AutoBrakeSW]>[1.000000]

&&

[SYSTEMS.MISC.StartEngRunning]==[1.000000]

calc=[0.000000]

execute=2,brake-1,-1.000000,

execute=4,laminar/B738/knob/autobrake_rto,0.000000,

execute=2,brake-rto,0.000000,

logic:

[SYSTEMS.BRAKES.AutoBrakeSW]==[1.000000]

&&

[SYSTEMS.MISC.StartEngRunning]==[1.000000]

calc=[0.000000]

execute=2,brake-off,-1.000000,

execute=4,laminar/B738/knob/autobrake_rto,0.000000,

execute=2,brake-rto,0.000000,

logic:

[SYSTEMS.BRAKES.AutoBrakeSW]==[0.000000]

&&

[SYSTEMS.MISC.StartEngRunning]==[1.000000]

calc=[0.000000]

execute=2,look-front,-1.000000,

logic:

[SYSTEMS.MISC.StartEngRunning]==[0.000000]

calc=[0.000000]

execute=10,not_define,0.000000,

logic:

calc=[0.000000]

out=DomeLight,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_DomeSW]==[1.000000]

calc=[0.000000]

execute=2,domewhite,-1.000000,

execute=4,laminar/B738/toggle_switch/cockpit_dome_dn,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_DomeSW]==[0.000000]

calc=[0.000000]

execute=2,ovhd-up,-1.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_DomeSW]==[-1.000000]

calc=[0.000000]

execute=2,domewhite,-1.000000,

execute=4,laminar/B738/toggle_switch/cockpit_dome_up,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,before taxi procedure,-1.000000,

execute=1,Before taxi procedure complete,0.000000,

logic:

calc=[0.000000]



devstack=BeforeTakeoff

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=before takeoff procedure

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,line up clearance obtained,-1.000000,

execute=12,before taxi checklist,-1.000000,

execute=1,Before takeoff procedure,0.000000,

logic:

instring=line up clearance obtained

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,line up clearance obtained,-1.000000,

execute=12,before taxi checklist,-1.000000,

execute=1,Before takeoff procedure,0.000000,

logic:

calc=[0.000000]

out=Call,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_SeatBeltsSW]==[0.000000]

calc=[0.000000]

execute=2,ovhd-4,-1.000000,

execute=2,belt-off,-1.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_dn,0.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_dn,0.000000,

execute=2,belt-on,0.000000,

execute=2,belt-on,-1.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_up,0.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_up,0.000000,

execute=2,belt-off,0.000000,

execute=2,belt-off,-1.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_dn,0.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_dn,0.000000,

execute=2,belt-on,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_SeatBeltsSW]==[1.000000]

calc=[0.000000]

execute=2,ovhd-4,-1.000000,

execute=2,belt-auto,-1.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_up,0.000000,

execute=2,belt-off,0.000000,

execute=2,belt-off,-1.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_dn,0.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_dn,0.000000,

execute=2,belt-on,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_SeatBeltsSW]==[2.000000]

calc=[0.000000]

execute=2,ovhd-4,-1.000000,

execute=2,belt-on,-1.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_up,0.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_up,0.000000,

execute=2,belt-off,0.000000,

execute=7,,0.200000,

execute=2,belt-off,-1.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_dn,0.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_dn,0.000000,

execute=2,belt-on,0.000000,

logic:

calc=[0.000000]

out=LandLights,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,ovhd-2,-1.000000,

execute=2,all-off,-1.000000,

execute=4,laminar/B738/spring_switch/landing_lights_all,0.000000,

execute=2,all-on,0.000000,

logic:

calc=[0.000000]

out=Strobe,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_NavSW]<=[0.000000]

calc=[0.000000]

execute=2,strobe-off,-1.000000,

execute=4,laminar/B738/toggle_switch/position_light_up,0.000000,

execute=4,laminar/B738/toggle_switch/position_light_up,0.000000,

execute=2,strobe-on,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_NavSW]==[1.000000]

calc=[0.000000]

execute=2,nav,-1.000000,

logic:

calc=[0.000000]

out=RwyTurn,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_RwyRightSW]==[1.000000]

&&

[SYSTEMS.LIGHTS.OVHD_RwyLeftSW]==[0.000000]

calc=[0.000000]

execute=2,runwayoffl,-1.000000,

execute=4,laminar/B738/switch/rwy_light_left_on,0.000000,

execute=2,runwayonl,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_RwyLeftSW]==[1.000000]

&&

[SYSTEMS.LIGHTS.OVHD_RwyRightSW]==[1.000000]

calc=[0.000000]

execute=2,taxilight,-1.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_RwyLeftSW]==[1.000000]

&&

[SYSTEMS.LIGHTS.OVHD_RwyRightSW]==[0.000000]

calc=[0.000000]

execute=2,runwayoffr,-1.000000,

execute=4,laminar/B738/switch/rwy_light_right_on,0.000000,

execute=2,runwayonr,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_RwyLeftSW]==[0.000000]

&&

[SYSTEMS.LIGHTS.OVHD_RwyRightSW]==[0.000000]

calc=[0.000000]

execute=2,runwayoffl,-1.000000,

execute=4,laminar/B738/switch/rwy_light_left_on,0.000000,

execute=2,runwayonl,0.000000,

execute=7,,0.200000,

execute=2,runwayoffr,-1.000000,

execute=4,laminar/B738/switch/rwy_light_right_on,0.000000,

execute=2,runwayonr,0.000000,

logic:

calc=[0.000000]

out=Taxi,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_TaxiSW]!=[0.000000]

calc=[0.000000]

execute=2,taxi-on,-1.000000,

execute=4,laminar/B738/toggle_switch/taxi_light_brightness_pos_up,0.000000,

execute=4,laminar/B738/toggle_switch/taxi_light_brightness_pos_up,0.000000,

execute=2,taxi-off,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_TaxiSW]==[0.000000]

calc=[0.000000]

execute=2,taxilight,-1.000000,

logic:

calc=[0.000000]

out=Tara,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.PEDESTAL.Transponder]!=[5.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

execute=2,tcas-test,-1.000000,

execute=4,laminar/B738/knob/transponder_tara,0.000000,

execute=2,tcas-tara,-1.000000,

logic:

[SYSTEMS.PEDESTAL.Transponder]==[5.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,line up clearance obtained,-1.000000,

execute=1,Before takeoff procedure complete,0.000000,

execute=12,before takeoff checklist,60.000000,

execute=0,Ready for before takeoff checklist!,0.000000,

logic:

calc=[0.000000]



devstack=Descent

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FLIGHTPHASE.PHASE]==[SYSTEMS.FLIGHTPHASE.Cruise]

&&

[SYSTEMS.FMS.Tod]<=[40.000000]

&&

[SYSTEMS.COPILOT.doPM_JobOnly]==[0.000000]

&&

[SYSOLD.Procedure.Descent]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,descent procedure,-1.000000,

execute=1,Descent procedure,0.000000,

logic:

instring=descent procedure

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,descent procedure,-1.000000,

execute=1,Descent procedure,0.000000,

logic:

calc=[0.000000]

out=Recall,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,masterwarn,-1.000000,

execute=5,laminar/B738/push_button/fo_six_pack,0.000000,

execute=7,,1.000000,

execute=6,laminar/B738/push_button/fo_six_pack,0.000000,

execute=2,rest01,-1.000000,

logic:

calc=[0.000000]

out=CourseDest,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,look-frd,-1.000000,

execute=2,course-off,-1.000000,

execute=8,jd/fo/rwyneedhdgdest,1.000000,

execute=8,jd/fo/rwyneedhdgdest,0.000000,

execute=2,course-on,-1.000000,

logic:

calc=[0.000000]

out=Vref,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FMS.FlapsAppr]<[15.000000]

&&

[SYSTEMS.COPILOT.doPM_JobOnly]==[0.000000]

calc=[0.000000]

execute=2,look-cdu,-1.000000,

execute=2,init,-1.000000,

execute=4,laminar/B738/button/fmc2_init_ref,0.000000,

execute=2,l6,-1.000000,

execute=4,laminar/B738/button/fmc2_6L,0.000000,

execute=2,l5,-1.000000,

execute=4,laminar/B738/button/fmc2_5L,0.000000,

execute=2,r2,-1.000000,

execute=4,laminar/B738/button/fmc2_2R,0.000000,

execute=7,,0.200000,

execute=2,r4,-1.000000,

execute=4,laminar/B738/button/fmc2_4R,0.000000,

execute=2,answer01,-1.000000,

execute=1,Sir; please check v reference speed and set minimum for approach,0.000000,

logic:

[SYSTEMS.FMS.FlapsAppr]>[0.000000]

&&

[SYSTEMS.COPILOT.doPM_JobOnly]==[0.000000]

calc=[0.000000]

execute=2,look-cdu,-1.000000,

execute=2,init,-1.000000,

execute=4,laminar/B738/button/fmc2_init_ref,0.000000,

execute=2,l6,-1.000000,

execute=4,laminar/B738/button/fmc2_6L,0.000000,

execute=2,l5,-1.000000,

execute=4,laminar/B738/button/fmc2_5L,0.000000,

execute=2,answer01,-1.000000,

execute=1,Sir; please check v reference speed and set minimum for approach,0.000000,

logic:

[SYSTEMS.COPILOT.doPM_JobOnly]==[1.000000]

calc=[0.000000]

execute=10,not_define,0.000000,

logic:

calc=[0.000000]

out=LandAlt,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.COPILOT.doPM_JobOnly]==[0.000000]

calc=[0.000000]

execute=2,l-alt-off,-1.000000,

execute=8,laminar/B738/pressurization/knobs/landing_alt,0.000000,

execute=8,jd/fo/needsetlandalt,1.000000,

execute=8,jd/fo/needsetlandalt,0.000000,

execute=2,l-alt-on,-1.000000,

execute=2,answer01,-1.000000,

execute=1,Please check that the landing altitude is set correctly,0.000000,

logic:

[SYSTEMS.COPILOT.doPM_JobOnly]==[1.000000]

calc=[0.000000]

execute=2,landalt,-1.000000,

logic:

calc=[0.000000]

out=AutoBrake,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.BRAKES.AutoBrakeSW]>[1.000000]

&&

[SYSTEMS.COPILOT.doPM_JobOnly]==[0.000000]

calc=[0.000000]

execute=2,look-front,-1.000000,

logic:

[SYSTEMS.BRAKES.AutoBrakeSW]<=[1.000000]

&&

[SYSTEMS.COPILOT.doPM_JobOnly]==[0.000000]

calc=[0.000000]

execute=2,brake-rto,-1.000000,

execute=4,laminar/B738/knob/autobrake_1,0.000000,

execute=2,brake-1,0.000000,

execute=1,Sir; check auto brake position,0.000000,

logic:

[SYSTEMS.COPILOT.doPM_JobOnly]==[1.000000]

calc=[0.000000]

execute=10,not_define,0.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,descent procedure,-1.000000,

execute=1,Descent procedure complete,0.000000,

logic:

calc=[0.000000]



devstack=AfterLanding

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=after landing procedure

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,after landing procedure,-1.000000,

execute=1,After landing procedure,0.000000,

logic:

[SYSTEMS.COPILOT.doPM_JobOnly]==[0.000000]

&&

[SYSTEMS.POSITION.GrSpeed]<=[60.000000]

&&

[SYSTEMS.POSITION.RwyDeltaArrival]>=[30.000000]

&&

[SYSTEMS.POSITION.ApprRwyDistArrival]>=[50.000000]

&&

[SYSTEMS.POSITION.ApprRwyDistArrival]<=[60.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,after landing procedure,-1.000000,

execute=1,After landing procedure,0.000000,

logic:

calc=[0.000000]

out=ProbeA,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.ProbeHeatA]!=[0.000000]

calc=[0.000000]

execute=2,ovhd-5,-1.000000,

execute=2,probeaon,-1.000000,

execute=8,laminar/B738/toggle_switch/capt_probes_pos,0.000000,

execute=2,probeaoff,0.000000,

logic:

calc=[0.000000]

execute=2,probeheat,-1.000000,

out=ProbeB,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.ProbeHeatB]!=[0.000000]

calc=[0.000000]

execute=2,ovhd-5,-1.000000,

execute=2,probebon,-1.000000,

execute=8,laminar/B738/toggle_switch/fo_probes_pos,0.000000,

execute=2,probeboff,0.000000,

logic:

calc=[0.000000]

execute=2,probeheat,-1.000000,

out=LandLights,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_LandLSW]!=[0.000000]

||

[SYSTEMS.LIGHTS.OVHD_LandRSW]!=[0.000000]

||

[SYSTEMS.LIGHTS.OVHD_LandLRetr]!=[0.000000]

||

[SYSTEMS.LIGHTS.OVHD_LandRRetr]!=[0.000000]

calc=[0.000000]

execute=2,all-1-on,-1.000000,

execute=4,laminar/B738/switch/land_lights_ret_right_up,0.000000,

execute=4,laminar/B738/switch/land_lights_ret_right_up,0.000000,

execute=4,laminar/B738/switch/land_lights_ret_left_up,0.000000,

execute=4,laminar/B738/switch/land_lights_ret_left_up,0.000000,

execute=8,laminar/B738/switch/land_lights_left_pos,0.000000,

execute=8,laminar/B738/switch/land_lights_right_pos,0.000000,

execute=2,all-1-off,0.000000,

execute=2,rest01,-1.000000,

logic:

calc=[0.000000]

execute=2,landlight,-1.000000,

out=RunwayLights,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_RwyRightSW]==[1.000000]

&&

[SYSTEMS.LIGHTS.OVHD_RwyLeftSW]==[0.000000]

calc=[0.000000]

execute=2,runwayoffl,-1.000000,

execute=4,laminar/B738/switch/rwy_light_left_on,0.000000,

execute=2,runwayonl,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_RwyLeftSW]==[1.000000]

&&

[SYSTEMS.LIGHTS.OVHD_RwyRightSW]==[1.000000]

calc=[0.000000]

execute=2,taxilight,-1.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_RwyLeftSW]==[1.000000]

&&

[SYSTEMS.LIGHTS.OVHD_RwyRightSW]==[0.000000]

calc=[0.000000]

execute=2,runwayoffr,-1.000000,

execute=4,laminar/B738/switch/rwy_light_right_on,0.000000,

execute=2,runwayonr,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_RwyLeftSW]==[0.000000]

&&

[SYSTEMS.LIGHTS.OVHD_RwyRightSW]==[0.000000]

calc=[0.000000]

execute=2,runwayoffl,-1.000000,

execute=4,laminar/B738/switch/rwy_light_left_on,0.000000,

execute=2,runwayonl,0.000000,

execute=7,,0.200000,

execute=2,runwayoffr,-1.000000,

execute=4,laminar/B738/switch/rwy_light_right_on,0.000000,

execute=2,runwayonr,0.000000,

logic:

calc=[0.000000]

out=Taxi,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_TaxiSW]!=[1.000000]

calc=[0.000000]

execute=2,taxi-off,-1.000000,

execute=4,laminar/B738/toggle_switch/taxi_light_brightness_pos_dn,0.000000,

execute=4,laminar/B738/toggle_switch/taxi_light_brightness_pos_dn,0.000000,

execute=2,taxi-on,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_TaxiSW]==[1.000000]

calc=[0.000000]

execute=2,taxilight,-1.000000,

logic:

calc=[0.000000]

out=Strobe,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_NavSW]>=[0.000000]

calc=[0.000000]

execute=2,strobe-on,-1.000000,

execute=4,laminar/B738/toggle_switch/position_light_down,0.000000,

execute=4,laminar/B738/toggle_switch/position_light_down,0.000000,

execute=2,strobe-nav,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_NavSW]==[-1.000000]

calc=[0.000000]

execute=2,nav,-1.000000,

logic:

calc=[0.000000]

out=Eng1Start,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng1StartSW]!=[1.000000]

calc=[0.000000]

execute=2,start1cont,-1.000000,

execute=4,laminar/B738/rotary/eng1_start_off,0.000000,

execute=2,start1auto,0.000000,

execute=2,rest01,-1.000000,

logic:

calc=[0.000000]

execute=2,lengstart,-1.000000,

out=Eng2Start,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng2StartSW]!=[1.000000]

calc=[0.000000]

execute=2,start2cont,-1.000000,

execute=4,laminar/B738/rotary/eng2_start_off,0.000000,

execute=2,start2auto,0.000000,

execute=2,rest01,-1.000000,

logic:

calc=[0.000000]

execute=2,rengstart,-1.000000,

out=AutoBrake,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.BRAKES.AutoBrakeSW]>[1.000000]

calc=[0.000000]

execute=2,brake-1,-1.000000,

execute=4,laminar/B738/knob/autobrake_off,0.000000,

execute=2,brake-off,0.000000,

logic:

[SYSTEMS.BRAKES.AutoBrakeSW]<[1.000000]

calc=[0.000000]

execute=2,brake-rto,-1.000000,

execute=4,laminar/B738/knob/autobrake_off,0.000000,

execute=2,brake-off,0.000000,

logic:

[SYSTEMS.BRAKES.AutoBrakeSW]==[1.000000]

calc=[0.000000]

execute=2,look-front,-1.000000,

logic:

calc=[0.000000]

out=FlapRetr,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FLAPS.FlapLever]!=[0.000000]

&&

[SYSTEMS.FLAPS.Ok0]==[1.000000]

calc=[0.000000]

execute=2,flaps,-1.000000,

execute=8,laminar/B738/flt_ctrls/flap_lever,0.000000,

execute=2,flaps0,0.000000,

execute=2,rest01,-1.000000,

logic:

[SYSTEMS.FLAPS.FlapLever]==[0.000000]

&&

[SYSTEMS.FLAPS.Ok0]==[1.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

execute=2,rest01,-1.000000,

logic:

calc=[0.000000]

out=Transponder,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.PEDESTAL.Transponder]!=[2.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

execute=2,tcas-test,-1.000000,

execute=4,laminar/B738/knob/transponder_altoff,0.000000,

execute=2,tcas-tara,-1.000000,

logic:

[SYSTEMS.PEDESTAL.Transponder]==[2.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

logic:

calc=[0.000000]

out=Spoiler,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.SPEEDBRAKE.SB_DrfSim]==[0.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

logic:

[SYSTEMS.SPEEDBRAKE.SB_DrfSim]!=[0.000000]

calc=[0.000000]

execute=2,splrs,-1.000000,

execute=8,laminar/B738/flt_ctrls/speedbrake_lever,0.000000,

execute=2,splrs-off,0.000000,

execute=2,rest01,-1.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,after landing procedure,-1.000000,

execute=1,After landing procedure complete,0.000000,

execute=2,rest01,-1.000000,

logic:

calc=[0.000000]



devstack=BeginShutdown

out=Titli,integer,,0.000000,,,,,,,,0,,

logic:

[EVENTS.Landing.StartBeginShDProc]==[1.000000]

&&

[SYSOLD.Procedure.BeginShD]==[0.000000]

calc=[0.000000]

execute=10,not_define,0.000000,

execute=12,shutdown procedure,-1.000000,

logic:

calc=[0.000000]

out=ExtPwrCheck,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.ExtPwrConnect]==[0.000000]

calc=[0.000000]

execute=2,ovhd-dn,-1.000000,

logic:

[SYSTEMS.ELEC.ExtPwrConnect]==[1.000000]

&&

[SYSTEMS.ELEC.ExtPwrSW]==[0.000000]

calc=[0.000000]

execute=2,ovhd-dn,-1.000000,

execute=2,grd-ctrl,-1.000000,

execute=8,sim/cockpit/electrical/gpu_on,1.000000,

execute=2,grd-on,0.000000,

logic:

[SYSTEMS.ELEC.ExtPwrConnect]==[1.000000]

&&

[SYSTEMS.ELEC.ExtPwrSW]==[1.000000]

calc=[0.000000]

execute=2,ovhd-dn,-1.000000,

logic:

calc=[0.000000]

out=ApuGenOnBusCheck,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.ExtPwrSW]==[1.000000]

calc=[0.000000]

execute=2,apu,-1.000000,

logic:

[SYSTEMS.APU.AvailAPU]==[0.000000]

&&

[SYSTEMS.APU.StartSW]==[0.000000]

calc=[0.000000]

execute=2,apu-off,-1.000000,

execute=4,laminar/B738/spring_toggle_switch/APU_start_pos_dn,0.000000,

execute=2,apu-cntr,0.000000,

execute=2,ovhd-dn,-1.000000,

execute=7,,10.000000,

execute=2,apu-cntr,-1.000000,

execute=4,laminar/B738/spring_toggle_switch/APU_start_pos_dn,0.000000,

execute=2,apu-start,0.000000,

execute=2,ovhd-dn,-1.000000,

execute=7,,40.000000,

logic:

[SYSTEMS.APU.AvailAPU]==[0.000000]

&&

[SYSTEMS.APU.StartSW]==[1.000000]

calc=[0.000000]

execute=2,apu-cntr,-1.000000,

execute=4,laminar/B738/spring_toggle_switch/APU_start_pos_dn,0.000000,

execute=2,apu-start,0.000000,

execute=2,ovhd-dn,-1.000000,

execute=7,,20.000000,

logic:

[SYSTEMS.APU.AvailAPU]==[1.000000]

calc=[0.000000]

execute=2,apu,-1.000000,

logic:

calc=[0.000000]

out=ApuGen1On,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.APU.ApuGenOff_Ann]!=[0.000000]

||

[SYSTEMS.ELEC.SourceIndLeft]!=[0.000000]

calc=[0.000000]

execute=2,apu1-cntr,-1.000000,

execute=4,laminar/B738/toggle_switch/apu_gen1_dn,0.000000,

execute=8,laminar/B738/electrical/apu_gen1_pos,1.000000,

execute=2,apu1-on,0.000000,

execute=7,,0.300000,

execute=8,laminar/B738/electrical/apu_gen1_pos,0.000000,

logic:

[SYSTEMS.ELEC.APUGen1Bus]==[1.000000]

&&

[SYSTEMS.ELEC.SourceIndLeft]==[0.000000]

calc=[0.000000]

execute=2,gencheck,-1.000000,

logic:

calc=[0.000000]

out=ApuGen2On,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.APU.ApuGenOff_Ann]!=[0.000000]

||

[SYSTEMS.ELEC.SourceIndRight]!=[0.000000]

calc=[0.000000]

execute=2,apu2-cntr,-1.000000,

execute=4,laminar/B738/toggle_switch/apu_gen2_dn,0.000000,

execute=8,laminar/B738/electrical/apu_gen2_pos,1.000000,

execute=2,apu2-on,0.000000,

execute=7,,0.300000,

execute=8,laminar/B738/electrical/apu_gen2_pos,0.000000,

logic:

[SYSTEMS.ELEC.APUGen2Bus]==[1.000000]

&&

[SYSTEMS.ELEC.SourceIndRight]==[0.000000]

calc=[0.000000]

execute=2,gencheck,-1.000000,

logic:

calc=[0.000000]

out=Eng1StartSW,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng1StartSW]!=[0.000000]

calc=[0.000000]

execute=2,start1cont,-1.000000,

execute=4,laminar/B738/rotary/eng1_start_off,0.000000,

execute=2,start1auto,0.000000,

logic:

calc=[0.000000]

execute=2,lengstart,-1.000000,

out=Eng2StartSW,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng2StartSW]!=[0.000000]

calc=[0.000000]

execute=2,start2cont,-1.000000,

execute=4,laminar/B738/rotary/eng2_start_off,0.000000,

execute=2,start2auto,0.000000,

logic:

calc=[0.000000]

execute=2,rengstart,-1.000000,

out=WingAnti,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.WingPB]==[0.000000]

calc=[0.000000]

execute=2,wing-ice,-1.000000,

logic:

[SYSTEMS.ICE.WingPB]>[0.000000]

calc=[0.000000]

execute=2,wice-on,-1.000000,

execute=4,laminar/B738/toggle_switch/wing_heat,0.000000,

execute=2,wice-off,0.000000,

logic:

calc=[0.000000]

out=Eng1Anti,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.ENG1IcePB]==[1.000000]

calc=[0.000000]

execute=2,e1ice-on,-1.000000,

execute=8,laminar/B738/ice/eng1_heat_pos,0.000000,

execute=2,e1ice-off,0.000000,

logic:

[SYSTEMS.ICE.ENG1IcePB]==[0.000000]

calc=[0.000000]

execute=2,eng-ice,-1.000000,

logic:

calc=[0.000000]

out=Eng2Anti,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.ENG2IcePB]==[1.000000]

calc=[0.000000]

execute=2,e2ice-on,-1.000000,

execute=8,laminar/B738/ice/eng2_heat_pos,0.000000,

execute=2,e2ice-off,0.000000,

logic:

[SYSTEMS.ICE.ENG2IcePB]==[0.000000]

calc=[0.000000]

execute=2,eng-ice,-1.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,shutdown procedure,-1.000000,

logic:

calc=[0.000000]



devstack=Shutdown

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.POSITION.WasInAir]==[1.000000]

&&

[SYSTEMS.POSITION.onGround]==[1.000000]

&&

[SYSOLD.Procedure.BeginShD]==[1.000000]

&&

[SYSTEMS.ENGINE.EngMastSumm]==[0.000000]

&&

[SYSOLD.Procedure.Shutdown]==[0.000000]

&&

[SYSTEMS.BRAKES.ParkBrakeHandlePos]==[1.000000]

&&

[SYSTEMS.COPILOT.doPM_JobOnly]==[0.000000]

&&

[SYSTEMS.FLAPS.FlapSet]==[0.000000]

&&

[EVENTS.FlapsOk.FlapsUP]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,shutdown procedure,-1.000000,

execute=1,Shutdown procedure,0.000000,

logic:

instring=shutdown procedure

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,shutdown procedure,-1.000000,

execute=1,Shutdown procedure,0.000000,

logic:

calc=[0.000000]

out=ParkingBrake,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.BRAKES.ParkBrakeHandlePos]==[0.000000]

calc=[0.000000]

execute=2,parkb-off,-1.000000,

execute=8,sim/flightmodel/controls/parkbrake,1.000000,

execute=8,laminar/B738/parking_brake_pos,1.000000,

execute=2,parkb-on,0.000000,

logic:

[SYSTEMS.BRAKES.ParkBrakeHandlePos]==[1.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

logic:

calc=[0.000000]

out=DomeLight,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_DomeSW]==[0.000000]

&&

[SYSTEMS.TIME.Night_Day]==[1.000000]

calc=[0.000000]

execute=2,domewhite,-1.000000,

execute=4,laminar/B738/toggle_switch/cockpit_dome_dn,0.000000,

execute=2,rest01,-1.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Apu,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.APU.AvailAPU]==[1.000000]

calc=[0.000000]

execute=2,apu,-1.000000,

logic:

[SYSTEMS.APU.AvailAPU]==[0.000000]

&&

[SYSTEMS.APU.StartSW]==[0.000000]

calc=[0.000000]

execute=2,apu-off,-1.000000,

execute=4,laminar/B738/spring_toggle_switch/APU_start_pos_dn,0.000000,

execute=2,apu-cntr,0.000000,

execute=2,ovhd-dn,-1.000000,

execute=7,,10.000000,

execute=2,apu-cntr,-1.000000,

execute=4,laminar/B738/spring_toggle_switch/APU_start_pos_dn,0.000000,

execute=2,apu-start,0.000000,

execute=2,ovhd-dn,-1.000000,

execute=7,,40.000000,

logic:

[SYSTEMS.APU.AvailAPU]==[0.000000]

&&

[SYSTEMS.APU.StartSW]==[1.000000]

calc=[0.000000]

execute=2,apu-cntr,-1.000000,

execute=4,laminar/B738/spring_toggle_switch/APU_start_pos_dn,0.000000,

execute=2,apu-start,0.000000,

execute=2,ovhd-dn,-1.000000,

execute=7,,20.000000,

logic:

calc=[0.000000]

out=ApuGenOffAnn,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.APU.ApuGenOff_Ann]!=[0.000000]

||

[SYSTEMS.ELEC.ACBusAvail]!=[0.000000]

calc=[0.000000]

execute=10,not_define,0.000000,

logic:

calc=[0.000000]

out=ApuGen1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.APU.ApuGenOff_Ann]!=[0.000000]

||

[SYSTEMS.ELEC.SourceIndLeft]!=[0.000000]

calc=[0.000000]

execute=2,apu1-cntr,-1.000000,

execute=4,laminar/B738/toggle_switch/apu_gen1_dn,0.000000,

execute=8,laminar/B738/electrical/apu_gen1_pos,1.000000,

execute=2,apu1-on,0.000000,

execute=7,,0.300000,

execute=8,laminar/B738/electrical/apu_gen1_pos,0.000000,

logic:

[SYSTEMS.ELEC.APUGen1Bus]==[1.000000]

&&

[SYSTEMS.ELEC.SourceIndLeft]==[0.000000]

calc=[0.000000]

execute=2,gencheck,-1.000000,

logic:

calc=[0.000000]

out=ApuGen2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.APU.ApuGenOff_Ann]!=[0.000000]

||

[SYSTEMS.ELEC.SourceIndRight]!=[0.000000]

calc=[0.000000]

execute=2,apu2-cntr,-1.000000,

execute=4,laminar/B738/toggle_switch/apu_gen2_dn,0.000000,

execute=8,laminar/B738/electrical/apu_gen2_pos,1.000000,

execute=2,apu2-on,0.000000,

execute=7,,0.300000,

execute=8,laminar/B738/electrical/apu_gen2_pos,0.000000,

logic:

[SYSTEMS.ELEC.APUGen2Bus]==[1.000000]

&&

[SYSTEMS.ELEC.SourceIndRight]==[0.000000]

calc=[0.000000]

execute=2,gencheck,-1.000000,

logic:

calc=[0.000000]

out=FastenSeat,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_SeatBeltsSW]==[0.000000]

calc=[0.000000]

execute=2,chime,-1.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_SeatBeltsSW]==[1.000000]

calc=[0.000000]

execute=2,belt-auto,-1.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_up,0.000000,

execute=2,belt-off,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_SeatBeltsSW]==[2.000000]

calc=[0.000000]

execute=2,belt-on,-1.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_up,0.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_up,0.000000,

execute=2,belt-off,0.000000,

logic:

calc=[0.000000]

out=Beacon,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_BeaconSW]!=[0.000000]

calc=[0.000000]

execute=2,beacon-on,-1.000000,

execute=8,sim/cockpit/electrical/beacon_lights_on,0.000000,

execute=2,beacon-off,0.000000,

logic:

calc=[0.000000]

execute=2,beacon,-1.000000,

out=FuelPump1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LAftPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,aft-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft1,0.000000,

execute=2,aft-l-off,0.000000,

logic:

calc=[0.000000]

execute=2,f-aft-l,-1.000000,

out=FuelPump2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]!=[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[0.000000]

calc=[0.000000]

execute=2,fwd-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft2,0.000000,

execute=2,fwd-l-off,0.000000,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]==[1.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]<[200.000000]

calc=[0.000000]

execute=2,f-fwd-l,-1.000000,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]==[1.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]>[200.000000]

calc=[0.000000]

execute=2,fwd-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft2,0.000000,

execute=2,fwd-l-off,0.000000,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]==[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]<[200.000000]

calc=[0.000000]

execute=2,fwd-l-off,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft2,1.000000,

execute=2,fwd-l-on,0.000000,

logic:

calc=[0.000000]

execute=2,ovhd-2,-1.000000,

out=FuelPump3,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RFwdPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,fwd-r-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_rgt2,0.000000,

execute=2,fwd-r-off,0.000000,

logic:

calc=[0.000000]

execute=2,f-fwd-r,-1.000000,

out=FuelPump4,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RAftPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,aft-r-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_rgt1,0.000000,

execute=2,aft-r-off,0.000000,

logic:

calc=[0.000000]

execute=2,f-aft-r,-1.000000,

out=FuelPump5,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LCtrPumpSW]!=[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[0.000000]

calc=[0.000000]

execute=2,ctr-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr1,0.000000,

execute=2,ctr-l-off,0.000000,

logic:

[SYSTEMS.FUEL.LCtrPumpSW]==[1.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]>[200.000000]

calc=[0.000000]

execute=2,f-ctr-l,-1.000000,

logic:

[SYSTEMS.FUEL.LCtrPumpSW]==[1.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]<[200.000000]

calc=[0.000000]

execute=2,ctr-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr1,0.000000,

execute=2,ctr-l-off,0.000000,

logic:

[SYSTEMS.FUEL.LCtrPumpSW]==[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]>[200.000000]

calc=[0.000000]

execute=2,ctr-l-off,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr1,1.000000,

execute=2,ctr-l-on,0.000000,

logic:

calc=[0.000000]

execute=2,ovhd-2,-1.000000,

out=FuelPump6,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RCtrPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,ctr-r-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr2,0.000000,

execute=2,ctr-r-off,0.000000,

logic:

calc=[0.000000]

execute=2,f-ctr-r,-1.000000,

out=WingsIce,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.WingPB]==[0.000000]

calc=[0.000000]

execute=2,wing-ice,-1.000000,

logic:

[SYSTEMS.ICE.WingPB]==[1.000000]

calc=[0.000000]

execute=2,wice-on,-1.000000,

execute=4,laminar/B738/toggle_switch/wing_heat,0.000000,

execute=2,wice-off,0.000000,

logic:

calc=[0.000000]

out=EngIce1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.ENG1IcePB]==[1.000000]

calc=[0.000000]

execute=2,e1ice-on,-1.000000,

execute=8,laminar/B738/ice/eng1_heat_pos,0.000000,

execute=2,e1ice-off,0.000000,

logic:

[SYSTEMS.ICE.ENG1IcePB]==[0.000000]

calc=[0.000000]

execute=2,eng-ice,-1.000000,

logic:

calc=[0.000000]

out=EngIce2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.ENG2IcePB]==[1.000000]

calc=[0.000000]

execute=2,e2ice-on,-1.000000,

execute=8,laminar/B738/ice/eng2_heat_pos,0.000000,

execute=2,e2ice-off,0.000000,

logic:

[SYSTEMS.ICE.ENG2IcePB]==[0.000000]

calc=[0.000000]

execute=2,eng-ice,-1.000000,

logic:

calc=[0.000000]

out=HydEng1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.Eng1PumpSW]!=[1.000000]

calc=[0.000000]

execute=2,hydeng1off,-1.000000,

execute=8,laminar/B738/toggle_switch/hydro_pumps1_pos,1.000000,

execute=2,hydeng1on,0.000000,

logic:

calc=[0.000000]

execute=2,lhydpump,-1.000000,

out=HydEng2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.Eng2PumpSW]!=[1.000000]

calc=[0.000000]

execute=2,hydeng2off,-1.000000,

execute=8,laminar/B738/toggle_switch/hydro_pumps2_pos,1.000000,

execute=2,hydeng2on,0.000000,

logic:

calc=[0.000000]

execute=2,rhydpump,-1.000000,

out=HydElec1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.ElecPump1]!=[0.000000]

calc=[0.000000]

execute=2,helec1on,-1.000000,

execute=8,laminar/B738/toggle_switch/electric_hydro_pumps2_pos,0.000000,

execute=2,helec1off,0.000000,

logic:

calc=[0.000000]

execute=2,1ehydpump,-1.000000,

out=HydElec2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.ElecPump2]!=[0.000000]

calc=[0.000000]

execute=2,helec2on,-1.000000,

execute=8,laminar/B738/toggle_switch/electric_hydro_pumps1_pos,0.000000,

execute=2,helec2off,0.000000,

logic:

calc=[0.000000]

execute=2,2ehydpump,-1.000000,

out=Pack1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Pack1]==[0.000000]

calc=[0.000000]

execute=2,pack-1-off,-1.000000,

execute=8,laminar/B738/air/l_pack_pos,1.000000,

execute=2,pack-1-aut,0.000000,

logic:

[SYSTEMS.AIR.Pack1]==[2.000000]

calc=[0.000000]

execute=2,pack-1-hig,-1.000000,

execute=8,laminar/B738/air/l_pack_pos,1.000000,

execute=2,pack-1-aut,0.000000,

logic:

[SYSTEMS.AIR.Pack1]==[1.000000]

calc=[0.000000]

execute=2,lpack,-1.000000,

logic:

calc=[0.000000]

out=Pack2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Pack2]==[0.000000]

calc=[0.000000]

execute=2,pack-2-off,-1.000000,

execute=8,laminar/B738/air/r_pack_pos,1.000000,

execute=2,pack-2-aut,0.000000,

logic:

[SYSTEMS.AIR.Pack2]==[2.000000]

calc=[0.000000]

execute=2,pack-2-hig,-1.000000,

execute=8,laminar/B738/air/r_pack_pos,1.000000,

execute=2,pack-2-aut,0.000000,

logic:

[SYSTEMS.AIR.Pack2]==[1.000000]

calc=[0.000000]

execute=2,rpack,-1.000000,

logic:

calc=[0.000000]

out=IsolValv,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.IsolValve]==[0.000000]

calc=[0.000000]

execute=2,isol-v-off,-1.000000,

execute=8,laminar/B738/air/isolation_valve_pos,2.000000,

execute=2,isol-v-ope,0.000000,

logic:

[SYSTEMS.AIR.IsolValve]==[2.000000]

calc=[0.000000]

execute=2,lsolvalv,-1.000000,

logic:

[SYSTEMS.AIR.IsolValve]==[1.000000]

calc=[0.000000]

execute=2,isol-v-aut,-1.000000,

execute=8,laminar/B738/air/isolation_valve_pos,2.000000,

execute=2,isol-v-ope,0.000000,

logic:

calc=[0.000000]

out=Eng1Bleed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Eng1BleedSW]!=[1.000000]

calc=[0.000000]

execute=2,bleed1-off,-1.000000,

execute=8,laminar/B738/toggle_switch/bleed_air_1_pos,1.000000,

execute=2,bleed1-on,0.000000,

logic:

[SYSTEMS.AIR.Eng1BleedSW]==[1.000000]

calc=[0.000000]

execute=2,lbleed,-1.000000,

logic:

calc=[0.000000]

out=Eng2Bleed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Eng2BleedSW]!=[1.000000]

calc=[0.000000]

execute=2,bleed2-off,-1.000000,

execute=8,laminar/B738/toggle_switch/bleed_air_2_pos,1.000000,

execute=2,bleed2-on,0.000000,

logic:

[SYSTEMS.AIR.Eng2BleedSW]==[1.000000]

calc=[0.000000]

execute=2,rbleed,-1.000000,

logic:

calc=[0.000000]

out=ApuBleed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.APUBleedSW]==[0.000000]

calc=[0.000000]

execute=2,ovhd-6,-1.000000,

execute=2,apuble-off,-1.000000,

execute=8,laminar/B738/toggle_switch/bleed_air_apu_pos,1.000000,

execute=2,apubleedon,0.000000,

logic:

[SYSTEMS.AIR.APUBleedSW]==[1.000000]

calc=[0.000000]

execute=2,ovhd-6,-1.000000,

logic:

calc=[0.000000]

out=Lights1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_LandLSW]!=[0.000000]

||

[SYSTEMS.LIGHTS.OVHD_LandRSW]!=[0.000000]

||

[SYSTEMS.LIGHTS.OVHD_LandLRetr]!=[0.000000]

||

[SYSTEMS.LIGHTS.OVHD_LandRRetr]!=[0.000000]

calc=[0.000000]

execute=2,all-1-on,-1.000000,

execute=4,laminar/B738/switch/land_lights_ret_right_up,0.000000,

execute=4,laminar/B738/switch/land_lights_ret_right_up,0.000000,

execute=4,laminar/B738/switch/land_lights_ret_left_up,0.000000,

execute=4,laminar/B738/switch/land_lights_ret_left_up,0.000000,

execute=8,laminar/B738/switch/land_lights_left_pos,0.000000,

execute=8,laminar/B738/switch/land_lights_right_pos,0.000000,

execute=2,all-1-off,0.000000,

logic:

calc=[0.000000]

execute=2,landlight,-1.000000,

out=Lights2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_RwyLeftSW]==[1.000000]

calc=[0.000000]

execute=2,runwayonl,-1.000000,

execute=4,laminar/B738/switch/rwy_light_left_off,0.000000,

execute=2,runwayoffl,0.000000,

logic:

calc=[0.000000]

execute=2,taxilight,-1.000000,

out=Lights3,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_RwyRightSW]==[1.000000]

calc=[0.000000]

execute=2,runwayonr,-1.000000,

execute=4,laminar/B738/switch/rwy_light_right_off,0.000000,

execute=2,runwayoffr,0.000000,

logic:

calc=[0.000000]

execute=2,taxilight,-1.000000,

out=Lights4,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_TaxiSW]!=[0.000000]

calc=[0.000000]

execute=2,taxi-on,-1.000000,

execute=4,laminar/B738/toggle_switch/taxi_light_brightness_pos_up,0.000000,

execute=4,laminar/B738/toggle_switch/taxi_light_brightness_pos_up,0.000000,

execute=2,taxi-off,0.000000,

logic:

calc=[0.000000]

execute=2,taxilight,-1.000000,

out=Lights5,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_LogoSW]!=[0.000000]

calc=[0.000000]

execute=2,logo-on,-1.000000,

execute=8,laminar/B738/toggle_switch/logo_light,0.000000,

execute=2,logo-off,0.000000,

logic:

calc=[0.000000]

execute=2,logolight,-1.000000,

out=Lights6,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_NavSW]==[0.000000]

calc=[0.000000]

execute=2,strobe-off,-1.000000,

execute=4,laminar/B738/toggle_switch/position_light_down,0.000000,

execute=2,strobe-nav,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_NavSW]==[1.000000]

calc=[0.000000]

execute=2,strobe-on,-1.000000,

execute=4,laminar/B738/toggle_switch/position_light_down,0.000000,

execute=4,laminar/B738/toggle_switch/position_light_down,0.000000,

execute=2,strobe-nav,0.000000,

logic:

calc=[0.000000]

execute=2,nav,-1.000000,

out=Lights7,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_BeaconSW]!=[0.000000]

calc=[0.000000]

execute=2,beacon-on,-1.000000,

execute=8,sim/cockpit/electrical/beacon_lights_on,0.000000,

execute=2,beacon-off,0.000000,

logic:

calc=[0.000000]

execute=2,beacon,-1.000000,

out=Lights8,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_WingSW]!=[0.000000]

calc=[0.000000]

execute=2,wing-on,-1.000000,

execute=4,laminar/B738/switch/wing_light_off,0.000000,

execute=2,wing-off,0.000000,

logic:

calc=[0.000000]

execute=2,winglight,-1.000000,

out=Lights9,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_WheelSW]!=[0.000000]

calc=[0.000000]

execute=2,well-on,-1.000000,

execute=8,sim/cockpit2/switches/generic_lights_switch[5],0.000000,

execute=2,well-off,0.000000,

logic:

calc=[0.000000]

execute=2,welllight,-1.000000,

out=FD,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MCP.FD2]==[1.000000]

calc=[0.000000]

execute=2,look-frd,-1.000000,

execute=2,fd-on,-1.000000,

execute=4,laminar/B738/autopilot/flight_director_fo_toggle,0.000000,

logic:

[SYSTEMS.MCP.FD2]==[0.000000]

calc=[0.000000]

execute=2,look-frd,-1.000000,

logic:

calc=[0.000000]

out=Transponder,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.PEDESTAL.Transponder]!=[1.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

execute=2,tcas-tara,-1.000000,

execute=4,laminar/B738/knob/transponder_stby,0.000000,

execute=2,tcas-test,-1.000000,

logic:

[SYSTEMS.PEDESTAL.Transponder]==[1.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,shutdown procedure,-1.000000,

execute=1,Shutdown procedure complete,0.000000,

execute=2,rest01,-1.000000,

logic:

calc=[0.000000]



devstack=Secure

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=secure procedure

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,secure procedure,-1.000000,

execute=1,Secure procedure,0.000000,

logic:

calc=[0.000000]

out=IrsL,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDUP.IRS_L]!=[0.000000]

calc=[0.000000]

execute=2,irs-l-nav,-1.000000,

execute=4,laminar/B738/toggle_switch/irs_L_left,0.000000,

execute=4,laminar/B738/toggle_switch/irs_L_left,0.000000,

execute=2,irs-l-off,0.000000,

logic:

calc=[0.000000]

execute=2,idrs,-1.000000,

out=IrsR,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDUP.IRS_R]!=[0.000000]

calc=[0.000000]

execute=2,irs-r-nav,-1.000000,

execute=4,laminar/B738/toggle_switch/irs_R_left,0.000000,

execute=4,laminar/B738/toggle_switch/irs_R_left,0.000000,

execute=2,irs-r-off,0.000000,

logic:

calc=[0.000000]

execute=2,idrs,-1.000000,

out=FltContrA,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.FltContrA]==[1.000000]

calc=[0.000000]

execute=2,flt-cont-a,-1.000000,

execute=4,laminar/B738/toggle_switch/flt_ctr_A_cover,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.FltContrA]==[0.000000]

calc=[0.000000]

execute=2,fltcontrol,-1.000000,

logic:

calc=[0.000000]

out=FlControlB,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.FltContrB]==[1.000000]

calc=[0.000000]

execute=2,flt-cont-b,-1.000000,

execute=4,laminar/B738/toggle_switch/flt_ctr_B_cover,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.SpoilerB]==[0.000000]

calc=[0.000000]

execute=2,fltcontrol,-1.000000,

logic:

calc=[0.000000]

out=AltFlaps,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.AltFlapCover]==[1.000000]

calc=[0.000000]

execute=2,alterflaps,-1.000000,

execute=4,laminar/B738/toggle_switch/alt_flaps_cover,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.AltFlapCover]==[0.000000]

calc=[0.000000]

execute=2,altflap,-1.000000,

logic:

calc=[0.000000]

out=SpoilerA,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.SpoilerA]==[1.000000]

calc=[0.000000]

execute=2,spoiler-a,-1.000000,

execute=4,laminar/B738/toggle_switch/spoiler_A_cover,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.SpoilerA]==[0.000000]

calc=[0.000000]

execute=2,spoiler-ab,-1.000000,

logic:

calc=[0.000000]

out=SpoilerB,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.SpoilerB]==[1.000000]

calc=[0.000000]

execute=2,spoiler-b,-1.000000,

execute=4,laminar/B738/toggle_switch/spoiler_B_cover,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.SpoilerB]==[0.000000]

calc=[0.000000]

execute=2,spoiler-ab,-1.000000,

logic:

calc=[0.000000]

out=YawDamper,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.YawDamper]==[0.000000]

calc=[0.000000]

execute=2,yaw-off,-1.000000,

execute=4,laminar/B738/toggle_switch/yaw_dumper,0.000000,

execute=2,yaw-on,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.YawDamper]==[1.000000]

calc=[0.000000]

execute=2,yawdamper,-1.000000,

logic:

calc=[0.000000]

out=VhfNav,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.VhfNavSource]>[0.000000]

calc=[0.000000]

execute=2,vhf-nav,-1.000000,

execute=4,laminar/B738/toggle_switch/vhf_nav_source_lft,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.VhfNavSource]<[0.000000]

calc=[0.000000]

execute=2,vhf-nav,-1.000000,

execute=4,laminar/B738/toggle_switch/vhf_nav_source_rgt,0.000000,

logic:

calc=[0.000000]

execute=2,vhf-disp,-1.000000,

out=Irs,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.IrsSource]>[0.000000]

calc=[0.000000]

execute=2,irs,-1.000000,

execute=4,laminar/B738/toggle_switch/irs_source_left,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.IrsSource]<[0.000000]

calc=[0.000000]

execute=2,irs,-1.000000,

execute=4,laminar/B738/toggle_switch/irs_source_right,0.000000,

logic:

calc=[0.000000]

execute=2,irs-disp,-1.000000,

out=Fmc,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.FmcSource]>[0.000000]

calc=[0.000000]

execute=2,fmc,-1.000000,

execute=4,laminar/B738/toggle_switch/fmc_source_left,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.FmcSource]<[0.000000]

calc=[0.000000]

execute=2,fmc,-1.000000,

execute=4,laminar/B738/toggle_switch/fmc_source_right,0.000000,

logic:

calc=[0.000000]

execute=2,irs-disp,-1.000000,

out=Source,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.SourceAuto]>[0.000000]

calc=[0.000000]

execute=2,source,-1.000000,

execute=4,laminar/B738/toggle_switch/dspl_source_left,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.SourceAuto]<[0.000000]

calc=[0.000000]

execute=2,source,-1.000000,

execute=4,laminar/B738/toggle_switch/dspl_source_right,0.000000,

logic:

calc=[0.000000]

execute=2,cp-disp,-1.000000,

out=CtrPanel,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.ControlSource]>[0.000000]

calc=[0.000000]

execute=2,ctr-panel,-1.000000,

execute=4,laminar/B738/toggle_switch/dspl_ctrl_pnl_left,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.ControlSource]<[0.000000]

calc=[0.000000]

execute=2,ctr-panel,-1.000000,

execute=4,laminar/B738/toggle_switch/dspl_ctrl_pnl_right,0.000000,

logic:

calc=[0.000000]

execute=2,cp-disp,-1.000000,

out=CrossFeed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.CrossFeedSW]>[0.000000]

calc=[0.000000]

execute=2,crossfeed,-1.000000,

execute=4,laminar/B738/toggle_switch/crossfeed_valve_off,0.000000,

logic:

[SYSTEMS.FUEL.CrossFeedSW]==[0.000000]

calc=[0.000000]

execute=2,cr-feed,-1.000000,

logic:

calc=[0.000000]

out=Pump1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LAftPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,aft-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft1,0.000000,

execute=2,aft-l-off,0.000000,

logic:

calc=[0.000000]

execute=2,f-aft-l,-1.000000,

out=Pump2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,fwd-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft2,0.000000,

execute=2,fwd-l-off,0.000000,

logic:

calc=[0.000000]

execute=2,f-ctr-l,-1.000000,

out=Pump3,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RFwdPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,fwd-r-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_rgt2,0.000000,

execute=2,fwd-r-off,0.000000,

logic:

calc=[0.000000]

execute=2,f-ctr-r,-1.000000,

out=Pump4,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RAftPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,aft-r-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_rgt1,0.000000,

execute=2,aft-r-off,0.000000,

logic:

calc=[0.000000]

execute=2,f-aft-r,-1.000000,

out=Pump5,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LCtrPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,ctr-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr1,0.000000,

execute=2,ctr-l-off,0.000000,

logic:

calc=[0.000000]

execute=2,f-ctr-l,-1.000000,

out=Pump6,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RCtrPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,ctr-r-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr2,0.000000,

execute=2,ctr-r-off,0.000000,

logic:

calc=[0.000000]

execute=2,f-ctr-r,-1.000000,

out=Util,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.CabUtil]==[0.000000]

calc=[0.000000]

execute=2,util-off,-1.000000,

execute=8,laminar/B738/toggle_switch/cab_util_pos,1.000000,

execute=2,util-on,-1.000000,

logic:

[SYSTEMS.ELEC.CabUtil]==[1.000000]

calc=[0.000000]

execute=2,utilcab,-1.000000,

logic:

calc=[0.000000]

out=Pass,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.IfePass]==[0.000000]

calc=[0.000000]

execute=2,ife-off,-1.000000,

execute=8,laminar/B738/toggle_switch/ife_pass_seat_pos,1.000000,

execute=2,ife-on,0.000000,

logic:

[SYSTEMS.ELEC.IfePass]==[1.000000]

calc=[0.000000]

execute=2,utilcab,-1.000000,

logic:

calc=[0.000000]

out=StbyPower,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.StandbyPowerPB]!=[1.000000]

calc=[0.000000]

execute=2,stby-off,-1.000000,

execute=8,laminar/B738/electric/standby_bat_pos,1.000000,

execute=4,laminar/B738/button_switch_cover03,0.000000,

execute=2,stby-on,0.000000,

logic:

[SYSTEMS.ELEC.StandbyPowerPB]==[1.000000]

calc=[0.000000]

execute=2,stndpower,-1.000000,

logic:

calc=[0.000000]

out=Drive1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.Gen1DiscCover]==[1.000000]

&&

[SYSTEMS.ELEC.Gen1Disc]==[0.000000]

calc=[0.000000]

execute=2,drive1,-1.000000,

execute=4,laminar/B738/button_switch_cover04,0.000000,

logic:

[SYSTEMS.ELEC.Gen1DiscCover]==[1.000000]

&&

[SYSTEMS.ELEC.Gen1Disc]==[1.000000]

calc=[0.000000]

execute=2,drive1,-1.000000,

execute=4,laminar/B738/one_way_switch/drive_disconnect1_off,0.000000,

execute=7,,0.300000,

execute=4,laminar/B738/button_switch_cover04,0.000000,

logic:

[SYSTEMS.ELEC.Gen1DiscCover]==[0.000000]

&&

[SYSTEMS.ELEC.Gen1Disc]==[1.000000]

calc=[0.000000]

execute=2,drive1,-1.000000,

execute=4,laminar/B738/button_switch_cover04,0.000000,

execute=7,,0.300000,

execute=4,laminar/B738/one_way_switch/drive_disconnect1_off,0.000000,

execute=4,laminar/B738/button_switch_cover04,0.000000,

logic:

[SYSTEMS.ELEC.Gen1DiscCover]==[0.000000]

&&

[SYSTEMS.ELEC.Gen1Disc]==[0.000000]

calc=[0.000000]

execute=2,stndpower,-1.000000,

logic:

calc=[0.000000]

out=Drive2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.Gen2DiscCover]==[1.000000]

&&

[SYSTEMS.ELEC.Gen2Disc]==[0.000000]

calc=[0.000000]

execute=2,drive2,-1.000000,

execute=4,laminar/B738/button_switch_cover05,0.000000,

logic:

[SYSTEMS.ELEC.Gen2DiscCover]==[1.000000]

&&

[SYSTEMS.ELEC.Gen2Disc]==[1.000000]

calc=[0.000000]

execute=2,drive2,-1.000000,

execute=4,laminar/B738/one_way_switch/drive_disconnect2_off,0.000000,

execute=7,,0.300000,

execute=4,laminar/B738/button_switch_cover05,0.000000,

logic:

[SYSTEMS.ELEC.Gen2DiscCover]==[0.000000]

&&

[SYSTEMS.ELEC.Gen2Disc]==[1.000000]

calc=[0.000000]

execute=2,drive2,-1.000000,

execute=4,laminar/B738/button_switch_cover05,0.000000,

execute=7,,0.300000,

execute=4,laminar/B738/one_way_switch/drive_disconnect2_off,0.000000,

execute=4,laminar/B738/button_switch_cover05,0.000000,

logic:

[SYSTEMS.ELEC.Gen2DiscCover]==[0.000000]

&&

[SYSTEMS.ELEC.Gen2Disc]==[0.000000]

calc=[0.000000]

execute=2,stndpower,-1.000000,

logic:

calc=[0.000000]

out=BusTrans,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.BasTransCover]==[0.000000]

&&

[SYSTEMS.ELEC.BusTransSW]==[1.000000]

calc=[0.000000]

execute=2,bustransf,-1.000000,

logic:

[SYSTEMS.ELEC.BasTransCover]==[0.000000]

&&

[SYSTEMS.ELEC.BusTransSW]==[0.000000]

calc=[0.000000]

execute=2,busoff,-1.000000,

execute=4,laminar/B738/button_switch_cover06,0.000000,

execute=8,sim/cockpit2/electrical/cross_tie,1.000000,

execute=7,,1.000000,

execute=4,laminar/B738/button_switch_cover06,0.000000,

execute=2,buson,-1.000000,

logic:

[SYSTEMS.ELEC.BasTransCover]==[1.000000]

&&

[0.000000]==[1.000000]

calc=[0.000000]

execute=2,bus-off,-1.000000,

execute=4,laminar/B738/button_switch_cover06,0.000000,

execute=2,bus-on,0.000000,

logic:

[SYSTEMS.ELEC.BasTransCover]==[1.000000]

&&

[SYSTEMS.ELEC.BusTransSW]==[0.000000]

calc=[0.000000]

execute=2,bus-off,-1.000000,

execute=8,sim/cockpit2/electrical/cross_tie,1.000000,

execute=4,laminar/B738/button_switch_cover06,0.000000,

execute=2,bus-on,0.000000,

logic:

calc=[0.000000]

out=Wiper1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WiperL]!=[0.000000]

calc=[0.000000]

execute=2,wiper1-low,-1.000000,

execute=4,laminar/B738/knob/left_wiper_dn,0.000000,

execute=4,laminar/B738/knob/left_wiper_dn,0.000000,

execute=4,laminar/B738/knob/left_wiper_dn,0.000000,

execute=2,wiper1-off,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.WiperL]==[0.000000]

calc=[0.000000]

execute=2,wiper1,-1.000000,

logic:

calc=[0.000000]

out=Wiper2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WiperR]!=[0.000000]

calc=[0.000000]

execute=2,wiper2-low,-1.000000,

execute=4,laminar/B738/knob/right_wiper_dn,0.000000,

execute=4,laminar/B738/knob/right_wiper_dn,0.000000,

execute=4,laminar/B738/knob/right_wiper_dn,0.000000,

execute=2,wiper2-off,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.WiperR]==[0.000000]

calc=[0.000000]

execute=2,wiper2,-1.000000,

logic:

calc=[0.000000]

out=EquipCool_S,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.EquipCool_S]==[1.000000]

calc=[0.000000]

execute=2,sup-altn,-1.000000,

execute=8,laminar/B738/toggle_switch/eq_cool_supply,0.000000,

execute=2,sup-norm,0.000000,

logic:

[SYSTEMS.OVHDSIDEL.EquipCool_S]==[0.000000]

calc=[0.000000]

execute=2,equipcool,-1.000000,

logic:

calc=[0.000000]

out=EquipCool_E,integer,,0.000000,,,,,,,,0,,

logic:

[PROCEDURES.Preflight.EquipCool_E]==[1.000000]

calc=[0.000000]

execute=2,exh-altn,-1.000000,

execute=8,laminar/B738/toggle_switch/eq_cool_exhaust,0.000000,

execute=2,exh-norm,0.000000,

logic:

[PROCEDURES.Preflight.EquipCool_E]==[0.000000]

calc=[0.000000]

execute=2,equipcool,-1.000000,

logic:

calc=[0.000000]

out=EmerExit,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.EmerExitSW]!=[0.000000]

calc=[0.000000]

execute=2,exiton,-1.000000,

execute=4,laminar/B738/push_button/emer_exit_full_off,0.000000,

execute=2,exitoff,0.000000,

logic:

[SYSTEMS.LIGHTS.EmerExitSW]==[0.000000]

calc=[0.000000]

execute=2,emerexit,-1.000000,

logic:

calc=[0.000000]

out=Chimes,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_NoSmokeSW]!=[0.000000]

calc=[0.000000]

execute=2,chimes-on,-1.000000,

execute=4,laminar/B738/toggle_switch/no_smoking_up,0.000000,

execute=2,chimes-off,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_NoSmokeSW]==[0.000000]

calc=[0.000000]

execute=2,chime,-1.000000,

logic:

calc=[0.000000]

out=FastenBelt,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_SeatBeltsSW]==[2.000000]

calc=[0.000000]

execute=2,belt-on,-1.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_up,0.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_up,0.000000,

execute=2,belt-off,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_SeatBeltsSW]==[1.000000]

calc=[0.000000]

execute=2,belt-auto,-1.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_up,0.000000,

execute=2,belt-off,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_SeatBeltsSW]==[0.000000]

calc=[0.000000]

execute=2,chime,-1.000000,

logic:

calc=[0.000000]

out=Heat1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WHeatLSide]!=[0.000000]

calc=[0.000000]

execute=2,wh1-on,-1.000000,

execute=4,laminar/B738/toggle_switch/window_heat_l_side,0.000000,

execute=2,wh1-off,0.000000,

logic:

calc=[0.000000]

execute=2,wh1,-1.000000,

out=Heat2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WHeatLFwd]!=[0.000000]

calc=[0.000000]

execute=2,wh2-off,-1.000000,

execute=4,laminar/B738/toggle_switch/window_heat_l_fwd,0.000000,

execute=2,wh2-off,0.000000,

logic:

calc=[0.000000]

execute=2,wh2,-1.000000,

out=Heat3,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WHeatRFwd]!=[0.000000]

calc=[0.000000]

execute=2,wh3-on,-1.000000,

execute=4,laminar/B738/toggle_switch/window_heat_r_fwd,0.000000,

execute=2,wh3-off,0.000000,

logic:

calc=[0.000000]

execute=2,wh3,-1.000000,

out=Heat4,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WHeatRSide]!=[0.000000]

calc=[0.000000]

execute=2,wh4-on,-1.000000,

execute=4,laminar/B738/toggle_switch/window_heat_r_side,0.000000,

execute=2,wh4-off,0.000000,

logic:

calc=[0.000000]

execute=2,wh4,-1.000000,

out=Probe_A,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.ProbeHeatA]!=[0.000000]

calc=[0.000000]

execute=2,probeaon,-1.000000,

execute=8,laminar/B738/toggle_switch/capt_probes_pos,0.000000,

execute=2,probeaoff,0.000000,

logic:

calc=[0.000000]

execute=2,probeheat,-1.000000,

out=Probe_B,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.ProbeHeatB]!=[0.000000]

calc=[0.000000]

execute=2,probebon,-1.000000,

execute=8,laminar/B738/toggle_switch/fo_probes_pos,0.000000,

execute=2,probeboff,0.000000,

logic:

calc=[0.000000]

execute=2,probeheat,-1.000000,

out=WingAntiIce,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.WingPB]==[0.000000]

calc=[0.000000]

execute=2,wing-ice,-1.000000,

logic:

[SYSTEMS.ICE.WingPB]>[0.000000]

calc=[0.000000]

execute=2,wice-on,-1.000000,

execute=4,laminar/B738/toggle_switch/wing_heat,0.000000,

execute=2,wice-off,0.000000,

logic:

calc=[0.000000]

out=Eng1AntiIce,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.ENG1IcePB]==[1.000000]

calc=[0.000000]

execute=2,e1ice-on,-1.000000,

execute=8,laminar/B738/ice/eng1_heat_pos,0.000000,

execute=2,e1ice-off,0.000000,

logic:

[SYSTEMS.ICE.ENG1IcePB]==[0.000000]

calc=[0.000000]

execute=2,eng-ice,-1.000000,

logic:

calc=[0.000000]

out=Eng2AntiIce,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.ENG2IcePB]==[1.000000]

calc=[0.000000]

execute=2,e2ice-on,-1.000000,

execute=8,laminar/B738/ice/eng2_heat_pos,0.000000,

execute=2,e2ice-off,0.000000,

logic:

[SYSTEMS.ICE.ENG2IcePB]==[0.000000]

calc=[0.000000]

execute=2,eng-ice,-1.000000,

logic:

calc=[0.000000]

out=HydEng1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.Eng1PumpSW]!=[0.000000]

calc=[0.000000]

execute=2,hydeng1on,-1.000000,

execute=8,laminar/B738/toggle_switch/hydro_pumps1_pos,0.000000,

execute=2,hydeng1off,0.000000,

logic:

calc=[0.000000]

execute=2,lhydpump,-1.000000,

out=HydElec2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.ElecPump2]!=[0.000000]

calc=[0.000000]

execute=2,helec2on,-1.000000,

execute=8,laminar/B738/toggle_switch/electric_hydro_pumps1_pos,0.000000,

execute=2,helec2off,0.000000,

logic:

calc=[0.000000]

execute=2,2ehydpump,-1.000000,

out=HydElec1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.ElecPump1]!=[0.000000]

calc=[0.000000]

execute=2,helec1on,-1.000000,

execute=8,laminar/B738/toggle_switch/electric_hydro_pumps2_pos,0.000000,

execute=2,helec1off,0.000000,

logic:

calc=[0.000000]

execute=2,1ehydpump,-1.000000,

out=HydEng2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.Eng2PumpSW]!=[0.000000]

calc=[0.000000]

execute=2,hydeng2on,-1.000000,

execute=8,laminar/B738/toggle_switch/hydro_pumps2_pos,0.000000,

execute=2,hydeng2off,0.000000,

logic:

calc=[0.000000]

execute=2,rhydpump,-1.000000,

out=TrimAir,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.TrimAir]==[1.000000]

calc=[0.000000]

execute=2,trim-on,-1.000000,

execute=8,laminar/B738/air/trim_air_pos,0.000000,

execute=2,trim-off,0.000000,

logic:

[SYSTEMS.AIR.TrimAir]==[0.000000]

calc=[0.000000]

execute=2,condition,-1.000000,

logic:

calc=[0.000000]

out=ContCab,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.ContCabTempSW]!=[0.500000]

calc=[0.000000]

execute=2,cont-cab,-1.000000,

execute=8,laminar/B738/air/cont_cab_temp/rheostat,0.500000,

logic:

[SYSTEMS.AIR.ContCabTempSW]==[0.500000]

calc=[0.000000]

execute=2,tempcont1,-1.000000,

logic:

calc=[0.000000]

out=FwdCab,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.FwdCabinTempSW]!=[0.500000]

calc=[0.000000]

execute=2,fwd-cab,-1.000000,

execute=8,laminar/B738/air/fwd_cab_temp/rheostat,0.500000,

logic:

[SYSTEMS.AIR.FwdCabinTempSW]==[0.500000]

calc=[0.000000]

execute=2,tempcont1,-1.000000,

logic:

calc=[0.000000]

out=AftCab,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.AftCabinTempSW]!=[0.500000]

calc=[0.000000]

execute=2,aft-cab,-1.000000,

execute=8,laminar/B738/air/aft_cab_temp/rheostat,0.500000,

logic:

[SYSTEMS.AIR.AftCabinTempSW]==[0.500000]

calc=[0.000000]

execute=2,tempcont1,-1.000000,

logic:

calc=[0.000000]

out=L_Fan,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.L_Fan]==[1.000000]

calc=[0.000000]

execute=2,fan-l-on,-1.000000,

execute=8,laminar/B738/air/l_recirc_fan_pos,0.000000,

execute=2,fan-l-off,0.000000,

logic:

[SYSTEMS.AIR.L_Fan]==[0.000000]

calc=[0.000000]

execute=2,recircfan,-1.000000,

logic:

calc=[0.000000]

out=R_Fan,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.R_Fan]==[1.000000]

calc=[0.000000]

execute=2,fan-r-on,-1.000000,

execute=8,laminar/B738/air/r_recirc_fan_pos,0.000000,

execute=2,fan-r-off,0.000000,

logic:

[SYSTEMS.AIR.R_Fan]==[0.000000]

calc=[0.000000]

execute=2,recircfan,-1.000000,

logic:

calc=[0.000000]

out=L_Pack,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Pack1]==[1.000000]

calc=[0.000000]

execute=2,pack-1-aut,-1.000000,

execute=8,laminar/B738/air/l_pack_pos,0.000000,

execute=2,pack-1-off,0.000000,

logic:

[SYSTEMS.AIR.Pack1]==[2.000000]

calc=[0.000000]

execute=2,pack-1-hig,-1.000000,

execute=8,laminar/B738/air/l_pack_pos,0.000000,

execute=2,pack-1-off,0.000000,

logic:

[SYSTEMS.AIR.Pack1]==[0.000000]

calc=[0.000000]

execute=2,lpack,-1.000000,

logic:

calc=[0.000000]

out=R_Pack,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Pack2]==[1.000000]

calc=[0.000000]

execute=2,pack-2-aut,-1.000000,

execute=8,laminar/B738/air/r_pack_pos,0.000000,

execute=2,pack-2-off,0.000000,

logic:

[SYSTEMS.AIR.Pack2]==[2.000000]

calc=[0.000000]

execute=2,pack-2-hig,-1.000000,

execute=8,laminar/B738/air/r_pack_pos,0.000000,

execute=2,pack-2-off,0.000000,

logic:

[SYSTEMS.AIR.Pack2]==[0.000000]

calc=[0.000000]

execute=2,rpack,-1.000000,

logic:

calc=[0.000000]

out=IzolValve,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.IsolValve]==[2.000000]

calc=[0.000000]

execute=2,isol-v-ope,-1.000000,

execute=8,laminar/B738/air/isolation_valve_pos,0.000000,

execute=2,isol-v-off,0.000000,

logic:

[SYSTEMS.AIR.IsolValve]==[0.000000]

calc=[0.000000]

execute=2,lsolvalv,-1.000000,

logic:

[SYSTEMS.AIR.IsolValve]==[1.000000]

calc=[0.000000]

execute=2,isol-v-aut,-1.000000,

execute=8,laminar/B738/air/isolation_valve_pos,0.000000,

execute=2,isol-v-off,0.000000,

logic:

calc=[0.000000]

out=Bleed1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Eng1BleedSW]!=[0.000000]

calc=[0.000000]

execute=2,bleed1-on,-1.000000,

execute=8,laminar/B738/toggle_switch/bleed_air_1_pos,0.000000,

execute=2,bleed1-off,0.000000,

logic:

[SYSTEMS.AIR.Eng1BleedSW]==[0.000000]

calc=[0.000000]

execute=2,lbleed,-1.000000,

logic:

calc=[0.000000]

out=Bleed2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Eng2BleedSW]!=[0.000000]

calc=[0.000000]

execute=2,bleed2-on,-1.000000,

execute=8,laminar/B738/toggle_switch/bleed_air_2_pos,0.000000,

execute=2,bleed2-off,0.000000,

logic:

[SYSTEMS.AIR.Eng2BleedSW]==[0.000000]

calc=[0.000000]

execute=2,rbleed,-1.000000,

logic:

calc=[0.000000]

out=ApuBleed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.APUBleedSW]==[1.000000]

calc=[0.000000]

execute=2,apubleedon,0.000000,

execute=8,laminar/B738/toggle_switch/bleed_air_apu_pos,0.000000,

execute=2,apuble-off,0.000000,

logic:

[SYSTEMS.AIR.APUBleedSW]==[0.000000]

calc=[0.000000]

execute=2,apubleed,-1.000000,

logic:

calc=[0.000000]

out=Altn,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDER.PressModeSel]<=[1.000000]

calc=[0.000000]

execute=2,altnpress,-1.000000,

logic:

[SYSTEMS.OVHDSIDER.PressModeSel]==[2.000000]

calc=[0.000000]

execute=2,altn-man,-1.000000,

execute=4,laminar/B738/toggle_switch/air_valve_ctrl_left,0.000000,

execute=2,altn-auto,0.000000,

logic:

[SYSTEMS.OVHDSIDER.PressModeSel]==[3.000000]

calc=[0.000000]

execute=2,altn-man,-1.000000,

execute=4,laminar/B738/toggle_switch/air_valve_ctrl_left,0.000000,

execute=4,laminar/B738/toggle_switch/air_valve_ctrl_left,0.000000,

execute=2,altn-auto,0.000000,

logic:

calc=[0.000000]

out=Lights1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_LandLSW]!=[0.000000]

||

[SYSTEMS.LIGHTS.OVHD_LandRSW]!=[0.000000]

||

[SYSTEMS.LIGHTS.OVHD_LandLRetr]!=[0.000000]

||

[SYSTEMS.LIGHTS.OVHD_LandRRetr]!=[0.000000]

calc=[0.000000]

execute=2,all-1-on,-1.000000,

execute=4,laminar/B738/switch/land_lights_ret_right_up,0.000000,

execute=4,laminar/B738/switch/land_lights_ret_right_up,0.000000,

execute=4,laminar/B738/switch/land_lights_ret_left_up,0.000000,

execute=4,laminar/B738/switch/land_lights_ret_left_up,0.000000,

execute=8,laminar/B738/switch/land_lights_left_pos,0.000000,

execute=8,laminar/B738/switch/land_lights_right_pos,0.000000,

execute=2,all-1-off,0.000000,

logic:

calc=[0.000000]

execute=2,landlight,-1.000000,

out=Lights2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_RwyLeftSW]==[1.000000]

calc=[0.000000]

execute=2,runwayonl,-1.000000,

execute=4,laminar/B738/switch/rwy_light_left_off,0.000000,

execute=2,runwayoffl,0.000000,

logic:

calc=[0.000000]

execute=2,taxilight,-1.000000,

out=Lights3,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_RwyRightSW]==[1.000000]

calc=[0.000000]

execute=2,runwayonr,-1.000000,

execute=4,laminar/B738/switch/rwy_light_right_off,0.000000,

execute=2,runwayoffr,0.000000,

logic:

calc=[0.000000]

execute=2,taxilight,-1.000000,

out=Lights4,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_TaxiSW]!=[0.000000]

calc=[0.000000]

execute=2,taxi-on,-1.000000,

execute=4,laminar/B738/toggle_switch/taxi_light_brightness_pos_up,0.000000,

execute=4,laminar/B738/toggle_switch/taxi_light_brightness_pos_up,0.000000,

execute=2,taxi-off,0.000000,

logic:

calc=[0.000000]

execute=2,taxilight,-1.000000,

out=Lights5,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_LogoSW]!=[0.000000]

calc=[0.000000]

execute=2,logo-on,-1.000000,

execute=8,laminar/B738/toggle_switch/logo_light,0.000000,

execute=2,logo-off,0.000000,

logic:

calc=[0.000000]

execute=2,logolight,-1.000000,

out=Lights6,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_NavSW]==[1.000000]

calc=[0.000000]

execute=2,strobe-on,-1.000000,

execute=4,laminar/B738/toggle_switch/position_light_down,0.000000,

execute=2,strobe-off,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_NavSW]==[-1.000000]

calc=[0.000000]

execute=2,strobe-nav,-1.000000,

execute=4,laminar/B738/toggle_switch/position_light_up,0.000000,

execute=2,strobe-off,0.000000,

logic:

calc=[0.000000]

execute=2,nav,-1.000000,

out=Lights7,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_BeaconSW]!=[0.000000]

calc=[0.000000]

execute=2,beacon-on,-1.000000,

execute=8,sim/cockpit/electrical/beacon_lights_on,0.000000,

execute=2,beacon-off,0.000000,

logic:

calc=[0.000000]

execute=2,beacon,-1.000000,

out=Lights8,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_WingSW]!=[0.000000]

calc=[0.000000]

execute=2,wing-on,-1.000000,

execute=4,laminar/B738/switch/wing_light_off,0.000000,

execute=2,wing-off,0.000000,

logic:

calc=[0.000000]

execute=2,winglight,-1.000000,

out=Lights9,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_WheelSW]!=[0.000000]

calc=[0.000000]

execute=2,well-on,-1.000000,

execute=8,sim/cockpit2/switches/generic_lights_switch[5],0.000000,

execute=2,well-off,0.000000,

logic:

calc=[0.000000]

execute=2,welllight,-1.000000,

out=Eng1Start,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng1StartSW]>[1.000000]

calc=[0.000000]

execute=2,start1cont,-1.000000,

execute=4,laminar/B738/rotary/eng1_start_off,0.000000,

execute=2,start1auto,0.000000,

logic:

[SYSTEMS.ENGINE.EngMasterSW_1]<[1.000000]

calc=[0.000000]

execute=2,start1grd,-1.000000,

execute=4,laminar/B738/rotary/eng1_start_off,0.000000,

execute=2,start1auto,0.000000,

logic:

calc=[0.000000]

execute=2,lengstart,-1.000000,

out=Eng2Start,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng2StartSW]<[1.000000]

calc=[0.000000]

execute=2,start2grd,-1.000000,

execute=4,laminar/B738/rotary/eng2_start_off,0.000000,

execute=2,start2auto,0.000000,

logic:

[SYSTEMS.ENGINE.EngMasterSW_2]>[1.000000]

calc=[0.000000]

execute=2,start2cont,-1.000000,

execute=4,laminar/B738/rotary/eng2_start_off,0.000000,

execute=2,start2auto,0.000000,

logic:

calc=[0.000000]

execute=2,rengstart,-1.000000,

out=FD,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MCP.FD2]==[1.000000]

calc=[0.000000]

execute=2,look-frd,-1.000000,

execute=2,fd-on,-1.000000,

execute=4,laminar/B738/autopilot/flight_director_fo_toggle,0.000000,

logic:

[SYSTEMS.MCP.FD2]==[0.000000]

calc=[0.000000]

execute=2,look-frd,-1.000000,

logic:

calc=[0.000000]

out=RW,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.PEDESTAL.RadarSWFo]==[1.000000]

calc=[0.000000]

execute=2,wxr,-1.000000,

execute=4,laminar/B738/EFIS_control/fo/push_button/wxr_press,0.000000,

logic:

[SYSTEMS.PEDESTAL.RadarSWFo]==[0.000000]

calc=[0.000000]

execute=2,look-frd,-1.000000,

logic:

calc=[0.000000]

out=MPDisplay,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FRONTPANEL.MainPanelDisplay]==[-1.000000]

calc=[0.000000]

execute=2,dus-norm,-1.000000,

execute=4,laminar/B738/toggle_switch/main_pnl_du_fo_left,0.000000,

logic:

[SYSTEMS.FRONTPANEL.MainPanelDisplay]==[0.000000]

calc=[0.000000]

execute=2,look-pfd,-1.000000,

logic:

[SYSTEMS.FRONTPANEL.MainPanelDisplay]==[1.000000]

calc=[0.000000]

execute=2,dus-norm,-1.000000,

execute=4,laminar/B738/toggle_switch/main_pnl_du_fo_right,0.000000,

logic:

calc=[0.000000]

out=LDisplay,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FRONTPANEL.LowerDisplay]==[1.000000]

calc=[0.000000]

execute=2,du-norm,-1.000000,

execute=4,laminar/B738/toggle_switch/lower_du_fo_right,0.000000,

logic:

[SYSTEMS.FRONTPANEL.LowerDisplay]==[0.000000]

calc=[0.000000]

execute=2,look-pfd,-1.000000,

logic:

[SYSTEMS.FRONTPANEL.LowerDisplay]==[2.000000]

calc=[0.000000]

execute=2,du-norm,-1.000000,

execute=4,laminar/B738/toggle_switch/lower_du_fo_left,0.000000,

logic:

calc=[0.000000]

out=GPWS,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FRONTPANEL.GPWSFlap]!=[0.000000]

calc=[0.000000]

execute=2,look-cdu,-1.000000,

execute=2,gpws-on,-1.000000,

execute=4,laminar/B738/toggle_switch/gpws_flap_cover,0.000000,

execute=2,gpws-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=GPWS1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FRONTPANEL.GPWSGear]!=[0.000000]

calc=[0.000000]

execute=2,look-cdu,-1.000000,

execute=2,gpws-on,-1.000000,

execute=4,laminar/B738/toggle_switch/gpws_gear_cover,0.000000,

execute=2,gpws-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=GPWS2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FRONTPANEL.GPWSTerr]!=[0.000000]

calc=[0.000000]

execute=2,look-cdu,-1.000000,

execute=2,gpws-on,-1.000000,

execute=4,laminar/B738/toggle_switch/gpws_terr_cover,0.000000,

execute=2,gpws-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=LG,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LG.LG_Lever]!=[1.000000]

calc=[0.000000]

execute=2,look-front,-1.000000,

execute=2,lg-off,-1.000000,

execute=8,laminar/B738/controls/gear_handle_down,1.000000,

execute=2,lg-down,0.000000,

logic:

[SYSTEMS.LG.LG_Lever]==[1.000000]

calc=[0.000000]

execute=2,look-front,-1.000000,

logic:

calc=[0.000000]

out=AutoBrake,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.BRAKES.AutoBrakeSW]>[1.000000]

calc=[0.000000]

execute=2,brake-1,-1.000000,

execute=4,laminar/B738/knob/autobrake_off,0.000000,

execute=2,brake-off,0.000000,

logic:

[SYSTEMS.BRAKES.AutoBrakeSW]<[1.000000]

calc=[0.000000]

execute=2,brake-rto,-1.000000,

execute=4,laminar/B738/knob/autobrake_off,0.000000,

execute=2,brake-off,0.000000,

logic:

[SYSTEMS.BRAKES.AutoBrakeSW]==[1.000000]

calc=[0.000000]

execute=2,look-front,-1.000000,

logic:

calc=[0.000000]

out=Vspeeds,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FRONTPANEL.VrefSet]!=[0.000000]

calc=[0.000000]

execute=2,spd-ref,-1.000000,

execute=8,laminar/B738/toggle_switch/spd_ref,0.000000,

logic:

[SYSTEMS.FRONTPANEL.VrefSet]==[0.000000]

calc=[0.000000]

execute=2,look-front,-1.000000,

logic:

calc=[0.000000]

out=N1Set,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FRONTPANEL.N1Set]!=[0.000000]

calc=[0.000000]

execute=2,n1-set,-1.000000,

execute=8,laminar/B738/toggle_switch/n1_set_source,0.000000,

logic:

[SYSTEMS.FRONTPANEL.N1Set]==[0.000000]

calc=[0.000000]

execute=2,look-front,-1.000000,

logic:

calc=[0.000000]

out=FuelFlow,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,flow-off,-1.000000,

execute=8,laminar/B738/toggle_switch/fuel_flow_pos,-1.000000,

execute=2,flow-reset,0.000000,

execute=7,,1.000000,

execute=2,flow-off,0.000000,

execute=8,laminar/B738/toggle_switch/fuel_flow_pos,0.000000,

logic:

calc=[0.000000]

out=Transponder,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.PEDESTAL.Transponder]!=[1.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

execute=2,tcas-tara,-1.000000,

execute=4,laminar/B738/knob/transponder_stby,0.000000,

execute=2,tcas-test,-1.000000,

logic:

[SYSTEMS.PEDESTAL.Transponder]==[1.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

logic:

calc=[0.000000]

out=Audio,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ACP.Com1On]!=[1.000000]

calc=[0.000000]

execute=2,vhf-1on,-1.000000,

execute=4,laminar/B738/comm/fo_com1_audio_sel,0.000000,

execute=8,laminar/B738/comm/fo_audio_vol_com1,1.000000,

logic:

[SYSTEMS.ACP.Com1On]==[1.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

logic:

calc=[0.000000]

out=Audio1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ACP.Com2On]!=[1.000000]

calc=[0.000000]

execute=2,vhf-2on,-1.000000,

execute=4,laminar/B738/comm/fo_com2_audio_sel,0.000000,

execute=8,laminar/B738/comm/fo_audio_vol_com2,1.000000,

logic:

[SYSTEMS.ACP.Com2On]==[1.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

logic:

calc=[0.000000]

out=Audio2,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,vhf-2,-1.000000,

execute=4,laminar/B738/audio/fo/mic_push2,0.000000,

logic:

calc=[0.000000]

out=TrimLock1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.PEDESTAL.TrimLock1]==[0.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

logic:

[SYSTEMS.PEDESTAL.TrimLock1]!=[0.000000]

calc=[0.000000]

execute=2,trimlock1,-1.000000,

execute=4,laminar/B738/toggle_switch/el_trim_lock,0.000000,

logic:

calc=[0.000000]

out=TrimLock2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.PEDESTAL.TrimLock2]==[0.000000]

calc=[0.000000]

execute=2,look-ped,-1.000000,

logic:

[SYSTEMS.PEDESTAL.TrimLock2]!=[0.000000]

calc=[0.000000]

execute=2,trimlock2,-1.000000,

execute=4,laminar/B738/toggle_switch/ap_trim_lock,0.000000,

logic:

calc=[0.000000]

out=ApuGen1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.APUGen1Bus]==[1.000000]

calc=[0.000000]

execute=2,apu1-on,-1.000000,

execute=4,laminar/B738/toggle_switch/apu_gen1_up,0.000000,

execute=2,apu1-cntr,0.000000,

logic:

[SYSTEMS.ELEC.APUGen1Bus]==[0.000000]

calc=[0.000000]

execute=2,gencheck,-1.000000,

logic:

calc=[0.000000]

out=ApuGen2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.APUGen2Bus]==[1.000000]

calc=[0.000000]

execute=2,apu2-on,-1.000000,

execute=4,laminar/B738/toggle_switch/apu_gen2_up,0.000000,

execute=2,apu2-cntr,0.000000,

logic:

[SYSTEMS.ELEC.APUGen2Bus]==[0.000000]

calc=[0.000000]

execute=2,gencheck,-1.000000,

logic:

calc=[0.000000]

out=ApuOff,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.APU.AvailAPU]==[0.000000]

calc=[0.000000]

execute=2,apu,-1.000000,

logic:

[SYSTEMS.APU.AvailAPU]==[1.000000]

calc=[0.000000]

execute=2,apu-cntr,-1.000000,

execute=4,laminar/B738/spring_toggle_switch/APU_start_pos_up,0.000000,

execute=4,laminar/B738/spring_toggle_switch/APU_start_pos_up,0.000000,

execute=2,apu-off,0.000000,

logic:

calc=[0.000000]

out=DomeLight,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_DomeSW]==[1.000000]

calc=[0.000000]

execute=2,domewhite,-1.000000,

execute=4,laminar/B738/toggle_switch/cockpit_dome_dn,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_DomeSW]==[0.000000]

calc=[0.000000]

execute=2,ovhd-up,-1.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_DomeSW]==[-1.000000]

calc=[0.000000]

execute=2,domewhite,-1.000000,

execute=4,laminar/B738/toggle_switch/cockpit_dome_up,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Bat,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.BatterySW]!=[0.000000]

calc=[0.000000]

execute=2,batton,-1.000000,

execute=4,laminar/B738/button_switch_cover02,0.000000,

execute=7,,0.200000,

execute=8,laminar/B738/electric/battery_pos,0.000000,

execute=2,battoff,0.000000,

logic:

[SYSTEMS.ELEC.BatterySW]==[0.000000]

calc=[0.000000]

execute=2,bat,-1.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,secure procedure,-1.000000,

execute=1,Secure procedure complete,0.000000,

execute=2,rest01,-1.000000,

logic:

calc=[0.000000]

