sys=CHECKLIST



devstack=Preflight

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=preflight checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

&&

[SYSTEMS.OVHDSIDEL.IrsAlign]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,preflight checklist,-1.000000,

execute=1,Preflight checklist!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Oxygen?,0.000000,

logic:

instring=preflight checklist

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed in flight!,0.000000,

execute=3,,0.000000,

logic:

instring=preflight checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

&&

[SYSTEMS.OVHDSIDEL.IrsAlign]>[0.000000]

calc=[0.000000]

execute=2,ovhd-1,-1.000000,

execute=1,Sir; we don't have IRS align,0.000000,

execute=0,Preflight checklist is not completed!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Oxygen,integer,,0.000000,,,,,,,,0,,

logic:

instring=tested one handred persent

||

instring=any

&&

[SYSTEMS.MISC.OxygenTest]==[1.000000]

calc=[0.000000]

execute=2,chkloxy,-1.000000,

execute=1,Tested one handred percent,0.000000,

execute=2,chklread,-1.000000,

execute=1,Pressurization mode selector?,0.000000,

execute=2,chklovhdrt,-1.000000,

logic:

instring=tested one handred persent

||

instring=any

&&

[SYSTEMS.MISC.OxygenTest]!=[1.000000]

calc=[0.000000]

execute=2,chkloxy,-1.000000,

execute=1,Tested one handred percent,0.000000,

execute=2,chklanswer,-1.000000,

execute=1,You haven't tested on your side,0.000000,

execute=2,chklread,-1.000000,

execute=1,Pressurization mode selector?,0.000000,

execute=2,chklovhdrt,-1.000000,

logic:

calc=[0.000000]

out=PressSel,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.CABPRESS.PressModeSelect]<[2.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=1,Auto!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Flight instruments?,0.000000,

logic:

[SYSTEMS.CABPRESS.PressModeSelect]==[2.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,press-man,-1.000000,

execute=8,1-sim/press/modeSelector,0.000000,

execute=8,1-sim/press/modeSelector/anim,0.000000,

execute=2,press-auto,0.000000,

execute=1,Auto!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Flight instruments?,0.000000,

logic:

calc=[0.000000]

out=FlightInstr,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.ELEC.BatterySW]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Sir; we don't have power,0.000000,

execute=1,Preflight checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

instring=any

&&

[SYSTEMS.ELEC.BatterySW]==[1.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

logic:

instring=any

&&

instring=say the current course, altitude and baro 

calc=[0.000000]

logic:

calc=[0.000000]

out=FlightInstr1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[0.000000]

&&

[SYSTEMS.MCP.BaroDiffFoMOd]>[0.020000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chbarodn,-1.000000,

execute=8,jd/fo/needsetbaro,1.000000,

execute=8,jd/fo/needsetbaro,0.000000,

execute=2,chbaroup,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=0,Heading <&SYSTEMS.POSITION.HDG_ND_Fo>,0.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Altitude <SYSTEMS.POSITION.AltimFO>,0.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Altimeter <&SYSTEMS.MCP.BaroSetHpaFO>,0.000000,

execute=2,chklread,-1.000000,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[0.000000]

&&

[SYSTEMS.MCP.BaroDiffFoMOd]<[0.020000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=0,Heading <&SYSTEMS.POSITION.HDG_ND_Fo>,0.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Altitude <SYSTEMS.POSITION.AltimFO>,0.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Altimeter <&SYSTEMS.MCP.BaroSetHpaFoFloor>,0.000000,

execute=2,chklread,-1.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=FlightInstr2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[1.000000]

&&

[SYSTEMS.MCP.BaroDiffFoMOd]>[0.020000]

&&

[SYSTEMS.MCP.ChangeHPA_Cap]==[0.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chklbarodn,-1.000000,

execute=8,1-sim/ng/baroLargeR/anim,0.000000,

execute=8,1-sim/ng/baroLargeR/anim/anim,0.000000,

execute=8,jd/fo/needsetbaro,0.000000,

execute=8,jd/fo/needsetbaro1,1.000000,

execute=8,jd/fo/needsetbaro1,0.000000,

execute=2,chklbaroup,-1.000000,

execute=0,Heading <&SYSTEMS.POSITION.HDG_ND_Fo>,0.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Altitude <SYSTEMS.POSITION.AltimFO>,0.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Altimeter <&SYSTEMS.MCP.BaroSetInHgFo100>,0.000000,

execute=2,chklread,-1.000000,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[1.000000]

&&

[SYSTEMS.MCP.BaroDiffFoMOd]>[0.020000]

&&

[SYSTEMS.MCP.ChangeHPA_Cap]==[-1.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chklbarodn,-1.000000,

execute=8,1-sim/ng/baroLargeR/anim,-1.000000,

execute=8,1-sim/ng/baroLargeR/anim/anim,-1.000000,

execute=8,jd/fo/needsetbaro,0.000000,

execute=8,jd/fo/needsetbaro1,1.000000,

execute=8,jd/fo/needsetbaro1,0.000000,

execute=2,chklbaroup,-1.000000,

execute=0,Heading <&SYSTEMS.POSITION.HDG_ND_Fo>,0.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Altitude <SYSTEMS.POSITION.AltimFO>,0.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Altimeter <&SYSTEMS.MCP.BaroSetHpaFoFloor>,0.000000,

execute=2,chklread,-1.000000,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[1.000000]

&&

[SYSTEMS.MCP.BaroDiffFoMOd]<=[0.020000]

&&

[SYSTEMS.MCP.ChangeHPA_Cap]==[0.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chklbarodn,-1.000000,

execute=8,1-sim/ng/baroLargeR/anim,0.000000,

execute=8,1-sim/ng/baroLargeR/anim/anim,0.000000,

execute=2,chklbaroup,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=0,Heading <&SYSTEMS.POSITION.HDG_ND_Fo>,0.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Altitude <SYSTEMS.POSITION.AltimFO>,0.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Altimeter <&SYSTEMS.MCP.BaroSetInHgFo100>,0.000000,

execute=2,chklread,-1.000000,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[1.000000]

&&

[SYSTEMS.MCP.BaroDiffFoMOd]<=[0.020000]

&&

[SYSTEMS.MCP.ChangeHPA_Cap]==[-1.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chklbarodn,-1.000000,

execute=8,1-sim/ng/baroLargeR/anim,-1.000000,

execute=8,1-sim/ng/baroLargeR/anim/anim,-1.000000,

execute=2,chklbaroup,-1.000000,

execute=0,Heading <&SYSTEMS.POSITION.HDG_ND_Fo>,0.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Altitude <SYSTEMS.POSITION.AltimFO>,0.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Altimeter <&SYSTEMS.MCP.BaroSetHpaFoFloor>,0.000000,

execute=2,chklread,-1.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=FlightInstr3,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MCP.BaroDiffCap]>[0.020000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=2,chklanswer,-1.000000,

execute=1,Sir; your QNH barometric pressure not set correct,0.000000,

execute=2,chklread,-1.000000,

execute=1,Parking brake?,0.000000,

logic:

[SYSTEMS.MCP.BaroDiffCap]<=[0.020000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chklread,-1.000000,

execute=1,Parking brake?,0.000000,

logic:

calc=[0.000000]

out=ParkingBrake,integer,,0.000000,,,,,,,,0,,

logic:

instring=set

&&

[SYSTEMS.BRAKES.ParkBrakeHandlePos]==[1.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=7,,0.300000,

execute=2,chklread,-1.000000,

execute=1,Fuel control switches?,0.000000,

logic:

instring=set

&&

[SYSTEMS.BRAKES.ParkBrakeHandlePos]==[0.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=7,,0.300000,

execute=1,Parking brake is not set,0.000000,

execute=2,chklread,-1.000000,

execute=1,Fuel control switches?,0.000000,

logic:

calc=[0.000000]

out=EngStartLev,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.ENGINE.EngMastSumm]==[0.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=7,,0.300000,

execute=2,chklread,-1.000000,

execute=1,Gear pins?,0.000000,

logic:

instring=any

&&

[SYSTEMS.ENGINE.EngMastSumm]>[0.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=1,Fuel control switches not cutoff; Preflight checklist is not completed!!,0.000000,

execute=3,,0.000000,

logic:

instring=cutoff

&&

[0.000000]==[1.000000]

calc=[0.000000]

logic:

calc=[0.000000]

out=GearPins,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

calc=[0.000000]

execute=2,chklanswer,-1.000000,

logic:

[0.000000]==[1.000000]

&&

instring=removed

calc=[0.000000]

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,rest01,-1.000000,

execute=1,Preflight checklist completed!,0.000000,

logic:

calc=[0.000000]



devstack=BeforeStart

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=before start checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,before start checklist,-1.000000,

execute=1,Before start checklist!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Fuel?,0.000000,

logic:

instring=before start checklist

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed in flight!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=GrndEq,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.GROUNDEQUIP.AllClear]==[0.000000]

calc=[0.000000]

execute=2,chklread,-1.000000,

logic:

[SYSTEMS.GROUNDEQUIP.AllClear]!=[0.000000]

calc=[0.000000]

execute=2,chklwindow,-1.000000,

execute=0,Sir; we're still being serviced by ground vehicles.,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=0,Before start checklist is not completed!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=DoorClose,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MISC.DoorsClosed]!=[1.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=7,,1.000000,

execute=2,chklanswer,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Sir; we don't have our doors closed,0.000000,

execute=2,rest01,-1.000000,

execute=0,Before start checklist is not completed!,0.000000,

execute=3,,0.000000,

logic:

[SYSTEMS.MISC.DoorsClosed]==[1.000000]

calc=[0.000000]

execute=2,chklread,-1.000000,

logic:

calc=[0.000000]

out=Fuel,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.MISC.TotalFuel]<[2500.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=1,Fuel quantity is too small for the flight. Before start checklist is not completed,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=3,,0.000000,

logic:

[0.000000]==[1.000000]

&&

instring=say fuel quantity

calc=[0.000000]

logic:

instring=any

&&

[SYSTEMS.MISC.TotalFuel]>[2500.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=2,chklread,-1.000000,

execute=1,Passenger signs?,0.000000,

logic:

calc=[0.000000]

out=Signs,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_SeatBeltsSW]==[0.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,belt-off,-1.000000,

execute=8,sim/cockpit/switches/fasten_seat_belts/anim,2.000000,

execute=2,belt-on,0.000000,

execute=1,On!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Window?,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_SeatBeltsSW]==[1.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,belt-off,-1.000000,

execute=8,sim/cockpit/switches/fasten_seat_belts/anim,2.000000,

execute=2,belt-on,0.000000,

execute=1,On!,0.000000,

execute=2,chklovhdup,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklread,-1.000000,

execute=1,Window?,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_SeatBeltsSW]==[2.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=1,On!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Window?,0.000000,

logic:

calc=[0.000000]

out=Windows,integer,,0.000000,,,,,,,,0,,

logic:

instring=locked

calc=[0.000000]

execute=2,chklwindow,-1.000000,

execute=1,locked,0.000000,

execute=2,chklread,-1.000000,

execute=1,M C P?,0.000000,

logic:

calc=[0.000000]

out=MCP1,double,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.FMS.V2]>[100.000000]

&&

[SYSTEMS.MCP.SpeedCompV2]>[1.000000]

&&

[SYSTEMS.MCP.SpeedCompV2]<[-1.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=1,The speed does not match the v2 speed from MCDU,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=0,Before start checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

instring=any

&&

[SYSTEMS.FMS.V2]>[100.000000]

&&

[SYSTEMS.MCP.SpeedCompV2]<=[1.000000]

&&

[SYSTEMS.MCP.SpeedCompV2]>=[-1.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=1,Speed <&SYSTEMS.MCP.Speed>,0.000000,

logic:

instring=any

&&

[SYSTEMS.FMS.V2]<[100.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=1,V two is not set in m c d u,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=0,Before start checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

instring=Say speed, heading and altitude to MCP panel

&&

[1.000000]==[0.000000]

calc=[0.000000]

logic:

calc=[0.000000]

out=MCP2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MCP.ALT]<[1500.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=0,Heading <&SYSTEMS.MCP.HDG>,0.000000,

execute=0,Altitude <SYSTEMS.MCP.ALT>,0.000000,

execute=0,The altitude is too low for flight,0.000000,

execute=2,chklread,-1.000000,

execute=1,Takeoff thrust?,0.000000,

logic:

[SYSTEMS.MCP.ALT]>[1500.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=0,Heading <&SYSTEMS.MCP.HDG>,0.000000,

execute=0,Altitude <SYSTEMS.MCP.ALT>,0.000000,

execute=2,chklread,-1.000000,

execute=1,Takeoff thrust?,0.000000,

logic:

calc=[0.000000]

out=TakeoffThrust,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FMS.AssumedTemp]>[0.000000]

calc=[0.000000]

execute=2,chklecam,-1.000000,

execute=1,Assumed temperature <SYSTEMS.FMS.AssumedTemp> degrees!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Takeoff speeds?,0.000000,

logic:

[SYSTEMS.FMS.AssumedTemp]<=[0.000000]

calc=[0.000000]

execute=2,chklecam,-1.000000,

execute=1,No assumed!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Takeoff speeds?,0.000000,

logic:

calc=[0.000000]

out=TakeoffSpeeds,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.FMS.SpeedsSum]<[300.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

execute=2,chcduinit,-1.000000,

execute=8,757Avionics/CDU2/init_ref,1.000000,

execute=2,chcdur6,-1.000000,

execute=8,757Avionics/CDU2/RLSK6,1.000000,

execute=2,chkl-cdu,-1.000000,

execute=1,Takeoff speeds is not set,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=0,Before start checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

instring=any

&&

[SYSTEMS.FMS.SpeedsSum]>[300.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

execute=2,chcduinit,-1.000000,

execute=8,757Avionics/CDU2/init_ref,1.000000,

execute=2,chcdur6,-1.000000,

execute=8,757Avionics/CDU2/RLSK6,1.000000,

execute=2,chkl-cdu,-1.000000,

execute=1,V one <SYSTEMS.FMS.V1>,0.000000,

execute=1,V rotate <SYSTEMS.FMS.Vr>,0.000000,

execute=1,V two <SYSTEMS.FMS.V2>,0.000000,

execute=2,chcdulegs,-1.000000,

execute=8,757Avionics/CDU2/legs,1.000000,

execute=2,chklread,-1.000000,

execute=1,CDU preflight?,0.000000,

logic:

instring=say takeoff speeds in cdu

&&

[1.000000]==[0.000000]

calc=[0.000000]

logic:

calc=[0.000000]

out=CDUPref,integer,,0.000000,,,,,,,,0,,

logic:

instring=completed

&&

[SYSTEMS.CDU.CDUPreflight]==[1.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

execute=1,Completed,0.000000,

execute=2,chklread,-1.000000,

execute=1,Rudder and aileron trim?,0.000000,

logic:

instring=completed

&&

[SYSTEMS.CDU.CDUPreflight]==[0.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

execute=1,CDU preflight is not completed,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=0,Before start checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=RudderTrim,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.PEDESTAL.RudderTrimComp]==[0.000000]

&&

[SYSTEMS.PEDESTAL.AileronTrimComp]==[0.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=7,,1.000000,

execute=2,chklread,-1.000000,

execute=1,Taxi and takeoff briefing?,0.000000,

logic:

instring=any

&&

[SYSTEMS.PEDESTAL.RudderTrimComp]==[1.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=1,Rudder trim is not zero position,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Before checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

instring=free and zero

&&

[1.000000]==[0.000000]

calc=[0.000000]

logic:

instring=any

&&

[SYSTEMS.PEDESTAL.AileronTrimComp]==[1.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=1,Rudder trim is not zero position,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Before checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=TaxiBriefing,integer,,0.000000,,,,,,,,0,,

logic:

instring=completed

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=1,Flight deck door?,0.000000,

execute=2,chklovhdrt,-1.000000,

logic:

calc=[0.000000]

out=DeckDoor,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MISC.DeckDoor]==[0.000000]

&&

[SYSTEMS.MISC.DeckDoorLock]==[0.000000]

calc=[0.000000]

execute=2,chkl-back,-1.000000,

execute=7,,1.000000,

execute=2,chklovhdrt,-1.000000,

execute=0,Closed and locked!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Red anti collision light?,0.000000,

logic:

[SYSTEMS.MISC.DeckDoor]>[0.000000]

&&

[SYSTEMS.MISC.DeckDoorLock]==[0.000000]

calc=[0.000000]

execute=2,chkl-back,-1.000000,

execute=8,anim/53/button,1.000000,

execute=8,anim/53/button/anim,1.000000,

execute=7,,1.500000,

execute=8,anim/53/button,0.000000,

execute=8,anim/53/button/anim,0.000000,

execute=7,,1.000000,

execute=2,chklovhdrt,-1.000000,

execute=0,Closed and locked!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Red anti collision light?,0.000000,

logic:

[SYSTEMS.MISC.DeckDoor]==[0.000000]

&&

[SYSTEMS.MISC.DeckDoorLock]==[1.000000]

calc=[0.000000]

execute=2,chkl-back,-1.000000,

execute=7,,1.000000,

execute=2,chklovhdrt,-1.000000,

execute=2,flt-door,-1.000000,

execute=8,anim/53/button,0.000000,

execute=8,anim/53/button/anim,0.000000,

execute=0,Closed and locked!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Red anti collision light?,0.000000,

logic:

[SYSTEMS.MISC.DeckDoor]>[0.000000]

&&

[SYSTEMS.MISC.DeckDoorLock]==[1.000000]

calc=[0.000000]

execute=2,chkl-back,-1.000000,

execute=7,,1.000000,

execute=2,chklovhdrt,-1.000000,

execute=2,flt-door,-1.000000,

execute=8,anim/53/button,0.000000,

execute=8,anim/53/button/anim,0.000000,

execute=0,Closed and locked!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Red anti collision light?,0.000000,

logic:

calc=[0.000000]

out=AntiCollision,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_BeaconSW]==[1.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=1,On,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_BeaconSW]==[0.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=2,red,-1.000000,

execute=8,anim/44/button,1.000000,

execute=8,anim/44/button/anim,1.000000,

execute=2,chklovhddn,-1.000000,

execute=1,On,0.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Before start checklist completed,0.000000,

logic:

calc=[0.000000]



devstack=BeforeTaxi

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=before taxi checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,before taxi checklist,-1.000000,

execute=1,Before taxi checklist!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Anti ice?,0.000000,

execute=2,chklovhddn,-1.000000,

logic:

instring=before taxi checklist

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed in flight!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=WingAntiIce,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.WingPB]==[1.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=1,Wing anti ice on,0.000000,

logic:

[SYSTEMS.ICE.WingPB]==[0.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=1,Wing anti ice off,0.000000,

logic:

calc=[0.000000]

out=EngAntiIce,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.ENG1IcePB]==[1.000000]

&&

[SYSTEMS.ICE.ENG2IcePB]==[0.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=1,Engine one anti ice on,0.000000,

execute=2,chklread,-1.000000,

execute=1,Left and right isolation valve?,0.000000,

logic:

[SYSTEMS.ICE.ENG1IcePB]==[0.000000]

&&

[SYSTEMS.ICE.ENG2IcePB]==[1.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=1,Engine two anti ice on,0.000000,

execute=2,chklread,-1.000000,

execute=1,Left and right isolation valve?,0.000000,

logic:

[SYSTEMS.ICE.ENG1IcePB]==[0.000000]

&&

[SYSTEMS.ICE.ENG2IcePB]==[0.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=1,Engine anti ice off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Left and right isolation valve?,0.000000,

logic:

[SYSTEMS.ICE.ENG1IcePB]==[1.000000]

&&

[SYSTEMS.ICE.ENG2IcePB]==[1.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=1,Engine anti ice on,0.000000,

execute=2,chklread,-1.000000,

execute=1,Left and right isolation valve?,0.000000,

logic:

calc=[0.000000]

out=LeftIsolValve,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.L_IsolValve]!=[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,l-isln,-1.000000,

execute=8,anim/59/button,0.000000,

execute=8,anim/59/button/anim,0.000000,

execute=8,jd/fo/_planshet,1.000000,

logic:

[SYSTEMS.AIR.L_IsolValve]==[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

logic:

calc=[0.000000]

out=RightIsolValve,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.R_IsolValve]!=[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,r-isln,-1.000000,

execute=8,anim/87/button,0.000000,

execute=1,Off,0.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklread,-1.000000,

execute=1,Recall?,0.000000,

logic:

[SYSTEMS.AIR.R_IsolValve]==[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Recall?,0.000000,

logic:

calc=[0.000000]

out=Recall,integer,,0.000000,,,,,,,,0,,

logic:

instring=checked

&&

[SYSTEMS.MCP.MasterCaution]==[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=1,Checked,0.000000,

execute=2,chklread,-1.000000,

execute=1,Autobrake?,0.000000,

logic:

instring=checked

&&

[SYSTEMS.MCP.MasterCaution]==[0.000000]

&&

[0.000000]==[1.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=1,Sir; recall button is not pressed!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Autobrake?,0.000000,

logic:

calc=[0.000000]

out=AutoBrake,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.BRAKES.AutoBrakeSW]!=[-1.000000]

calc=[0.000000]

execute=2,chklecam,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,abr-off,-1.000000,

execute=8,anim/rhotery/25/anim,-1.000000,

execute=2,abr-rto,0.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklecam,-1.000000,

execute=1,Rejected takeoff,0.000000,

execute=2,chklread,-1.000000,

execute=1,Ground equipment?,0.000000,

logic:

instring=any

&&

[SYSTEMS.BRAKES.AutoBrakeSW]==[-1.000000]

calc=[0.000000]

execute=2,chklecam,-1.000000,

execute=1,Rejected takeoff,0.000000,

execute=2,chklread,-1.000000,

execute=1,Ground equipment?,0.000000,

logic:

instring=rejected takeoff

&&

[0.000000]==[1.000000]

calc=[0.000000]

logic:

calc=[0.000000]

out=Ground equipment,integer,,0.000000,,,,,,,,0,,

logic:

instring=clear

&&

[SYSTEMS.GROUNDEQUIP.AllClear]==[0.000000]

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=2,chklwindow,-1.000000,

execute=1,Clear,0.000000,

logic:

instring=clear

&&

[SYSTEMS.GROUNDEQUIP.AllClear]>[0.000000]

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=2,chklwindow,-1.000000,

execute=1,Sir; not clear!,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Before taxi checklist is not completed!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Before taxi checklist completed,0.000000,

execute=2,rest01,-1.000000,

logic:

calc=[0.000000]



devstack=BeforeTakeoff

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=before takeoff checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,before takeoff checklist,-1.000000,

execute=1,Before takeoff checklist!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Briefing?,0.000000,

execute=2,chkl-mcp,-1.000000,

logic:

instring=before takeoff checklist

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed in flight!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Briefing,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=1,Packs?,0.000000,

logic:

instring=reviewed

&&

[0.000000]==[1.000000]

calc=[0.000000]

logic:

calc=[0.000000]

out=Packs,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Pack1]==[0.000000]

&&

[SYSTEMS.AIR.Pack2]==[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=1,Off!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Flaps?,0.000000,

logic:

[SYSTEMS.AIR.Pack1]==[1.000000]

&&

[SYSTEMS.AIR.Pack2]==[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=1,Auto!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Flaps?,0.000000,

logic:

[SYSTEMS.AIR.Pack1]>[0.000000]

&&

[SYSTEMS.AIR.Pack2]==[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=1,One pack on!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Flaps?,0.000000,

logic:

[SYSTEMS.AIR.Pack1]==[0.000000]

&&

[SYSTEMS.AIR.Pack2]>[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=1,One pack on!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Flaps?,0.000000,

logic:

calc=[0.000000]

out=Flaps,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FLAPS.FlapsFact]==[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-ped,-1.000000,

execute=1,Flaps is not set,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Before takeoff checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

[SYSTEMS.FLAPS.FlapCompCDU]!=[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-ped,-1.000000,

execute=1,Flaps is not set for takeoff position,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Before takeoff checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

[SYSTEMS.FLAPS.FlapCompCDU]==[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

logic:

[0.000000]==[1.000000]

calc=[0.000000]

logic:

[SYSTEMS.FLAPS.FlapsFact]>[20.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-ped,-1.000000,

execute=1,This position of the flaps is not used for takeoff,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Before takeoff checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=FlapsSet,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FLAPS.FlapsFact]==[1.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,One set; green light; detent,0.000000,

execute=2,chklread,-1.000000,

execute=1,Stabilizer trim?,0.000000,

logic:

[SYSTEMS.FLAPS.FlapsFact]==[5.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,Five set; green light; detent,0.000000,

execute=2,chklread,-1.000000,

execute=1,Stabilizer trim?,0.000000,

logic:

[SYSTEMS.FLAPS.FlapsFact]==[15.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,Fifteen set; green light; detent,0.000000,

execute=2,chklread,-1.000000,

execute=1,Stabilizer trim?,0.000000,

logic:

[SYSTEMS.FLAPS.FlapsFact]==[20.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,Twenty set; green light; detent!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Stabilizer trim?,0.000000,

logic:

calc=[0.000000]

out=StabTrim,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.THS.ThsError]<[0.250000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chklread,-1.000000,

execute=1,Speedbrake lever?,0.000000,

logic:

instring=any

&&

[SYSTEMS.THS.ThsError]>[0.250000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=1,Is not set for takeoff position,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Before takoff checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

instring=check and say trim position

&&

[0.000000]==[1.000000]

calc=[0.000000]

logic:

calc=[0.000000]

out=SpeedBrake,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.SPEEDBRAKE.SB_DrfSim]==[0.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chklread,-1.000000,

execute=1,Flight controls?,0.000000,

logic:

instring=any

&&

[SYSTEMS.SPEEDBRAKE.SB_DrfSim]>[0.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=1,Not down detent position. Before takeoff checklist is not completed,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=3,,0.000000,

logic:

instring=down detent

&&

[0.000000]==[1.000000]

calc=[0.000000]

logic:

calc=[0.000000]

out=FlightControls,integer,,0.000000,,,,,,,,0,,

logic:

instring=checked

&&

[SYSTEMS.FLGHTCONT.FlightContrChecked]==[1.000000]

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=1,Cabin?,0.000000,

logic:

instring=checked

&&

[SYSTEMS.FLGHTCONT.FlightContrChecked]==[0.000000]

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=1,Flight controls is not checked,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Before takeoff checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Cabin,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=2,chklovhdrt,-1.000000,

logic:

instring=secure

&&

[0.000000]==[1.000000]

calc=[0.000000]

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Before takeoff checklist completed,0.000000,

logic:

calc=[0.000000]



devstack=AfterTakeoff

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=after takeoff checklist

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,after takeoff checklist,-1.000000,

execute=1,After takeoff checklist!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Paks?,0.000000,

execute=2,chklovhdrt,-1.000000,

logic:

instring=after takeoff checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed on the ground!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Pack1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Pack1]!=[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,pck1-off,-1.000000,

execute=8,1-sim/cond/leftPackSelector,1.000000,

execute=8,1-sim/cond/leftPackSelector/anim,1.000000,

execute=2,pck1-auto,0.000000,

logic:

[SYSTEMS.AIR.Pack1]==[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

logic:

calc=[0.000000]

out=Pack2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Pack2]!=[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,pck2-off,-1.000000,

execute=8,1-sim/cond/rightPackSelector,1.000000,

execute=8,1-sim/cond/rightPackSelector/anim,1.000000,

execute=2,pck2-auto,0.000000,

logic:

[SYSTEMS.AIR.Pack2]==[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

logic:

calc=[0.000000]

out=Packs,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Pack1]==[1.000000]

&&

[SYSTEMS.AIR.Pack2]==[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Auto,0.000000,

execute=2,chklread,-1.000000,

execute=1,Landing gear?,0.000000,

logic:

calc=[0.000000]

out=LandingGear,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LG.LG_Lever]==[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,lg-up,-1.000000,

execute=8,1-sim/cockpit/switches/gear_handle,0.500000,

execute=8,1-sim/cockpit/switches/gear_handle/anim,0.500000,

execute=2,lg-off,0.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chkl-cdu,-1.000000,

execute=1,Up and Off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Flaps?,0.000000,

logic:

[SYSTEMS.LG.LG_Lever]==[0.500000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=1,Up and off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Flaps?,0.000000,

logic:

[SYSTEMS.LG.LG_Lever]==[1.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=1,Down; After takeoff checklist is not completed,0.000000,

execute=8,jd/fo/_planshet,0.000000,

logic:

calc=[0.000000]

out=Flaps,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FLAPS.FlapsFact]==[0.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,Up; no light; detent,0.000000,

logic:

[SYSTEMS.FLAPS.FlapsFact]>[0.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,Flaps extendet,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,After takeoff checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=ToTheLine,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MISC.TransAltDone]==[1.000000]

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=1,Altimeters?,0.000000,

logic:

[SYSTEMS.MISC.TransAltDone]==[0.000000]

calc=[2.000000]

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=0,Waiting transition altitude!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Altimeters,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

logic:

instring=say the baro set on the altimeter

&&

[1.000000]==[0.000000]

calc=[0.000000]

logic:

calc=[0.000000]

out=Altimeters1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MCP.BaroStdFo]==[0.000000]

&&

[SYSTEMS.MCP.BaroStdCap]==[1.000000]

&&

[SYSTEMS.MISC.AvioPanelChange]==[1.000000]

calc=[0.000000]

execute=2,look-frd,-1.000000,

execute=2,baro-std,-1.000000,

execute=8,jd/fo/needsetbaro,0.000000,

execute=8,jd/fo/needsetbaro1,0.000000,

execute=8,1-sim/ng/baro/std/R,1.000000,

execute=2,look-cap,-1.000000,

execute=2,answer01,-1.000000,

execute=1,Standard baro set cross checked,0.000000,

logic:

[SYSTEMS.MCP.BaroStdFo]==[1.000000]

&&

[SYSTEMS.MCP.BaroStdCap]==[1.000000]

&&

[SYSTEMS.MISC.AvioPanelChange]==[1.000000]

calc=[0.000000]

execute=2,look-frd,-1.000000,

execute=2,look-cap,-1.000000,

execute=1,Standard baro set cross checked,0.000000,

logic:

[SYSTEMS.MCP.BaroStdFo]==[0.000000]

&&

[SYSTEMS.MCP.BaroStdCap]==[0.000000]

&&

[SYSTEMS.MISC.AvioPanelChange]==[1.000000]

calc=[0.000000]

execute=2,look-frd,-1.000000,

execute=2,baro-std,-1.000000,

execute=8,jd/fo/needsetbaro,0.000000,

execute=8,jd/fo/needsetbaro1,0.000000,

execute=8,1-sim/ng/baro/std/R,1.000000,

execute=2,look-cap,-1.000000,

execute=1,Standard set; not cross checked,0.000000,

execute=2,look-cap,-1.000000,

execute=0,Please check baro on Your side!,0.000000,

execute=1,After takeoff checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

[SYSTEMS.MCP.BaroStdFo]==[1.000000]

&&

[SYSTEMS.MCP.BaroStdCap]==[0.000000]

&&

[SYSTEMS.MISC.AvioPanelChange]==[1.000000]

calc=[0.000000]

execute=2,look-frd,-1.000000,

execute=2,look-cap,-1.000000,

execute=1,Standard set; not cross checked,0.000000,

execute=2,look-cap,-1.000000,

execute=0,Please check baro on Your side!,0.000000,

execute=1,After takeoff checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Altimeters2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[0.000000]

&&

[SYSTEMS.MCP.BaroDiffSTDMod]<[0.010000]

calc=[0.000000]

execute=2,look-frd,-1.000000,

execute=2,baro-set,-1.000000,

execute=8,jd/fo/needsetbaro,0.000000,

execute=8,sim/cockpit2/gauges/actuators/barometer_setting_in_hg_copilot,29.920000,

execute=2,baro-set1,-1.000000,

execute=2,look-cap,-1.000000,

execute=2,answer01,-1.000000,

execute=1,Standard baro set cross checked,0.000000,

execute=2,look-front,-1.000000,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[0.000000]

&&

[SYSTEMS.MCP.BaroDiffSTDMod]>[0.010000]

calc=[0.000000]

execute=2,look-frd,-1.000000,

execute=2,baro-set,-1.000000,

execute=8,jd/fo/needsetbaro,0.000000,

execute=8,sim/cockpit2/gauges/actuators/barometer_setting_in_hg_copilot,29.920000,

execute=2,baro-set1,-1.000000,

execute=2,look-cap,-1.000000,

execute=1,Standard set; not cross checked,0.000000,

execute=2,look-cap,-1.000000,

execute=1,Please check baro on Your side!,0.000000,

execute=1,After takeoff checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[1.000000]

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,After takeoff checklist completed,0.000000,

logic:

calc=[0.000000]



devstack=Descent

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=descent checklist

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,descent checklist,-1.000000,

execute=1,Descent checklist!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklovhdrt,-1.000000,

execute=1,Pressurization?,0.000000,

logic:

instring=descent checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed on the ground!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Press,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.CABPRESS.LandAltNeed]!=[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=1,Landing altitude not set for landing,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Descent checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

[SYSTEMS.CABPRESS.LandAltNeed]==[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=1,Landing altitude <SYSTEMS.CABPRESS.LandAltSet> set!,0.000000,

execute=7,,1.000000,

execute=2,chklread,-1.000000,

execute=1,Seat belt sign?,0.000000,

logic:

calc=[0.000000]

out=SeatBelt,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_SeatBeltsSW]==[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=2,belt-off,-1.000000,

execute=8,sim/cockpit/switches/fasten_seat_belts/anim,2.000000,

execute=2,belt-on,0.000000,

execute=0,Seat Belts is on!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Recall?,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_SeatBeltsSW]==[2.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=0,Is on!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Recall?,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_SeatBeltsSW]==[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=2,belt-off,-1.000000,

execute=8,sim/cockpit/switches/fasten_seat_belts/anim,2.000000,

execute=2,belt-on,0.000000,

execute=0,Seat Belts is on!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Recall?,0.000000,

logic:

calc=[0.000000]

out=Recall,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,recall,-1.000000,

execute=8,1-sim/gauges/caution_recall,1.000000,

execute=2,chklread,-1.000000,

execute=1,Autobrake?,0.000000,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[1.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,recall-1,-1.000000,

execute=8,1-sim/gauges/caution_recall,1.000000,

execute=2,chklread,-1.000000,

execute=1,Autobrake?,0.000000,

logic:

calc=[0.000000]

out=Autobrake,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.BRAKES.AutoBrakeSW]<[2.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=1,Sir; autobrake is not set,0.000000,

execute=2,chklread,-1.000000,

execute=1,Landing data?,0.000000,

logic:

instring=any

&&

[SYSTEMS.BRAKES.AutoBrakeSW]>[1.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=7,,1.000000,

execute=2,chklread,-1.000000,

execute=1,Landing data?,0.000000,

logic:

instring=say autobrake position

&&

[1.000000]==[0.000000]

calc=[0.000000]

logic:

calc=[0.000000]

out=LandingData,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.FMS.Vref]<[110.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

execute=2,chcduinit,-1.000000,

execute=8,757Avionics/CDU2/init_ref,1.000000,

execute=2,chcdul6,-1.000000,

execute=8,757Avionics/CDU2/LLSK6,1.000000,

execute=2,chcdul5,-1.000000,

execute=8,757Avionics/CDU2/LLSK5,1.000000,

execute=1,V reference is not set,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Descent checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

instring=say v reference speed and minimums

&&

[1.000000]==[0.000000]

calc=[0.000000]

logic:

instring=any

calc=[0.000000]

execute=2,chklread,-1.000000,

logic:

calc=[0.000000]

out=LandingData1,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

execute=2,chcduinit,-1.000000,

execute=8,757Avionics/CDU2/init_ref,1.000000,

execute=2,chcdul6,-1.000000,

execute=8,757Avionics/CDU2/LLSK6,1.000000,

execute=2,chcdul5,-1.000000,

execute=8,757Avionics/CDU2/LLSK5,1.000000,

execute=1,V reference <SYSTEMS.FMS.Vref>,0.000000,

logic:

calc=[0.000000]

out=LandingData2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[0.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chklminsdn,-1.000000,

execute=1,Minimums <SYSTEMS.MCP.DH> set!,0.000000,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[1.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chklanswer,-1.000000,

execute=1,Sorry; but I can't see what you've set yet!,0.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[1.000000]

execute=2,chklread,-1.000000,

execute=8,jd/fo/needsetdh,0.000000,

execute=8,jd/fo/needsetdh,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Descent checklist completed,0.000000,

logic:

calc=[0.000000]



devstack=Approach

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=approach checklist

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,approach checklist,-1.000000,

execute=1,Approach checklist!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Altimeters?,0.000000,

logic:

instring=approach checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed on the ground!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Altim,integer,,0.000000,,,,,,,,0,,

logic:

instring=say baro pressure on the pfd

&&

[1.000000]==[0.000000]

calc=[0.000000]

logic:

instring=any

&&

[SYSTEMS.MCP.BaroStdCap]==[1.000000]

&&

[SYSTEMS.MISC.AvioPanelChange]==[1.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,Sir; you have a standard baro set,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Approach checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

instring=any

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

logic:

calc=[0.000000]

out=Altim1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[0.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chbarodn,-1.000000,

execute=8,jd/fo/needsetbaro2,1.000000,

execute=8,jd/fo/needsetbaro2,0.000000,

execute=2,chbaroup,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Altimeter <&SYSTEMS.MCP.BaroSetHpaFO> set!!,0.000000,

execute=2,chkl-mcp,-1.000000,

execute=0,Cross checked; passing altitude <SYSTEMS.POSITION.ALT> now!,0.000000,

execute=2,chklread,-1.000000,

execute=1,NAV Aids?,0.000000,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[1.000000]

calc=[0.000000]

execute=2,chklread,-1.000000,

logic:

calc=[0.000000]

out=Altim2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[1.000000]

&&

[SYSTEMS.MCP.ChangeHPA_Cap]==[0.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chklbarodn,-1.000000,

execute=8,1-sim/ng/baro/std/R,0.000000,

execute=8,1-sim/ng/baroLargeR/anim,0.000000,

execute=8,1-sim/ng/baroLargeR/anim/anim,0.000000,

execute=8,jd/fo/needsetbaro3,0.000000,

execute=8,jd/fo/needsetbaro3,1.000000,

execute=8,jd/fo/needsetbaro3,0.000000,

execute=2,chklbaroup,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Altimeter <&SYSTEMS.MCP.BaroSetInHgFo100> set!,0.000000,

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=0,Cross checked; passing altitude <SYSTEMS.POSITION.ALT> now!,0.000000,

execute=2,chklread,-1.000000,

execute=1,NAV Aids?,0.000000,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[1.000000]

&&

[SYSTEMS.MCP.ChangeHPA_Cap]==[-1.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chklbarodn,-1.000000,

execute=8,1-sim/ng/baro/std/R,0.000000,

execute=8,1-sim/ng/baroLargeR/anim,-1.000000,

execute=8,1-sim/ng/baroLargeR/anim/anim,-1.000000,

execute=8,jd/fo/needsetbaro3,0.000000,

execute=8,jd/fo/needsetbaro3,1.000000,

execute=8,jd/fo/needsetbaro3,0.000000,

execute=2,chklbaroup,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Altimeter <&SYSTEMS.MCP.BaroSetHpaFO> set!!,0.000000,

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=0,Cross checked; passing altitude <SYSTEMS.POSITION.ALT> now!,0.000000,

execute=2,chklread,-1.000000,

execute=1,NAV Aids?,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=NavAids,integer,,0.000000,,,,,,,,0,,

logic:

instring=set

calc=[0.000000]

execute=2,chklread,-1.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[1.000000]

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Approach checklist completed,0.000000,

logic:

calc=[0.000000]



devstack=Landing

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=landing checklist

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,landing checklist,5.000000,

execute=1,Landing checklist!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklovhddn,-1.000000,

execute=1,Cabin?,0.000000,

logic:

instring=landing checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed on the ground!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Cabin,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=1,Secure!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Speed brake?,0.000000,

logic:

calc=[0.000000]

out=SpeedBrake,integer,,0.000000,,,,,,,,0,,

logic:

instring=arm

&&

[SYSTEMS.SPEEDBRAKE.SB_DrfSim]<=[-0.450000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=7,,1.000000,

execute=2,chklread,-1.000000,

execute=1,Landing gear?,0.000000,

logic:

instring=arm

&&

[SYSTEMS.SPEEDBRAKE.SB_DrfSim]!=[-0.500000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=1,Speed brake is not arm,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Landing checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=LandingGear,integer,,0.000000,,,,,,,,0,,

logic:

instring=down

&&

[SYSTEMS.LG.LG_Lever]!=[1.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

execute=1,Sir; is not down position,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Landing checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

instring=down

&&

[SYSTEMS.LG.LG_Lever]==[1.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

execute=7,,1.000000,

execute=2,chklread,-1.000000,

execute=1,Flaps?,0.000000,

logic:

calc=[0.000000]

out=Flaps,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.FLAPS.FlapsFact]==[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-ped,-1.000000,

execute=1,Flaps is not set,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Landing checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

instring=any

&&

[SYSTEMS.FLAPS.FlapCompApp]!=[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-ped,-1.000000,

execute=1,Flaps is not set for landing position,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Landing checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

instring=any

&&

[SYSTEMS.FLAPS.FlapCompApp]==[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-ped,-1.000000,

execute=0,Flaps <SYSTEMS.FLAPS.FlapsFact> set!,0.000000,

execute=2,chklread,-1.000000,

logic:

instring=say flap position

&&

[0.000000]==[1.000000]

calc=[0.000000]

logic:

instring=any

&&

[SYSTEMS.FMS.FlapsAppr]<[25.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-ped,-1.000000,

execute=1,This position of the flaps is not used for landing,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Landing checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[1.000000]

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Landing checklist completed,0.000000,

logic:

calc=[0.000000]



devstack=Shutdown

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=shutdown checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,shutdown checklist,-1.000000,

execute=1,Shutdown checklist!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklovhddn,-1.000000,

execute=1,Hydraulic panel?,0.000000,

logic:

instring=shutdown checklist

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed in flight!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=HydEng1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.Eng1PumpSW]!=[1.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,hyd-l-eng,-1.000000,

execute=8,anim/8/button,1.000000,

execute=8,anim/8/button/anim,1.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=HydEng2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.Eng2PumpSW]!=[1.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,hyd-r-eng,-1.000000,

execute=8,anim/11/button,1.000000,

execute=8,anim/11/button/anim,1.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=HydElec1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.ElecPump1]!=[0.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,elec-1-hyd,-1.000000,

execute=8,anim/9/button,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=HydElec2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.ElecPump2]!=[0.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,elec-2-hyd,-1.000000,

execute=8,anim/10/button,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=HydDemL,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.PumpDemandL]!=[0.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,dem-l-auto,-1.000000,

execute=8,1-sim/hyd/elecSwitchLeft,0.000000,

execute=8,1-sim/hyd/elecSwitchLeft/anim,0.000000,

execute=2,dem-l-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=HydDemC,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.PumpDemandC]!=[0.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,dem-c-auto,-1.000000,

execute=8,1-sim/hyd/airSwitch,0.000000,

execute=8,1-sim/hyd/airSwitch/anim,0.000000,

execute=2,dem-c-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=HydDemR,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.PumpDemandR]!=[0.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,dem-r-auto,-1.000000,

execute=8,1-sim/hyd/elecSwitchRight,0.000000,

execute=8,1-sim/hyd/elecSwitchRight/anim,0.000000,

execute=2,dem-r-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=HydSet,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Set,0.000000,

execute=2,chklread,-1.000000,

execute=1,Fuel pumps?,0.000000,

logic:

calc=[0.000000]

out=Pump1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LAftPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,fp-l-aft,-1.000000,

execute=8,anim/32/button,0.000000,

execute=8,anim/32/button/anim,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pump2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,fp-l-fwd,-1.000000,

execute=8,anim/35/button,0.000000,

execute=8,anim/35/button/anim,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pump3,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LCtrPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,fp-c-l,-1.000000,

execute=8,anim/38/button,0.000000,

execute=8,anim/38/button/anim,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pump4,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RCtrPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,fp-c-r,-1.000000,

execute=8,anim/39/button,0.000000,

execute=8,anim/39/button/anim,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pump5,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RFwdPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,fp-r-fwd,-1.000000,

execute=8,anim/37/button,0.000000,

execute=8,anim/37/button/anim,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pump6,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RAftPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,fp-r-aft,-1.000000,

execute=8,anim/34/button,0.000000,

execute=8,anim/34/button/anim,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Cross,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.CrossFeed2SW]!=[0.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,fp-xfeed2,-1.000000,

execute=8,anim/36/button,0.000000,

execute=8,anim/36/button/anim,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Xfeed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.CrossFeed1SW]!=[0.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,fp-xfeed1,-1.000000,

execute=8,anim/33/button,0.000000,

execute=8,anim/33/button/anim,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=FuelPumpsOff,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Speedbrake lever?,0.000000,

logic:

calc=[0.000000]

out=SpeedBrake,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.SPEEDBRAKE.SB_DrfSim]==[0.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chklread,-1.000000,

execute=1,Flaps?,0.000000,

logic:

instring=any

&&

[SYSTEMS.SPEEDBRAKE.SB_DrfSim]!=[0.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=1,Not down detent!,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Shutdown checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

instring=down detent

&&

[0.000000]==[1.000000]

calc=[0.000000]

logic:

calc=[0.000000]

out=Flaps,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FLAPS.FlapsFact]>[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-ped,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,flaps,-1.000000,

execute=8,sim/cockpit2/controls/flap_ratio,0.000000,

execute=2,flaps0,0.000000,

execute=1,Up,0.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklread,-1.000000,

execute=1,Parking brake?,0.000000,

logic:

[SYSTEMS.FLAPS.FlapsFact]==[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-ped,-1.000000,

execute=1,Up,0.000000,

execute=2,chklread,-1.000000,

execute=1,Parking brake?,0.000000,

logic:

calc=[0.000000]

out=ParkingBrake,integer,,0.000000,,,,,,,,0,,

logic:

instring=set

&&

[SYSTEMS.BRAKES.ParkBrakeHandlePos]==[1.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=7,,0.300000,

execute=2,chklread,-1.000000,

execute=1,Fuel control switches?,0.000000,

logic:

instring=set

&&

[SYSTEMS.BRAKES.ParkBrakeHandlePos]==[0.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=7,,0.300000,

execute=1,Parking brake is not set,0.000000,

execute=2,chklread,-1.000000,

execute=1,Fuel control switches?,0.000000,

logic:

calc=[0.000000]

out=EngStartLever,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.ENGINE.EngMastSumm]==[0.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=7,,0.300000,

execute=2,chklread,-1.000000,

execute=1,Weather radar?,0.000000,

logic:

instring=any

&&

[SYSTEMS.ENGINE.EngMastSumm]>[0.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=1,Engine start levers is not cutoff,0.000000,

execute=1,Shutdown checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

instring=cutoff

&&

[0.000000]==[1.000000]

calc=[0.000000]

logic:

calc=[0.000000]

out=WeatherRadar,integer,,0.000000,,,,,,,,0,,

logic:

instring=off

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

logic:

calc=[0.000000]

out=WeatherRadar1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[0.000000]

&&

[SYSTEMS.PEDESTAL.WxrFoOn]==[0.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[0.000000]

&&

[SYSTEMS.PEDESTAL.WxrFoOn]==[1.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

execute=7,,1.000000,

execute=2,chklwxr,-1.000000,

execute=8,1-sim/ndpanel/2/hsiWxr,0.000000,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[1.000000]

&&

[SYSTEMS.PEDESTAL.RadarSWFo]==[0.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[1.000000]

&&

[SYSTEMS.PEDESTAL.RadarSWFo]==[1.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

execute=7,,1.000000,

execute=2,chklwxr,-1.000000,

execute=8,efis/fpds/2/wxrTerrOnDisplay,0.000000,

logic:

calc=[0.000000]

out=WeatherRadar2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[0.000000]

&&

[SYSTEMS.PEDESTAL.WxrCapOn]==[0.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

execute=1,Off!,0.000000,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[0.000000]

&&

[SYSTEMS.PEDESTAL.WxrCapOn]==[1.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

execute=1,Your radar is not off!,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Shutdown checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[1.000000]

&&

[SYSTEMS.PEDESTAL.RadarSWCap]==[0.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

execute=1,Off!,0.000000,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[1.000000]

&&

[SYSTEMS.PEDESTAL.RadarSWCap]==[1.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

execute=1,Your radar is not off!,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Shutdown checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[1.000000]

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Shutdown checklist completed,0.000000,

logic:

calc=[0.000000]



devstack=Secure

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=secure checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,secure checklist,5.000000,

execute=1,Secure checklist!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklovhdup,-1.000000,

execute=1,IRS Selectors?,0.000000,

logic:

instring=secure checklist

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed in flight!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Irs1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDUP.IRS_L]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,irs1-nav,-1.000000,

execute=8,anim/rhotery/3/anim,0.000000,

execute=8,1-sim/irs/1/modeSel,0.000000,

execute=2,irs1-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Irs2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDUP.IRS_C]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,irs2-nav,-1.000000,

execute=8,anim/rhotery/4/anim,0.000000,

execute=8,1-sim/irs/2/modeSel,0.000000,

execute=2,irs2-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Irs3,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDUP.IRS_R]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,irs3-nav,-1.000000,

execute=8,anim/rhotery/5/anim,0.000000,

execute=8,1-sim/irs/3/modeSel,0.000000,

execute=2,irs3-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=IrsOff,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=1,Off!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Emergency exit lights?,0.000000,

logic:

calc=[0.000000]

out=EmerExit,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.EmerExitSW]!=[1.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,emer-off,-1.000000,

execute=8,1-sim/emer/lightsCover,1.000000,

execute=8,1-sim/emer/lightsCover/anim,1.000000,

execute=1,Off,0.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklread,-1.000000,

execute=1,Window heat?,0.000000,

logic:

[SYSTEMS.LIGHTS.EmerExitSW]==[1.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Window heat?,0.000000,

logic:

calc=[0.000000]

out=WindowHeat1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDER.WindHeatLside]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,side-l,-1.000000,

execute=8,anim/47/button,0.000000,

execute=8,anim/47/button/anim,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=WindowHeat2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDER.WindHeatLfwd]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,fwd-l,-1.000000,

execute=8,anim/48/button,0.000000,

execute=8,anim/48/button/anim,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=WindowHeat3,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDER.WindHeatRfwd]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,fwd-r,-1.000000,

execute=8,anim/49/button,0.000000,

execute=8,anim/49/button/anim,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=WindowHeat4,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDER.WindHeatRside]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,side-r,-1.000000,

execute=8,anim/50/button,0.000000,

execute=8,anim/50/button/anim,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=WindowHeat,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Packs?,0.000000,

logic:

calc=[0.000000]

out=Pack1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Pack1]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,pck1-auto,-1.000000,

execute=8,1-sim/cond/leftPackSelector,0.000000,

execute=8,1-sim/cond/leftPackSelector/anim,0.000000,

execute=2,pck1-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pack2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Pack2]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,pck2-auto,-1.000000,

execute=8,1-sim/cond/rightPackSelector,0.000000,

execute=8,1-sim/cond/rightPackSelector/anim,0.000000,

execute=2,pck2-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Packs,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Ground power?,0.000000,

logic:

calc=[0.000000]

out=ExtPower,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.ExtPwrSW]==[1.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,ext-pwr,-1.000000,

execute=8,anim/16/button,0.000000,

execute=8,anim/16/button/anim,0.000000,

execute=1,Off,0.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklread,-1.000000,

execute=1,A P U?,0.000000,

logic:

[SYSTEMS.ELEC.ExtPwrSW]==[0.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

execute=1,A P U?,0.000000,

logic:

calc=[0.000000]

out=APU,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.APU.StartSW]>[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,apu-on,-1.000000,

execute=8,1-sim/engine/APUStartSelector,0.000000,

execute=8,1-sim/engine/APUStartSelector/anim,0.000000,

execute=2,apu-off,0.000000,

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Standby power selector?,0.000000,

logic:

[SYSTEMS.APU.StartSW]==[0.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Standby power selector?,0.000000,

logic:

calc=[0.000000]

out=StbyPower,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.StandbyPowerPB]>[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,stby-auto,-1.000000,

execute=8,1-sim/engine/APUStartSelector,0.000000,

execute=8,1-sim/engine/APUStartSelector/anim,0.000000,

execute=2,stby-off,0.000000,

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Battery switch?,0.000000,

logic:

[SYSTEMS.ELEC.StandbyPowerPB]==[0.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Battery switch?,0.000000,

logic:

calc=[0.000000]

out=Battery,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.BatterySW]!=[0.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,battery,-1.000000,

execute=8,1-sim/electrical/batteryCover,1.000000,

execute=8,1-sim/electrical/batteryCover/anim,1.000000,

execute=8,anim/14/button,0.000000,

execute=8,anim/14/button/anim,0.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

logic:

[SYSTEMS.ELEC.BatterySW]==[0.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[1.000000]

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Secure checklist completed,0.000000,

logic:

calc=[0.000000]



devstack=Before de icing

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=before de icing checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=1,Before de icing checklist!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,A P U?,0.000000,

execute=2,chklovhddn,-1.000000,

logic:

instring=before de icing checklist

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed in flight!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Apu,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.APU.APUAvail]==[0.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=0,Is off,0.000000,

execute=2,chklread,-1.000000,

execute=0,Flaps?,0.000000,

execute=2,chkl-ped,-1.000000,

logic:

[SYSTEMS.APU.APUAvail]==[1.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=0,Is on,0.000000,

execute=2,chklread,-1.000000,

execute=0,Flaps?,0.000000,

execute=2,chkl-ped,-1.000000,

logic:

calc=[0.000000]

out=Flaps,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FLAPS.FlapsFact]!=[0.000000]

&&

[SYSTEMS.FLAPS.Ok0]==[1.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,flaps,-1.000000,

execute=8,sim/flightmodel/controls/flaprqst,0.000000,

execute=2,flaps0,0.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=0,Retracted,0.000000,

execute=2,chklread,-1.000000,

execute=1,Thrust levers?,0.000000,

execute=2,chkl-ped,-1.000000,

execute=2,chklanswer,-1.000000,

logic:

[SYSTEMS.FLAPS.FlapsFact]==[0.000000]

&&

[SYSTEMS.FLAPS.Ok0]==[1.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=0,Checked; Up set,0.000000,

execute=2,chklread,-1.000000,

execute=1,Thrust levers?,0.000000,

execute=2,chkl-ped,-1.000000,

logic:

calc=[0.000000]

out=ThrusLever,integer,,0.000000,,,,,,,,0,,

logic:

instring=idle

&&

[SYSTEMS.ENGINE.Eng1Lever]<[0.050000]

&&

[SYSTEMS.ENGINE.Eng2Lever]<[0.050000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chklread,-1.000000,

execute=1,Stabilised trim?,0.000000,

execute=2,chkl-ped,-1.000000,

logic:

instring=idle

&&

[SYSTEMS.ENGINE.Eng1Lever]>[0.050000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=0,Sir; is not idle position,0.000000,

execute=2,chklanswer,-1.000000,

execute=0,Before de icing checklist is not completed,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=3,,0.000000,

logic:

instring=idle

&&

[SYSTEMS.ENGINE.Eng2Lever]>[0.050000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=0,Sir; is not idle position,0.000000,

execute=2,chklanswer,-1.000000,

execute=0,Before de icing checklist is not completed,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Trim,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.THS.ThsError]<[0.200000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chklread,-1.000000,

execute=1,Engine bleed air switches?,0.000000,

execute=2,chklovhdrt,-1.000000,

logic:

instring=any

&&

[SYSTEMS.THS.ThsError]>[0.200000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=1,Is not set for takeoff position,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=0,Before de icing checklist is not completed,0.000000,

execute=3,,0.000000,

logic:

[0.000000]==[1.000000]

&&

instring=check and set trim for takeoff position

calc=[0.000000]

logic:

calc=[0.000000]

out=Eng1Bleed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Eng1BleedSW]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,bleed-l,-1.000000,

execute=8,anim/60/button,0.000000,

execute=8,anim/60/button/anim,0.000000,

execute=8,anim/60/button/anim,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Eng2Bleed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Eng2BleedSW]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,bleed-r,-1.000000,

execute=8,anim/62/button,0.000000,

execute=8,anim/62/button/anim,0.000000,

execute=8,anim/62/button/anim,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=EngineBleed,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Is off,0.000000,

execute=2,chklread,-1.000000,

execute=1,A P U bleed air switch?,0.000000,

logic:

calc=[0.000000]

out=APUBleed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.APUBleedSW]==[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,bleed-apu,-1.000000,

execute=8,anim/61/button,0.000000,

execute=8,anim/61/button/anim,0.000000,

execute=8,anim/61/button/anim,0.000000,

execute=1,Is off,0.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklread,-1.000000,

logic:

[SYSTEMS.AIR.APUBleedSW]==[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=1,Is off,0.000000,

execute=2,chklread,-1.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Before de icing checklist completed,0.000000,

logic:

calc=[0.000000]



devstack=After de icing

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=after de icing checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=1,After de icing checklist!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Chrono?,0.000000,

execute=2,chkl-frd,-1.000000,

logic:

instring=after de icing checklist

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed in flight!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Chrono,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,chrono,-1.000000,

execute=8,1-sim/gauges/clockChronoKnob_right,1.000000,

execute=0,Wait one minute,0.000000,

execute=2,look-frd,-1.000000,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,chrono1,-1.000000,

execute=8,1-sim/gauges/clockChronoKnob_right,1.000000,

execute=0,Wait one minute,0.000000,

execute=2,look-frd,-1.000000,

logic:

calc=[0.000000]

out=Chrono1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[0.000000]

&&

[SYSTEMS.TIME.Timer1min]==[1.000000]

calc=[0.000000]

execute=2,chrono,-1.000000,

execute=8,1-sim/gauges/clockChronoKnob_right,1.000000,

execute=7,,0.300000,

execute=8,1-sim/gauges/clockChronoKnob_right,1.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,A P U Bleed?,0.000000,

execute=2,chklovhdrt,-1.000000,

logic:

[SYSTEMS.MISC.AvioPanelChange]==[1.000000]

&&

[SYSTEMS.TIME.Timer1min]==[1.000000]

calc=[0.000000]

execute=2,chrono1,-1.000000,

execute=8,1-sim/gauges/clockChronoKnob_right,1.000000,

execute=7,,0.300000,

execute=8,1-sim/gauges/clockChronoKnob_right,1.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,A P U Bleed?,0.000000,

execute=2,chklovhdrt,-1.000000,

logic:

calc=[0.000000]

out=APUBleed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.APU.APUAvail]==[1.000000]

&&

[SYSTEMS.AIR.APUBleedSW]==[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=0,Is on,0.000000,

execute=2,chklread,-1.000000,

execute=1,Engine bleed air switches?,0.000000,

execute=2,chklovhdrt,-1.000000,

logic:

[SYSTEMS.APU.APUAvail]==[1.000000]

&&

[SYSTEMS.AIR.APUBleedSW]==[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,bleed-apu,-1.000000,

execute=8,anim/61/button,1.000000,

execute=8,anim/61/button/anim,1.000000,

execute=8,anim/61/button/anim,1.000000,

execute=0,Is on,0.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklread,-1.000000,

execute=1,Engine bleed air switches?,0.000000,

execute=2,chklovhdrt,-1.000000,

logic:

[SYSTEMS.APU.APUAvail]==[0.000000]

&&

[SYSTEMS.AIR.APUBleedSW]==[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,bleed-apu,-1.000000,

execute=8,anim/61/button,0.000000,

execute=8,anim/61/button/anim,0.000000,

execute=8,anim/61/button/anim,0.000000,

execute=0,Is off,0.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklread,-1.000000,

execute=1,Engine bleed air switches?,0.000000,

execute=2,chklovhdrt,-1.000000,

logic:

[SYSTEMS.APU.APUAvail]==[0.000000]

&&

[SYSTEMS.AIR.APUBleedSW]==[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=0,Is off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Engine bleed air switches?,0.000000,

execute=2,chklovhdrt,-1.000000,

logic:

calc=[0.000000]

out=Eng1Bleed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Eng1BleedSW]!=[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,bleed-l,-1.000000,

execute=8,anim/60/button,1.000000,

execute=8,anim/60/button/anim,1.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Eng2Bleed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Eng2BleedSW]!=[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,bleed-r,-1.000000,

execute=8,anim/62/button,1.000000,

execute=8,anim/62/button/anim,1.000000,

execute=8,anim/62/button/anim,1.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=EngineBleed,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Is on,0.000000,

execute=2,chklread,-1.000000,

logic:

calc=[0.000000]

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,After de icing checklist completed,0.000000,

logic:

calc=[0.000000]

