sys=SYSTEMS



dev=MISC

out=LookFoDeg,double,,0.000000,,,jd/fo/delta_hdg2fo,exist,,,,0,,

out=LookChecklist,integer,,0.000000,,,jd/fo/_planshet,exist,,,,0,,

out=Glass,integer,,0.000000,,,jd/fo/_glass,exist,,,,0,,

out=BaroDone,integer,,0.000000,,,,,,,,0,,

logic:

[CHECKLIST.AfterTakeoffDL.ToTheLine]==[2.000000]

calc=[1.000000]

logic:

[SYSTEMS.POSITION.onGround]==[1.000000]

calc=[0.000000]

logic:

calc=[SYSTEMS.MISC.BaroDone]

out=LightLevel,integer,,0.000000,,,sim/graphics/animation/draw_light_level,exist,,,,0,,

out=DeckDoor,double,,0.000000,,,laminar/B738/door/flt_dk_door_ratio,exist,,,,0,,

out=DoorLFwd,double,,0.000000,,,737u/doors/L1,exist,,,,0,,

out=DoorRFwd,double,,0.000000,,,737u/doors/R1,exist,,,,0,,

out=DoorLAft,double,,0.000000,,,737u/doors/L2,exist,,,,0,,

out=DoorRAft,double,,0.000000,,,737u/doors/R2,exist,,,,0,,

out=CargoFwd,double,,0.000000,,,737u/doors/Fwd_Cargo,exist,,,,0,,

out=CargoAft,double,,0.000000,,,737u/doors/aft_Cargo,exist,,,,0,,

out=DoorEmer1,double,,0.000000,,,737u/doors/emerg1,exist,,,,0,,

out=DoorEmer2,double,,0.000000,,,737u/doors/emerg2,exist,,,,0,,

out=DoorEmer3,double,,0.000000,,,737u/doors/emerg3,exist,,,,0,,

out=DoorEmer4,double,,0.000000,,,737u/doors/emerg4,exist,,,,0,,

out=DoorsClosed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MISC.DoorLFwd]==[0.000000]

&&

[SYSTEMS.MISC.DoorRFwd]==[0.000000]

&&

[SYSTEMS.MISC.DoorRFwd]==[0.000000]

&&

[SYSTEMS.MISC.DoorRAft]==[0.000000]

&&

[SYSTEMS.MISC.CargoFwd]==[0.000000]

&&

[SYSTEMS.MISC.CargoAft]==[0.000000]

&&

[SYSTEMS.MISC.DoorEmer1]==[0.000000]

&&

[SYSTEMS.MISC.DoorEmer2]==[0.000000]

&&

[SYSTEMS.MISC.DoorEmer3]==[0.000000]

&&

[SYSTEMS.MISC.DoorEmer4]==[0.000000]

calc=[1.000000]

logic:

calc=[0.000000]

out=TotalFuel,integer,,0.000000,,,sim/flightmodel/weight/m_fuel_total,exist,,,,0,,

out=AltComp,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.MCP.ALT]-[SYSTEMS.POSITION.ALT]

out=AltCompMod,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MISC.AltComp]<[0.000000]

calc=[SYSTEMS.MISC.AltComp]*[-1.000000]

logic:

calc=[SYSTEMS.MISC.AltComp]

out=CG_THS,double,,0.000000,,,laminar/B738/tab/cg_pos,exist,,,,0,,

out=TrimPos,double,,0.000000,,,laminar/B738/flt_ctrls/trim_wheel,exist,,,,0,,

out=DeIcing,integer,,0.000000,,,laminar/B738/de_ice_truck/hide,exist,,,,0,,

out=PowerPlus4Min,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.ACBusAvail]==[2.000000]

&&

[SYSTEMS.MISC.PowerPlus4Min]<[8600.000000]

calc=[SYSTEMS.MISC.PowerPlus4Min]+[1.000000]

logic:

[SYSTEMS.MISC.PowerPlus4Min]>=[8600.000000]

||

[SYSTEMS.ELEC.ACBusAvail]!=[2.000000]

calc=[0.000000]

logic:

calc=[SYSTEMS.MISC.PowerPlus4Min]

out=StartEngRunning,integer,,0.000000,,,sim/operation/prefs/startup_running,exist,,,,0,,

out=ModelAircraft,integer,,0.000000,,,jd/cpl/lu_mode,exist,,,,0,,



dev=COPILOT

out=isAnnounceNeed,integer,,0.000000,,,jd/copilot/comments,new,,,,1,,

out=doPM_JobOnly,integer,PM&PF;PM,0.000000,,,jd/copilot/realmode,new,,,,1,,



dev=EVENTCONTROL

out=EventCounter,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.EVENTCONTROL.EventCounter]>[17.000000]

calc=[1.000000]

logic:

calc=[SYSTEMS.EVENTCONTROL.EventCounter]+[1.000000]

out=TimerCounter,integer,,5.000000,,,,,,,,0,,

logic:

[SYSTEMS.EVENTCONTROL.TimerCounter]>[19.000000]

calc=[5.000000]

logic:

calc=[SYSTEMS.EVENTCONTROL.TimerCounter]+[1.000000]

out=Timer,double,,10000.000000,0.000000,,,,,,,0,,

logic:

[SYSTEMS.POSITION.RA]>[5.000000]

&&

[SYSTEMS.EVENTCONTROL.Timer]==[10000.000000]

calc=[SYSTEMS.EVENTCONTROL.TimerCounter]*[60.000000]

logic:

[SYSTEMS.EVENTCONTROL.Timer]>[0.000000]

&&

[SYSTEMS.EVENTCONTROL.Timer]!=[10000.000000]

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[SYSTEMS.EVENTCONTROL.Timer]-[SYSTEMS.TIME.FRP]

logic:

[SYSTEMS.EVENTCONTROL.EventRun]!=[-1.000000]

calc=[SYSTEMS.EVENTCONTROL.TimerCounter]*[60.000000]

logic:

calc=[SYSTEMS.EVENTCONTROL.Timer]

out=EventRun,integer,,-1.000000,,,,,,,,0,,

logic:

[SYSTEMS.EVENTCONTROL.Timer]==[0.000000]

calc=[SYSTEMS.EVENTCONTROL.EventCounter]

logic:

calc=[-1.000000]



dev=ACP

out=Com1On,integer,,0.000000,,,laminar/B738/comm/fo_audio_sel_com1,exist,,,,0,,

out=Com1Vol,double,,0.000000,,,laminar/B738/comm/fo_audio_vol_com1,exist,,,,0,,

out=Com2On,integer,,0.000000,,,laminar/B738/comm/fo_audio_sel_com2,exist,,,,0,,

out=Com2Vol,integer,,0.000000,,,laminar/B738/comm/fo_audio_vol_com2,exist,,,,0,,

out=Nav1,integer,,0.000000,,,sim/cockpit/radios/nav1_freq_hz,exist,,,,0,,

out=Nav2,integer,,0.000000,,,sim/cockpit/radios/nav2_freq_hz,exist,,,,0,,



dev=TIME

out=TFT,double,sec,0.000000,,,sim/time/total_flight_time_sec,exist,,,,0,,

out=FrameRate,integer,frame/sec,0.000000,,,,,,,,0,,

logic:

calc=[1.000000]/[SYSTEMS.TIME.FRP]

out=FRP,double,sec,60.000000,,,sim/operation/misc/frame_rate_period,exist,,,,0,,

logic:

calc=[SYSTEMS.TIME.TFT]-[SYSTEMS.TIME.TFT_Old]

out=TFT_Old,double,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.TIME.TFT]

out=Night_Day,integer,,0.000000,,,sim/graphics/animation/draw_light_level,exist,,,,0,,

out=ClockSW,integer,,0.000000,,,laminar/B738/clock/fo/et,exist,,,,0,,

out=Chrono,integer,,0.000000,,,laminar/B738/clock/fo/chrono_mode,exist,,,,0,,

out=Timer1min,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.TIME.Clock60Sec]>[59.000000]

&&

[SYSTEMS.TIME.Chrono]==[1.000000]

calc=[1.000000]

logic:

[SYSTEMS.TIME.Chrono]!=[1.000000]

calc=[0.000000]

logic:

calc=[SYSTEMS.TIME.Timer1min]

out=Clock60Sec,integer,,0.000000,,,laminar/B738/clock/fo/chrono_seconds,exist,,,,0,,



dev=POSITION

out=RA,double,ft,0.000000,,,sim/cockpit2/gauges/indicators/radio_altimeter_height_ft_pilot,exist,,,,0,,

out=ALT,double,ft,0.000000,,,sim/cockpit2/gauges/indicators/altitude_ft_pilot,exist,,,,0,,

logic:

calc=flr[SYSTEMS.POSITION.AltimFO]

out=AltimFO,integer,,0.000000,,,sim/cockpit2/gauges/indicators/altitude_ft_copilot,exist,,,,0,,

out=HDGMagFo,integer,,0.000000,,,laminar/B738/nd/hdg_mag_fo,exist,,,,0,,

logic:

calc=[SYSTEMS.POSITION.HDGMagFo]*[1.000000]

out=HDG_ND_Fo,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.POSITION.HDGMagFo]>[0.000000]

calc=[SYSTEMS.POSITION.HDGMagFo]

logic:

[SYSTEMS.POSITION.HDGMagFo]<[0.000000]

calc=[SYSTEMS.POSITION.HDGMagFo]*[-1.000000]

logic:

calc=[0.000000]

out=AirSpdKT,double,knots,0.000000,,,sim/cockpit2/gauges/indicators/airspeed_kts_pilot,exist,,,,0,,

out=MACH,double,mach,0.000000,,,sim/flightmodel/misc/machno,exist,,,,0,,

out=GrSpeed,double,kt,0.000000,,,sim/flightmodel/position/groundspeed,exist,,,,0,,

logic:

calc=*[1.943840]

out=GrSpeedMS,double,m/s,0.000000,,,sim/flightmodel/position/groundspeed,exist,,,,0,,

out=onAir,integer,yes,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.POSITION.RA]>[2.000000]

calc=[1.000000]

logic:

calc=[0.000000]

out=WasInAir,integer,yes,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[1.000000]

logic:

[COMMANDS.Flight.Reset]==[1.000000]

calc=[0.000000]

logic:

calc=[SYSTEMS.POSITION.WasInAir]

out=onGround,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.POSITION.RA]<=[2.000000]

calc=[1.000000]

logic:

calc=[0.000000]

out=Beta,double,,0.000000,,,sim/flightmodel/position/beta,exist,,,,0,,

out=PhiRoll,double,deg,0.000000,,,sim/flightmodel/position/phi,exist,,,,0,,

out=VVI,double,knots,0.000000,,,sim/cockpit2/gauges/indicators/vvi_fpm_pilot,exist,,,,0,,

out=CG,integer,%,0.000000,,,AirbusFBW/CGLocationPercent,exist,,,,0,,

out=GForce,double,,0.000000,,,sim/flightmodel2/misc/gforce_normal,exist,,,,0,,

out=GForceMax,double,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.POSITION.RA]>[10.000000]

calc=[1.000000]

logic:

[SYSTEMS.POSITION.GForce]>[SYSTEMS.POSITION.GForceMax]

calc=[SYSTEMS.POSITION.GForce]

logic:

calc=[SYSTEMS.POSITION.GForceMax]

out=RwyDeltaDep,double,,0.000000,,,jd/cpl/zibo/to_rwy/delta_hdg_deg,exist,,,,0,,

out=ApprRwyDistDep,integer,,0.000000,,,jd/cpl/zibo/to_rwy/dist_m,exist,,,,0,,

out=RwyDeltaArrival,integer,,0.000000,,,jd/cpl/zibo/ldg_rwy/delta_hdg_deg,exist,,,,0,,

out=ApprRwyDistArrival,integer,,0.000000,,,jd/cpl/zibo/ldg_rwy/dist_m,exist,,,,0,,



dev=FLGHTCONT

out=Pitch,integer,,0.000000,,,sim/flightmodel2/wing/elevator1_deg[8],exist,,,,0,,

out=Roll,double,,0.000000,,,sim/flightmodel2/controls/roll_ratio,exist,,,,0,,

out=Rudder,double,,0.000000,,,sim/flightmodel2/wing/rudder1_deg[0],exist,,,,0,,

out=CheckedPitch,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FLGHTCONT.Pitch]>[15.000000]

||

[SYSTEMS.FLGHTCONT.Pitch]<[-15.000000]

calc=[1.000000]

logic:

calc=[SYSTEMS.FLGHTCONT.CheckedPitch]

out=CheckedRoll,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FLGHTCONT.Roll]>[0.900000]

||

[SYSTEMS.FLGHTCONT.Roll]<[-0.900000]

calc=[1.000000]

logic:

calc=[SYSTEMS.FLGHTCONT.CheckedRoll]

out=CheckedRudder,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FLGHTCONT.Rudder]>[19.000000]

||

[SYSTEMS.FLGHTCONT.Rudder]<[-19.000000]

calc=[1.000000]

logic:

calc=[SYSTEMS.FLGHTCONT.CheckedRudder]

out=FlightContrChecked,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FLGHTCONT.CheckedPitch]==[1.000000]

&&

[SYSTEMS.FLGHTCONT.CheckedRoll]==[1.000000]

&&

[SYSTEMS.FLGHTCONT.CheckedRudder]==[1.000000]

calc=[1.000000]

logic:

calc=[SYSTEMS.FLGHTCONT.FlightContrChecked]



dev=WEATHER

out=SAT,double,,0.000000,,,sim/weather/temperature_ambient_c,exist,,,,0,,

out=TAT,double,degC,0.000000,,,sim/cockpit2/temperature/outside_air_LE_temp_degc,exist,,,,0,,

out=WindDir,integer,deg,0.000000,,,sim/weather/wind_direction_degt,exist,,,,0,,

logic:

calc=flr[1.000000]

out=WindSpeed,integer,kt,0.000000,,,sim/cockpit2/gauges/indicators/wind_speed_kts,exist,,,,0,,

logic:

calc=+[1.000000]flr[1.000000]

out=Visibility,integer,m,0.000000,,,sim/weather/visibility_reported_m,exist,,,,0,,

logic:

calc=flr[0.000000]

out=Rain,integer,%,0.000000,,,sim/weather/precipitation_on_aircraft_ratio,exist,,,,0,,

logic:

calc=*[100.000000]flr[1.000000]

out=BaroCurrent,integer,inhgX100,0.000000,,,sim/weather/barometer_current_inhg,exist,,,,0,,

logic:

calc=*[100.000000]flr[1.000000]

out=BaroSealevel100,integer,inhgX100,0.000000,,,sim/weather/barometer_sealevel_inhg,exist,,,,0,,

logic:

calc=*[100.000000]flr[1.000000]

out=BaroSeaLevel,double,,0.000000,,,sim/weather/barometer_sealevel_inhg,exist,,,,0,,

out=baroCurrent,double,inhg,0.000000,,,sim/weather/barometer_current_inhg,exist,,,,0,,

out=isFoBaroSetNeed,integer,,0.000000,,,jd/fo/needsetbaro,new,,,,0,,

logic:

calc=[SYSTEMS.WEATHER.isFoBaroSetNeed]

out=isFoBaroSetNeed_1,integer,,0.000000,,,jd/fo/needsetbaro1,new,,,,0,,

out=BaroSeaLevel,double,inhg,0.000000,,,sim/weather/barometer_sealevel_inhg,exist,,,,0,,

out=BaroSeaLevelHPA,double,inhg,0.000000,,,sim/weather/barometer_sealevel_inhg,exist,,,,0,,

logic:

calc=[SYSTEMS.WEATHER.BaroSeaLevel]*[33.884998]



dev=LIGHTS

out=PfdLt,double,,0.000000,,,AirbusFBW/DUBrightness[2],exist,,,,0,,

out=LedLandingLights,integer,,0.000000,,,laminar/B738/led_lights,exist,,,,0,,

out=OVHD_SeatBeltsSW,integer,,0.000000,,,laminar/B738/toggle_switch/seatbelt_sign_pos,exist,,,,0,,

out=OVHD_NoSmokeSW,integer,,0.000000,,,laminar/B738/toggle_switch/no_smoking_pos,exist,,,,0,,

out=OVHD_NavSW,integer,,0.000000,,,laminar/B738/toggle_switch/position_light_pos,exist,,,,0,,

out=OVHD_WingSW,integer,,0.000000,,,sim/cockpit2/switches/generic_lights_switch[0],exist,,,,0,,

out=OVHD_BeaconSW,integer,,0.000000,,,sim/cockpit2/switches/beacon_on,exist,,,,0,,

out=OVHD_RwyLeftSW,integer,,0.000000,,,laminar/B738/toggle_switch/rwy_light_left,exist,,,,0,,

out=OVHD_RwyRightSW,integer,,0.000000,,,laminar/B738/toggle_switch/rwy_light_right,exist,,,,0,,

out=OVHD_LandLSW,integer,,0.000000,,,laminar/B738/switch/land_lights_left_pos,exist,,,,0,,

out=OVHD_LandRSW,integer,,0.000000,,,laminar/B738/switch/land_lights_right_pos,exist,,,,0,,

out=OVHD_LandLRetr,integer,,0.000000,,,laminar/B738/switch/land_lights_ret_left_pos,exist,,,,0,,

out=OVHD_LandRRetr,integer,,0.000000,,,laminar/B738/switch/land_lights_ret_right_pos,exist,,,,0,,

out=OVHD_TaxiSW,integer,,0.000000,,,laminar/B738/toggle_switch/taxi_light_brightness_pos,exist,,,,0,,

out=OVHD_LogoSW,integer,,0.000000,,,laminar/B738/toggle_switch/logo_light,exist,,,,0,,

out=OVHD_WheelSW,integer,,0.000000,,,sim/cockpit2/switches/generic_lights_switch[5],exist,,,,0,,

out=OVHD_DomeSW,integer,,0.000000,,,laminar/B738/toggle_switch/cockpit_dome_pos,exist,,,,0,,

out=OVHD_Panel,double,,0.000000,,,laminar/B738/electric/panel_brightness[2],exist,,,,0,,

out=OVHD_Circuit,double,,0.000000,,,sim/cockpit2/switches/generic_lights_switch[27],exist,,,,0,,

out=PFD_Panel,double,,0.000000,,,sim/cockpit2/switches/panel_brightness_ratio[1],exist,,,,0,,

out=PED_Panel,double,,0.000000,,,sim/cockpit2/switches/panel_brightness_ratio[3],exist,,,,0,,

out=EmerExitSW,integer,,0.000000,,,laminar/B738/toggle_switch/emer_exit_lights,exist,,,,0,,

out=EmerExitCover,double,,0.000000,,,laminar/B738/button_switch/cover_position[9],exist,,,,0,,

out=Summ,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.LIGHTS.OVHD_LandLSW]+[SYSTEMS.LIGHTS.OVHD_LandRSW]+[SYSTEMS.LIGHTS.OVHD_LandLRetr]+[SYSTEMS.LIGHTS.OVHD_LandRRetr]

out=LightsOff,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_BeaconSW]==[0.000000]

&&

[SYSTEMS.LIGHTS.OVHD_NavSW]==[0.000000]

&&

[SYSTEMS.LIGHTS.OVHD_RwyLeftSW]==[0.000000]

&&

[SYSTEMS.LIGHTS.OVHD_LandLSW]<=[1.000000]

&&

[SYSTEMS.LIGHTS.OVHD_LandRSW]<=[1.000000]

&&

[SYSTEMS.LIGHTS.OVHD_TaxiSW]==[0.000000]

calc=[1.000000]

logic:

calc=[0.000000]

out=LightsPax,integer,,0.000000,,,laminar/B738/tab/line04g[37],exist,,,,0,,



dev=BRAKES

out=ParkBrakeHandlePos,integer,,0.000000,,,laminar/B738/parking_brake_pos,exist,,,,0,,

out=AutoBrakeSW,integer,,0.000000,,,laminar/B738/autobrake/autobrake_pos,exist,,,,0,,



dev=FMS

out=V1,integer,,0.000000,,,laminar/B738/FMS/v1_set,exist,,,,0,,

out=V1minus10,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.FMS.V1]-[2.000000]

out=V2,integer,,0.000000,,,laminar/B738/FMS/v2_set,exist,,,,0,,

out=VR,integer,,0.000000,,,laminar/B738/FMS/vr_set,exist,,,,0,,

out=Vref,integer,,0.000000,,,laminar/B738/FMS/approach_speed,exist,,,,0,,

out=FlapsAppr,integer,,0.000000,,,laminar/B738/FMS/approach_flaps,exist,,,,0,,

out=Tod,integer,,0.000000,,,laminar/B738/fms/vnav_td_dist,exist,,,,0,,

out=SpeedsSum,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.FMS.V1]+[SYSTEMS.FMS.VR]+[SYSTEMS.FMS.V2]

out=VRminus10,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.FMS.VR]-[3.000000]

out=TOThrustEng1,double,,0.000000,,,laminar/B738/engine/eng1_N1_bug,exist,,,,0,,

out=ToThrustEng2,double,,0.000000,,,laminar/B738/engine/eng2_N1_bug,exist,,,,0,,

out=ThrustSet,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.FMS.TOThrustEng1]-[0.030000]*[100.000000]

out=AltDest,integer,,0.000000,,,laminar/B738/fms/des_icao_alt,exist,,,,0,,

out=AltDestComp,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.FMS.AltDest]-[SYSTEMS.CABPRESS.LandAlt]

out=AltDestMod,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FMS.AltDestComp]>[0.000000]

calc=[SYSTEMS.FMS.AltDestComp]

logic:

[SYSTEMS.FMS.AltDestComp]<[0.000000]

calc=[SYSTEMS.FMS.AltDestComp]*[-1.000000]

logic:

calc=[SYSTEMS.FMS.AltDestMod]

out=AltAerodrom,integer,,0.000000,,,laminar/B738/FMS/aerodrom_altitude,exist,,,,0,,

out=AccelHeigt,integer,,0.000000,,,laminar/B738/FMS/accel_height,exist,,,,0,,

out=Acceleration,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.FMS.AltAerodrom]+[SYSTEMS.FMS.AccelHeigt]

out=CrzAlt,integer,,0.000000,,,laminar/B738/autopilot/fmc_cruise_alt,exist,,,,0,,

out=CrzAlt_It_was,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.POSITION.ALT]>[SYSTEMS.FMS.CrzAltMinus100]

calc=[1.000000]

logic:

calc=[SYSTEMS.FMS.CrzAlt_It_was]

out=CrzAltPlus100,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.FMS.CrzAlt]+[100.000000]

out=CrzAltMinus100,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.FMS.CrzAlt]-[100.000000]

out=CrzAltMinus1000,integer,,0.000000,0.000000,,,,,,,0,,

logic:

calc=[SYSTEMS.FMS.CrzAlt]-[1000.000000]

out=CrzAltPlus1000,integer,,0.000000,0.000000,,,,,,,0,,

logic:

calc=[SYSTEMS.FMS.CrzAlt]+[1000.000000]

out=TransAlt,integer,,0.000000,,,laminar/B738/FMS/fmc_trans_alt,exist,,,,0,,

out=TransAltMinus300,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.FMS.TransAlt]-[300.000000]

out=TransAltMinus1000,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.FMS.TransAlt]-[1000.000000]

out=TransAltMinus1300,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.FMS.TransAlt]-[1300.000000]

out=TransLevel,integer,,0.000000,,,laminar/B738/FMS/fmc_trans_lvl,exist,,,,0,,

out=TransLevelPlus300,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.FMS.TransLevel]+[300.000000]

out=TransLevelPlus1000,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.FMS.TransLevel]+[1000.000000]

out=TransLevelPlus1300,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.FMS.TransLevel]+[1300.000000]

out=MDA,double,,0.000000,,,laminar/B738/pfd/dh_pilot,exist,,,,0,,

out=DH,double,,0.000000,,,sim/cockpit/misc/radio_altimeter_minimum,exist,,,,0,,

out=DHplus100,double,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.FMS.DH]+[100.000000]

out=BlockFuel,integer,,0.000000,,,toliss_airbus/init/BlockFuel,exist,,,,0,,

out=ZFW,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.FMS.GW]-[SYSTEMS.MISC.TotalFuel]

out=GW,integer,,0.000000,,,sim/flightmodel/weight/m_total,exist,,,,0,,

out=GWCDU,integer,,0.000000,,,laminar/B738/FMS/fmc_gw,exist,,,,0,,

out=FlightPlane,integer,,0.000000,,,laminar/B738/FMS/fpln_dist,exist,,,,0,,

out=FlapsMCDU,integer,,0.000000,,,laminar/B738/FMS/takeoff_flaps,exist,,,,0,,

out=CGMCDU,integer,,0.000000,,,laminar/B738/FMS/fmc_cg,exist,,,,0,,

out=AP1_state,integer,,0.000000,,,AirbusFBW/AP1Engage,exist,,,,0,,

out=AP2_state,integer,,0.000000,,,AirbusFBW/AP2Engage,exist,,,,0,,

out=HdgRunwayInFms,integer,,0.000000,,,laminar/B738/fms/ref_runway_crs,exist,,,,0,,

logic:

calc=[SYSTEMS.FMS.HdgRunwayInFms]flr[1.000000]

out=HdgRunwayDest,integer,,0.000000,,,laminar/B738/fms/des_runway_crs,exist,,,,0,,

logic:

calc=[SYSTEMS.FMS.HdgRunwayDest]flr[1.000000]



dev=NAV

out=LocDev,double,,0.000000,,,laminar/radios/pilot/nav_hdef,exist,,,,0,,

out=GSDev,double,,0.000000,,,laminar/radios/pilot/nav_vdef,exist,,,,0,,

out=DME_Ils,double,,0.000000,,,laminar/radios/pilot/nav_dme,exist,,,,0,,

out=NavObs,double,,0.000000,,,laminar/radios/pilot/nav_obs,exist,,,,0,,

out=NavCourse,double,,0.000000,,,laminar/radios/pilot/nav_course,exist,,,,0,,

out=LocMode,integer,,0.000000,,,sim/cockpit/autopilot/mode_hnav,exist,,,,0,,

out=GSMode,integer,,0.000000,,,sim/cockpit/autopilot/mode_gls,exist,,,,0,,

out=Nav2Get,integer,,0.000000,,,jd/copilot/nav2set,new,,,,0,,

logic:

calc=[SYSTEMS.NAV.Nav2Get]

out=Nav2SetCopilot,integer,,0.000000,,,sim/cockpit/radios/nav2_freq_hz,exist,sim/cockpit/radios/nav2_freq_hz,exist,,0,,

logic:

[SYSTEMS.NAV.Nav2Get]==[1.000000]

calc=[SYSTEMS.ACP.Nav1]

logic:

calc=[SYSTEMS.NAV.Nav2SetCopilot]



dev=CDU

out=CDUPreflight,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FMS.GWCDU]>[0.000000]

&&

[SYSTEMS.FMS.FlapsMCDU]>[0.000000]

&&

[SYSTEMS.FMS.CGMCDU]>[0.000000]

&&

[SYSTEMS.FMS.V1]>[0.000000]

&&

[SYSTEMS.FMS.VR]>[0.000000]

&&

[SYSTEMS.FMS.V2]>[0.000000]

calc=[1.000000]

logic:

calc=[0.000000]



dev=LG

out=LG_Lever,double,,0.000000,,,laminar/B738/controls/gear_handle_down,exist,,,,0,,



dev=FLAPS

out=FlapLever,double,,0.000000,,,sim/cockpit2/controls/flap_ratio,exist,,,,0,,

out=FlapsMove,double,,0.000000,,,sim/flightmodel2/controls/flap_handle_deploy_ratio,exist,,,,0,,

out=FlapsMove_It_was,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FLAPS.FlapsMove]>[0.050000]

calc=[1.000000]

logic:

calc=[SYSTEMS.FLAPS.FlapsMove_It_was]

out=Flaps1Deg,double,,0.000000,,,sim/flightmodel2/wing/flap1_deg,exist,,,,0,,

out=Flaps2Deg,double,,0.000000,,,sim/flightmodel2/wing/flap2_deg,exist,,,,0,,

out=FlapsComp,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.FLAPS.Flaps1Deg]-[SYSTEMS.FLAPS.Flaps2Deg]

out=FlapsCopmMod,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FLAPS.FlapsComp]<[0.000000]

calc=[SYSTEMS.FLAPS.FlapsComp][-1.000000]

logic:

[SYSTEMS.FLAPS.FlapsComp]>=[0.000000]

calc=[SYSTEMS.FLAPS.FlapsComp]

logic:

calc=[0.000000]

out=FlapSet,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.FLAPS.FlapsMove]

graf=0.000000,0.000000

graf=0.020000,0.000000

graf=0.115000,1.000000

graf=0.135000,1.000000

graf=0.240000,2.000000

graf=0.260000,2.000000

graf=0.365000,5.000000

graf=0.385000,5.000000

graf=0.490000,10.000000

graf=0.510000,10.000000

graf=0.615000,15.000000

graf=0.635000,15.000000

graf=0.740000,25.000000

graf=0.760000,25.000000

graf=0.865000,30.000000

graf=0.885000,30.000000

graf=0.980000,40.000000

graf=1.000000,40.000000

out=FlapCompCDU,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.FLAPS.FlapSet]-[SYSTEMS.FMS.FlapsMCDU]

out=FlapCompApp,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.FLAPS.FlapSet]-[SYSTEMS.FMS.FlapsAppr]

out=Ok0,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.POSITION.onGround]==[1.000000]

calc=[1.000000]

logic:

[SYSTEMS.POSITION.onAir]==[1.000000]

&&

[SYSTEMS.POSITION.AirSpdKT]<[250.000000]

calc=[1.000000]

logic:

calc=[0.000000]

out=Ok1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.POSITION.onGround]==[1.000000]

calc=[1.000000]

logic:

[SYSTEMS.POSITION.onAir]==[1.000000]

&&

[SYSTEMS.POSITION.AirSpdKT]<[250.000000]

calc=[1.000000]

logic:

calc=[0.000000]

out=Ok2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.POSITION.onGround]==[1.000000]

calc=[1.000000]

logic:

[SYSTEMS.POSITION.onAir]==[1.000000]

&&

[SYSTEMS.POSITION.AirSpdKT]<[250.000000]

calc=[1.000000]

logic:

calc=[0.000000]

out=Ok5,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.POSITION.onGround]==[1.000000]

calc=[1.000000]

logic:

[SYSTEMS.POSITION.onAir]==[1.000000]

&&

[SYSTEMS.POSITION.AirSpdKT]<[250.000000]

calc=[1.000000]

logic:

calc=[0.000000]

out=Ok10,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.POSITION.onGround]==[1.000000]

calc=[1.000000]

logic:

[SYSTEMS.POSITION.onAir]==[1.000000]

&&

[SYSTEMS.POSITION.AirSpdKT]<[210.000000]

calc=[1.000000]

logic:

calc=[0.000000]

out=Ok15,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.POSITION.onGround]==[1.000000]

calc=[1.000000]

logic:

[SYSTEMS.POSITION.onAir]==[1.000000]

&&

[SYSTEMS.POSITION.AirSpdKT]<[200.000000]

calc=[1.000000]

logic:

calc=[0.000000]

out=Ok25,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.POSITION.onGround]==[1.000000]

calc=[1.000000]

logic:

[SYSTEMS.POSITION.onAir]==[1.000000]

&&

[SYSTEMS.POSITION.AirSpdKT]<[190.000000]

calc=[1.000000]

logic:

calc=[0.000000]

out=Ok30,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.POSITION.onGround]==[1.000000]

calc=[1.000000]

logic:

[SYSTEMS.POSITION.onAir]==[1.000000]

&&

[SYSTEMS.POSITION.AirSpdKT]<[175.000000]

calc=[1.000000]

logic:

calc=[0.000000]

out=Ok40,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.POSITION.onGround]==[1.000000]

calc=[1.000000]

logic:

[SYSTEMS.POSITION.onAir]==[1.000000]

&&

[SYSTEMS.POSITION.AirSpdKT]<[162.000000]

calc=[1.000000]

logic:

calc=[0.000000]



dev=SPEEDBRAKE

out=SB_DrfSim,double,,0.000000,,,sim/cockpit2/controls/speedbrake_ratio,exist,,,,0,,

out=SB_Lever,double,,0.000000,,,laminar/B738/flt_ctrls/speedbrake_lever,exist,,,,0,,



dev=THS

out=SimThsK,double,,0.000000,,,sim/flightmodel2/controls/elevator_trim,exist,,,,0,,

out=ThsUpRange,integer,,0.000000,,,sim/aircraft/controls/acf_hstb_trim_up,exist,,,,0,,

out=ThsDnRange,integer,,0.000000,,,sim/aircraft/controls/acf_hstb_trim_dn,exist,,,,0,,

out=ThsNow,double,,0.000000,,,sim/flightmodel2/controls/stabilizer_deflection_degrees,exist,,,,0,,

logic:

calc=*[1.000000]

graf=-9.000000,17.000000

graf=8.150000,0.000000

out=ThsToNeed,double,,0.000000,,,laminar/B738/FMS/trim_calc,exist,,,,0,,

out=ThsToNeed10,double,,0.000000,,,laminar/B738/FMS/trim_calc,exist,,,,0,,

logic:

calc=*[10.000000]

out=ThsError,double,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.THS.ThsNow]>=[SYSTEMS.THS.ThsToNeed]

calc=[SYSTEMS.THS.ThsNow]-[SYSTEMS.THS.ThsToNeed]

logic:

calc=[SYSTEMS.THS.ThsToNeed]-[SYSTEMS.THS.ThsNow]

out=SimThsNeedK,double,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.THS.ThsToNeed]>[0.000000]

calc=[SYSTEMS.THS.ThsToNeed]/[SYSTEMS.THS.ThsUpRange]

logic:

calc=[SYSTEMS.THS.ThsToNeed]/[SYSTEMS.THS.ThsDnRange]



dev=WEIGHT

out=GW,double,kg,0.000000,,,sim/flightmodel/weight/m_total,exist,,,,0,,

out=FOB,double,kg,0.000000,,,sim/flightmodel/weight/m_fuel_total,exist,,,,0,,



dev=FCOMPHASE

out=PHASE,integer,,0.000000,,,AirbusFBW/ECAMFlightPhase,exist,,,,0,,

out=NotPowered,integer,,0.000000,,,,,,,,0,,

out=Powered,integer,,1.000000,,,,,,,,0,,

out=OneEngStart,integer,,2.000000,,,,,,,,0,,

out=EngToPwr,integer,,3.000000,,,,,,,,0,,

out=80Kts,integer,,4.000000,,,,,,,,0,,

out=LiftOff,integer,,5.000000,,,,,,,,0,,

out=1500ftClimb,integer,,6.000000,,,,,,,,0,,

out=800ftDescend,integer,,7.000000,,,,,,,,0,,

out=TouchDown,integer,,8.000000,,,,,,,,0,,

out=80ktsRollOut,integer,,9.000000,,,,,,,,0,,

out=AllEngShutDown,integer,,10.000000,,,,,,,,0,,



dev=FLIGHTPHASE

out=PHASE,integer,,0.000000,,,laminar/B738/FMS/flight_phase,exist,,,,0,,

out=Preflight,integer,,0.000000,,,,,,,,0,,

out=Climb,integer,,1.000000,,,,,,,,0,,

out=Cruise,integer,,2.000000,,,,,,,,0,,

out=Descent,integer,,5.000000,,,,,,,,0,,

out=Approach,integer,,7.000000,,,,,,,,0,,

out=GoAround,integer,,8.000000,,,,,,,,0,,

out=Done,integer,,0.000000,,,,,,,,0,,



dev=ENGINE

out=Eng1N1,double,,0.000000,,,sim/flightmodel/engine/ENGN_N1_[0],exist,,,,0,,

out=Eng2N1,double,,0.000000,,,sim/flightmodel/engine/ENGN_N1_[1],exist,,,,0,,

out=N1Copm,double,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.ENGINE.Eng1N1]-[SYSTEMS.ENGINE.Eng2N1]

out=N1CopmMod,double,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.N1Copm]<[0.000000]

calc=[SYSTEMS.ENGINE.N1Copm]*[-1.000000]

logic:

[SYSTEMS.ENGINE.N1Copm]>[0.000000]

calc=[SYSTEMS.ENGINE.N1Copm]

logic:

calc=[0.000000]

out=Eng1N2,double,,0.000000,,,laminar/B738/engine/indicators/N2_percent_1,exist,,,,0,,

out=Eng2N2,double,,0.000000,,,laminar/B738/engine/indicators/N2_percent_2,exist,,,,0,,

out=Eng1Lever,double,,0.000000,,,laminar/B738/engine/thr_lvr1,exist,,,,0,,

out=Eng2Lever,double,,0.000000,,,laminar/B738/engine/thr_lvr2,exist,,,,0,,

out=EngMasterSW_1,double,,0.000000,,,laminar/B738/engine/mixture_ratio1,exist,,,,0,,

out=EngMasterSW_2,double,,0.000000,,,laminar/B738/engine/mixture_ratio2,exist,,,,0,,

out=EngMastSumm,double,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.ENGINE.EngMasterSW_1]+[SYSTEMS.ENGINE.EngMasterSW_2]

out=Eng1StartSW,integer,,0.000000,,,laminar/B738/engine/starter1_pos,exist,,,,0,,

out=Eng2StartSW,integer,,0.000000,,,laminar/B738/engine/starter2_pos,exist,,,,0,,

out=Starter1,integer,,0.000000,,,jd/fo/starter1,new,,,,0,,

out=Starter2,integer,,0.000000,,,jd/fo/starter2,new,,,,0,,

out=Eng1Run,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng1N2]>=[55.000000]

&&

[SYSTEMS.ENGINE.EngMasterSW_1]==[1.000000]

calc=[1.000000]

logic:

calc=[0.000000]

out=Eng2Run,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng2N2]>=[55.000000]

&&

[SYSTEMS.ENGINE.EngMasterSW_2]==[1.000000]

calc=[1.000000]

logic:

calc=[0.000000]

out=EngsRun,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.ENGINE.Eng1Run]+[SYSTEMS.ENGINE.Eng2Run]

out=EngRunWas,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng1N2]>=[30.000000]

&&

[SYSTEMS.ENGINE.Eng2N2]>=[30.000000]

calc=[1.000000]

logic:

[SYSTEMS.ENGINE.Eng1N2]<[15.000000]

&&

[SYSTEMS.ENGINE.Eng2N2]<[15.000000]

&&

[SYSTEMS.POSITION.WasInAir]==[1.000000]

calc=[0.000000]

logic:

calc=[SYSTEMS.ENGINE.EngRunWas]

out=ReversL,double,,0.000000,,,sim/flightmodel2/engines/thrust_reverser_deploy_ratio[0],exist,,,,0,,

out=Revers1annunc,integer,,0.000000,,,laminar/B738/annunciator/reverser_fail_0,exist,,,,0,,

out=ReversR,double,,0.000000,,,sim/flightmodel2/engines/thrust_reverser_deploy_ratio[1],exist,,,,0,,

out=Revers2annunc,integer,,0.000000,,,laminar/B738/annunciator/reverser_fail_1,exist,,,,0,,

out=RevGreen,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.ReversL]>[0.000000]

&&

[SYSTEMS.ENGINE.ReversR]>[0.000000]

calc=[1.000000]

logic:

calc=[0.000000]

out=OilQtyEng1,double,,0.000000,,,sim/flightmodel/engine/ENGN_oil_quan[0],exist,,,,0,,

out=OilQtyEng2,double,,0.000000,,,sim/flightmodel/engine/ENGN_oil_quan[0],exist,,,,0,,

out=EEC1,integer,,0.000000,,,sim/cockpit2/engine/actuators/fadec_on[0],exist,,,,0,,

out=EEC1Cover,double,,0.000000,,,laminar/B738/button_switch/cover_position[0],exist,,,,0,,

out=EEC2,integer,,0.000000,,,sim/cockpit2/engine/actuators/fadec_on[1],exist,,,,0,,

out=EEC2Cover,double,,0.000000,,,laminar/B738/button_switch/cover_position[1],exist,,,,0,,



dev=AIR

out=Pack1,integer,,0.000000,,,laminar/B738/air/l_pack_pos,exist,,,,0,,

out=Pack2,integer,,0.000000,,,laminar/B738/air/r_pack_pos,exist,,,,0,,

out=SummPacks,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.AIR.Pack1]+[SYSTEMS.AIR.Pack2]

out=Eng1BleedSW,integer,,0.000000,,,laminar/B738/toggle_switch/bleed_air_1_pos,exist,,,,0,,

out=Eng2BleedSW,integer,,0.000000,,,laminar/B738/toggle_switch/bleed_air_2_pos,exist,,,,0,,

out=APUBleedSW,integer,,0.000000,,,laminar/B738/toggle_switch/bleed_air_apu_pos,exist,,,,0,,

out=TrimAir,integer,,0.000000,,,laminar/B738/air/trim_air_pos,exist,,,,0,,

out=L_Fan,integer,,0.000000,,,laminar/B738/air/l_recirc_fan_pos,exist,,,,0,,

out=R_Fan,integer,,0.000000,,,laminar/B738/air/r_recirc_fan_pos,exist,,,,0,,

out=ContCabTempSW,double,,0.000000,,,laminar/B738/air/cont_cab_temp/rheostat,exist,,,,0,,

out=FwdCabinTempSW,double,,0.000000,,,laminar/B738/air/fwd_cab_temp/rheostat,exist,,,,0,,

out=AftCabinTempSW,double,,0.000000,,,laminar/B738/air/aft_cab_temp/rheostat,exist,,,,0,,

out=IsolValve,integer,,0.000000,,,laminar/B738/air/isolation_valve_pos,exist,,,,0,,

out=TempRheostatLeft,double,,0.000000,,,laminar/B738/air/cont_cab_temp/rheostat_700,exist,,,,0,,

out=TempRheostatRight,double,,0.000000,,,laminar/B738/air/pass_cab_temp/rheostat_700,exist,,,,0,,



dev=MCP

out=FD2,integer,,0.000000,,,laminar/B738/autopilot/pfd_fd_cmd_fo,exist,,,,0,,

out=MasterCaution,integer,,0.000000,,,laminar/B738/annunciator/master_caution_light,exist,,,,0,,

out=AP1,integer,,0.000000,,,laminar/B738/autopilot/cmd_a_status,exist,,,,0,,

out=AP2,integer,,0.000000,,,laminar/B738/autopilot/cmd_b_status,exist,,,,0,,

out=APSum,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.MCP.AP1]+[SYSTEMS.MCP.AP2]

out=VorLocPB,integer,,0.000000,,,laminar/B738/autopilot/vorloc_status,exist,,,,0,,

out=Speed,integer,,0.000000,,,laminar/B738/autopilot/mcp_speed_dial_kts,exist,,,,0,,

out=SpeedCompV2,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.MCP.Speed]-[SYSTEMS.FMS.V2]

out=HDG,integer,,0.000000,,,laminar/B738/autopilot/mcp_hdg_dial,exist,,,,0,,

out=ALT,double,,0.000000,,,laminar/B738/autopilot/mcp_alt_dial,exist,,,,0,,

out=isNewALT,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MCP.ALT]!=[SYSTEMS.MCP.ALT_Old]

calc=[1.000000]

logic:

calc=[0.000000]

out=ALT_Old,double,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.MCP.ALT]

out=ApprPB,integer,,0.000000,,,laminar/B738/autopilot/app_status,exist,,,,0,,

out=ApprPBwasARM,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MCP.ApprPB]==[1.000000]

calc=[1.000000]

logic:

calc=[SYSTEMS.MCP.ApprPBwasARM]

out=AthrMode,integer,,0.000000,,,AirbusFBW/ATHRmode2,exist,,,,0,,

out=SPDManaged,double,,0.000000,,,AirbusFBW/SPDmanaged,exist,,,,0,,

out=BaroStdCap,integer,,0.000000,,,laminar/B738/EFIS/baro_set_std_pilot,exist,,,,0,,

out=ChangeHPA_Cap,integer,,0.000000,,,laminar/B738/EFIS_control/capt/baro_in_hpa,exist,,,,0,,

out=BaroStdFo,integer,,0.000000,,,laminar/B738/EFIS/baro_set_std_copilot,exist,,,,0,,

out=ChangeHPA_Fo,integer,,0.000000,,,laminar/B738/EFIS_control/fo/baro_in_hpa,exist,,,,0,,

out=BaroSetInHgCap,double,,0.000000,,,sim/cockpit2/gauges/actuators/barometer_setting_in_hg_pilot,exist,,,,0,,

out=BaroSetHpaCap,double,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.MCP.BaroSetInHgCap]*[33.884998]

out=SetQNHBaroInHgFo,double,,0.000000,,,sim/cockpit2/gauges/actuators/barometer_setting_in_hg_copilot,exist,sim/cockpit2/gauges/actuators/barometer_setting_in_hg_copilot,exist,,0,,

logic:

[SYSTEMS.WEATHER.isFoBaroSetNeed]==[1.000000]

calc=[SYSTEMS.WEATHER.BaroSeaLevel]

logic:

calc=[SYSTEMS.MCP.SetQNHBaroInHgFo]

out=SetBaroInHgFO,double,,0.000000,,,sim/cockpit2/gauges/actuators/barometer_setting_in_hg_copilot,exist,sim/cockpit2/gauges/actuators/barometer_setting_in_hg_copilot,exist,,0,,

logic:

[SYSTEMS.WEATHER.isFoBaroSetNeed_1]==[1.000000]

calc=[SYSTEMS.MCP.BaroSetInHgCap]

logic:

calc=[SYSTEMS.MCP.SetBaroInHgFO]

out=BaroSetInHgFO,double,,0.000000,,,sim/cockpit2/gauges/actuators/barometer_setting_in_hg_copilot,exist,,,,0,,

out=BaroSetInHgFo100,double,x100,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.MCP.BaroSetInHgFO]*[100.000000]

out=BaroSetHpaFO,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.MCP.BaroSetInHgFO]*[33.884998]

out=BaroSetHpaFoFloor,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.MCP.BaroSetHpaFO]flr[1.000000]

out=inHg_or_hPaCap,integer,,0.000000,,,AirbusFBW/BaroUnitCapt,exist,,,,0,,

out=inHg_or_hPaFo,integer,,0.000000,,,AirbusFBW/BaroUnitFO,exist,,,,0,,

out=BaroDiffCap,double,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.WEATHER.BaroSeaLevel]-[SYSTEMS.MCP.BaroSetInHgCap]

out=MDA_DH_CapSet,integer,,0.000000,,,laminar/B738/pfd/dh_pilot,exist,,,,0,,

out=DH_CoPilot,integer,,0.000000,,,laminar/B738/pfd/dh_copilot,exist,laminar/B738/pfd/dh_copilot,exist,,0,,

logic:

[SYSTEMS.MCP.DH_need]==[1.000000]

calc=[SYSTEMS.MCP.MDA_DH_CapSet]

logic:

calc=[SYSTEMS.MCP.DH_CoPilot]

out=MDA_CoPilot,integer,,0.000000,,,laminar/B738/pfd/dh_copilot,exist,laminar/B738/pfd/dh_copilot,exist,,0,,

logic:

[SYSTEMS.MCP.MDA_need]==[1.000000]

calc=[SYSTEMS.MCP.MDA_DH_CapSet]

logic:

calc=[SYSTEMS.MCP.MDA_CoPilot]

out=MDA_need,integer,,0.000000,,,jd/fo/needsetmda,new,,,,0,,

out=DH_need,integer,,0.000000,,,jd/fo/needsetdh,new,,,,0,,

out=CrzNeed,integer,,0.000000,,,jd/fo/needsetcrz,new,,,,0,,

out=RadioSwCap,integer,,0.000000,,,laminar/B738/EFIS_control/cpt/minimums,exist,,,,0,,

out=RadioSwFo,integer,,0.000000,,,laminar/B738/EFIS_control/fo/minimums,exist,,,,0,,

out=Course2,integer,,0.000000,,,laminar/B738/autopilot/course_copilot,exist,,,,0,,

out=Course2need,integer,,0.000000,,,jd/fo/rwyneedhdg,new,,,,0,,

out=Course2needDest,integer,,0.000000,,,jd/fo/rwyneedhdgdest,new,,,,0,,

out=Course2Set,integer,,0.000000,,,laminar/B738/autopilot/course_copilot,exist,laminar/B738/autopilot/course_copilot,exist,,0,,

logic:

[SYSTEMS.MCP.Course2need]==[1.000000]

calc=[SYSTEMS.FMS.HdgRunwayInFms]

logic:

calc=[SYSTEMS.MCP.Course2Set]

out=Course2SetDest,integer,,0.000000,,,laminar/B738/autopilot/course_copilot,exist,laminar/B738/autopilot/course_copilot,exist,,0,,

logic:

[SYSTEMS.MCP.Course2needDest]==[1.000000]

calc=[SYSTEMS.FMS.HdgRunwayDest]

logic:

calc=[SYSTEMS.MCP.Course2SetDest]



dev=PFD

out=FlapsUpShow,integer,,0.000000,,,laminar/B738/pfd/flaps_up_show,exist,,,,0,,

out=FlapsUp,integer,,0.000000,,,laminar/B738/pfd/flaps_up,exist,,,,0,,

out=Flaps1Show,integer,,0.000000,,,laminar/B738/pfd/flaps_1_show,exist,,,,0,,

out=Flaps1,integer,,0.000000,,,laminar/B738/pfd/flaps_1,exist,,,,0,,

out=Flaps2Show,integer,,0.000000,,,laminar/B738/pfd/flaps_2_show,exist,,,,0,,

out=Flaps2,integer,,0.000000,,,laminar/B738/pfd/flaps_2,exist,,,,0,,

out=Flaps5Show,integer,,0.000000,,,laminar/B738/pfd/flaps_5_show,exist,,,,0,,

out=Flaps5,integer,,0.000000,,,laminar/B738/pfd/flaps_5,exist,,,,0,,

out=Flaps10Show,integer,,0.000000,,,laminar/B738/pfd/flaps_10_show,exist,,,,0,,

out=Flaps10,integer,,0.000000,,,laminar/B738/pfd/flaps_10,exist,,,,0,,

out=Flaps15Show,integer,,0.000000,,,laminar/B738/pfd/flaps_15_show,exist,,,,0,,

out=Flaps15,integer,,0.000000,,,laminar/B738/pfd/flaps_15,exist,,,,0,,

out=Flaps25Show,integer,,0.000000,,,laminar/B738/pfd/flaps_25_show,exist,,,,0,,

out=Flaps25,integer,,0.000000,,,laminar/B738/pfd/flaps_25,exist,,,,0,,



dev=FRONTPANEL

out=TerrNDSW,integer,,0.000000,,,AirbusFBW/TerrainSelectedND2,exist,,,,0,,

out=SysPage,integer,,0.000000,,,laminar/B738/systems/lowerDU_page2,exist,,,,0,,

out=EngPag,integer,,0.000000,,,laminar/B738/systems/lowerDU_page,exist,,,,0,,

out=ClockFO,integer,,0.000000,,,laminar/B738/clock/chrono_display_mode_fo,exist,,,,0,,

out=MainPanelDisplay,integer,,0.000000,,,laminar/B738/display_units/idu_fo,exist,,,,0,,

out=LowerDisplay,integer,,0.000000,,,laminar/B738/display_units/ldu,exist,,,,0,,

out=GPWSFlap,double,,0.000000,,,laminar/B738/toggle_switch/gpws_flap_cover_pos,exist,,,,0,,

out=GPWSGear,double,,0.000000,,,laminar/B738/toggle_switch/gpws_gear_cover_pos,exist,,,,0,,

out=GPWSTerr,double,,0.000000,,,laminar/B738/toggle_switch/gpws_terr_cover_pos,exist,,,,0,,

out=VrefSet,integer,,0.000000,,,laminar/B738/toggle_switch/spd_ref,exist,,,,0,,

out=N1Set,integer,,0.000000,,,laminar/B738/toggle_switch/n1_set_source,exist,,,,0,,



dev=PEDESTAL

out=EngSelectSW,integer,,0.000000,,,AirbusFBW/ENGModeSwitch,exist,,,,0,,

out=Transponder,integer,,0.000000,,,laminar/B738/knob/transponder_pos,exist,,,,0,,

out=Tcas,integer,,0.000000,,,laminar/B738/knob/transponder_pos,exist,,,,0,,

out=ATC,integer,,0.000000,,,AirbusFBW/XPDRTCASMode,exist,,,,0,,

out=ATTHDGSW,integer,,0.000000,,,AirbusFBW/AttitudeSwitching,exist,,,,0,,

out=AIRDATASW,integer,,0.000000,,,AirbusFBW/AirDataSwitching,exist,,,,0,,

out=EISDMCSW,integer,,0.000000,,,AirbusFBW/DMCSwitching,exist,,,,0,,

out=ECAMSW,integer,,0.000000,,,AirbusFBW/ECAMNDSwitching,exist,,,,0,,

out=EngModeSW,integer,,0.000000,,,AirbusFBW/ENGModeSwitch,exist,,,,0,,

out=RadarSWCap,integer,,0.000000,,,laminar/B738/EFIS/EFIS_wx_on,exist,,,,0,,

out=RadarSWFo,integer,,0.000000,,,laminar/B738/EFIS/fo/EFIS_wx_on,exist,,,,0,,

out=PWS_SW,integer,,0.000000,,,ckpt/ped/radar/pwr/anim,exist,,,,0,,

out=RudderTrim,double,,0.000000,,,sim/cockpit2/controls/rudder_trim,exist,,,,0,,

out=RudderTrimComp,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.PEDESTAL.RudderTrim]<[-0.040000]

calc=[1.000000]

logic:

[SYSTEMS.PEDESTAL.RudderTrim]>[0.040000]

calc=[1.000000]

logic:

calc=[0.000000]

out=AileronTrim,double,,0.000000,,,sim/cockpit2/controls/aileron_trim,exist,,,,0,,

out=AileronTrimComp,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.PEDESTAL.AileronTrim]<[-0.100000]

calc=[1.000000]

logic:

[SYSTEMS.PEDESTAL.AileronTrim]>[0.100000]

calc=[1.000000]

logic:

calc=[0.000000]

out=TrimLock1,integer,,0.000000,,,laminar/B738/toggle_switch/el_trim_lock_pos,exist,,,,0,,

out=TrimLock2,integer,,0.000000,,,laminar/B738/toggle_switch/ap_trim_lock_pos,exist,,,,0,,



dev=ECAMPAGE

out=Fctl,integer,,0.000000,,,AirbusFBW/SDFCTL,exist,,,,0,,

out=Eng,integer,,0.000000,,,AirbusFBW/SDENG,exist,,,,0,,

out=Bleed,integer,,0.000000,,,AirbusFBW/SDBLEED,exist,,,,0,,

out=Press,integer,,0.000000,,,AirbusFBW/SDPRESS,exist,,,,0,,

out=Elec,integer,,0.000000,,,AirbusFBW/SDELEC,exist,,,,0,,

out=Hyd,integer,,0.000000,,,AirbusFBW/SDHYD,exist,,,,0,,

out=Fuel,integer,,0.000000,,,AirbusFBW/SDFUEL,exist,,,,0,,

out=Apu,integer,,0.000000,,,AirbusFBW/SDAPU,exist,,,,0,,

out=Cond,integer,,0.000000,,,AirbusFBW/SDCOND,exist,,,,0,,

out=Door,integer,,0.000000,,,AirbusFBW/SDDOOR,exist,,,,0,,

out=Wheel,integer,,0.000000,,,AirbusFBW/SDWHEEL,exist,,,,0,,

out=STS,integer,,0.000000,,,AirbusFBW/SDSTATUS,exist,,,,0,,

out=All,integer,,0.000000,,,AirbusFBW/SDPage,exist,,,,0,,



dev=FIRE

out=Eng1FirePB,double,,0.000000,,,laminar/B738/fire/engine01/ext_switch/pos_arm,exist,,,,0,,

out=Eng2FirePB,double,,0.000000,,,laminar/B738/fire/engine02/ext_switch/pos_arm,exist,,,,0,,

out=APUFirePB,double,,0.000000,,,laminar/B738/fire/apu/ext_switch/pos_arm,exist,,,,0,,



dev=HYD

out=Eng1PumpSW,integer,,0.000000,,,laminar/B738/toggle_switch/hydro_pumps1_pos,exist,,,,0,,

out=ElecPump2,integer,,0.000000,,,laminar/B738/toggle_switch/electric_hydro_pumps1_pos,exist,,,,0,,

out=ElecPump1,integer,,0.000000,,,laminar/B738/toggle_switch/electric_hydro_pumps2_pos,exist,,,,0,,

out=Eng2PumpSW,integer,,0.000000,,,laminar/B738/toggle_switch/hydro_pumps2_pos,exist,,,,0,,

out=HydQty_A,double,,0.000000,,,laminar/B738/hydraulic/hyd_A_qty[0],exist,,,,0,,

out=HydQty_B,double,,0.000000,,,laminar/B738/hydraulic/hyd_B_qty[1],exist,,,,0,,



dev=FUEL

out=LAftPumpSW,integer,,0.000000,,,laminar/B738/fuel/fuel_tank_pos_lft1,exist,,,,0,,

out=LFwdPumpSW,integer,,0.000000,,,laminar/B738/fuel/fuel_tank_pos_lft2,exist,,,,0,,

out=LCtrPumpSW,integer,,0.000000,,,laminar/B738/fuel/fuel_tank_pos_ctr1,exist,,,,0,,

out=CrossFeedSW,double,,0.000000,,,laminar/B738/knobs/cross_feed,exist,,,,0,,

out=RCtrPumpSW,integer,,0.000000,,,laminar/B738/fuel/fuel_tank_pos_ctr2,exist,,,,0,,

out=RFwdPumpSW,integer,,0.000000,,,laminar/B738/fuel/fuel_tank_pos_rgt2,exist,,,,0,,

out=RAftPumpSW,integer,,0.000000,,,laminar/B738/fuel/fuel_tank_pos_rgt1,exist,,,,0,,

out=PumpsAll,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LAftPumpSW]==[1.000000]

&&

[SYSTEMS.FUEL.LFwdPumpSW]==[1.000000]

&&

[SYSTEMS.FUEL.LCtrPumpSW]==[1.000000]

&&

[SYSTEMS.FUEL.RCtrPumpSW]==[1.000000]

&&

[SYSTEMS.FUEL.RFwdPumpSW]==[1.000000]

&&

[SYSTEMS.FUEL.RAftPumpSW]==[1.000000]

calc=[1.000000]

logic:

calc=[0.000000]

out=PumpsNoCtr,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LAftPumpSW]==[1.000000]

&&

[SYSTEMS.FUEL.LAftPumpSW]==[1.000000]

&&

[SYSTEMS.FUEL.RFwdPumpSW]==[1.000000]

&&

[SYSTEMS.FUEL.RAftPumpSW]==[1.000000]

calc=[1.000000]

logic:

calc=[0.000000]

out=CenterTank,integer,,0.000000,,,laminar/B738/fuel/center_tank_kgs,exist,,,,0,,



dev=ELEC

out=Gen1and2SW,integer,,0.000000,,,laminar/B738/electrical/gen1_pos,exist,,,,0,,

out=GenON,integer,,0.000000,,,sim/cockpit2/annunciators/generator,exist,,,,0,,

out=APUGen1Bus,integer,,0.000000,,,laminar/B738/electrical/apu_power_bus1,exist,,,,0,,

out=APUGen2Bus,integer,,0.000000,,,laminar/B738/electrical/apu_power_bus2,exist,,,,0,,

out=ApuGenBusAvail,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.APUGen1Bus]!=[0.000000]

||

[SYSTEMS.ELEC.APUGen2Bus]!=[0.000000]

calc=[1.000000]

logic:

calc=[0.000000]

out=SourceIndLeft,double,,0.000000,,,laminar/B738/annunciator/source_off1,exist,,,,0,,

out=SourceIndRight,double,,0.000000,,,laminar/B738/annunciator/source_off2,exist,,,,0,,

out=BatterySW,integer,,0.000000,,,laminar/B738/electric/battery_pos,exist,,,,0,,

out=StandbyPowerPB,integer,,0.000000,,,laminar/B738/electric/standby_bat_pos,exist,,,,0,,

out=StanddyPowerCover,double,,0.000000,,,laminar/B738/button_switch/cover_position[3],exist,,,,0,,

out=BasTransCover,double,,0.000000,,,laminar/B738/button_switch/cover_position[6],exist,,,,0,,

out=BusTransSW,integer,,0.000000,,,sim/cockpit2/electrical/cross_tie,exist,,,,0,,

out=ExtPwrSW,integer,,0.000000,,,sim/cockpit/electrical/gpu_on,exist,,,,0,,

out=ExtPwrConnect,integer,,0.000000,,,laminar/B738/fmod/gpu_deployed,exist,,,,0,,

out=JetwayPower,integer,,0.000000,,,laminar/B738/jetway_power,exist,,,,0,,

out=Gen2SW,integer,,0.000000,,,AirbusFBW/ElecOHPArray[1],exist,,,,0,,

out=CabUtil,integer,,0.000000,,,laminar/B738/toggle_switch/cab_util_pos,exist,,,,0,,

out=IfePass,integer,,0.000000,,,laminar/B738/toggle_switch/ife_pass_seat_pos,exist,,,,0,,

out=Gen1DiscCover,double,,0.000000,,,laminar/B738/button_switch/cover_position[4],exist,,,,0,,

out=Gen2DiscCover,double,,0.000000,,,laminar/B738/button_switch/cover_position[5],exist,,,,0,,

out=Gen1Disc,integer,,0.000000,,,laminar/B738/one_way_switch/drive_disconnect1_pos,exist,,,,0,,

out=Gen2Disc,integer,,0.000000,,,laminar/B738/one_way_switch/drive_disconnect2_pos,exist,,,,0,,

out=ACBus1,integer,,0.000000,,,laminar/B738/electric/ac_tnsbus1_status,exist,,,,0,,

out=ACBus2,integer,,0.000000,,,laminar/B738/electric/ac_tnsbus2_status,exist,,,,0,,

out=ACBusAvail,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.ELEC.ACBus1]+[SYSTEMS.ELEC.ACBus2]



dev=CABPRESS

out=LandAlt,integer,,0.000000,,,laminar/B738/pressurization/knobs/landing_alt,exist,,,,0,,

out=LandAltNeed,integer,,0.000000,,,jd/fo/needsetlandalt,new,,,,0,,

out=LandAltSet,integer,,0.000000,,,laminar/B738/pressurization/knobs/landing_alt,exist,laminar/B738/pressurization/knobs/landing_alt,exist,,0,,

logic:

[SYSTEMS.CABPRESS.LandAltNeed]==[1.000000]

calc=[SYSTEMS.FMS.AltDest]

logic:

calc=[SYSTEMS.CABPRESS.LandAltSet]

out=FltAlt,integer,,0.000000,,,sim/cockpit/pressure/max_allowable_altitude,exist,,,,0,,

out=FltAltSet,integer,,0.000000,,,sim/cockpit/pressure/max_allowable_altitude,exist,sim/cockpit/pressure/max_allowable_altitude,exist,,0,,

logic:

[SYSTEMS.MCP.CrzNeed]==[1.000000]

calc=[SYSTEMS.FMS.CrzAlt]

logic:

calc=[SYSTEMS.CABPRESS.FltAltSet]



dev=ICE

out=WingPB,double,,0.000000,,,laminar/B738/system/wing_anti_ice_valve[1],exist,,,,0,,

out=ENG1IcePB,integer,,0.000000,,,laminar/B738/ice/eng1_heat_pos,exist,,,,0,,

out=ENG2IcePB,integer,,0.000000,,,laminar/B738/ice/eng2_heat_pos,exist,,,,0,,

out=ProbeHeatA,integer,,0.000000,,,laminar/B738/toggle_switch/capt_probes_pos,exist,,,,0,,

out=ProbeHeatB,integer,,0.000000,,,laminar/B738/toggle_switch/fo_probes_pos,exist,,,,0,,

out=AntiIceOn,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.ICE.WingPB]+[SYSTEMS.ICE.ENG1IcePB]+[SYSTEMS.ICE.ENG2IcePB]



dev=APU

out=StartSW,integer,,0.000000,,,laminar/B738/spring_toggle_switch/APU_start_pos,exist,,,,0,,

out=AvailAPU,double,,0.000000,,,sim/cockpit/engine/APU_running,exist,,,,0,,

out=ApuGenOff_Ann,double,,0.000000,,,laminar/B738/annunciator/apu_gen_off_bus,exist,,,,0,,



dev=OVHDSIDEL

out=VhfNavSource,integer,,0.000000,,,laminar/B738/toggle_switch/vhf_nav_source,exist,,,,0,,

out=IrsSource,integer,,0.000000,,,laminar/B738/toggle_switch/irs_source,exist,,,,0,,

out=FmcSource,integer,,0.000000,,,laminar/B738/toggle_switch/fmc_source,exist,,,,0,,

out=SourceAuto,integer,,0.000000,,,laminar/B738/toggle_switch/dspl_source,exist,,,,0,,

out=ControlSource,integer,,0.000000,,,laminar/B738/toggle_switch/dspl_ctrl_pnl,exist,,,,0,,

out=WHeatLSide,integer,,0.000000,,,laminar/B738/ice/window_heat_l_side_pos,exist,,,,0,,

out=WHeatLFwd,integer,,0.000000,,,laminar/B738/ice/window_heat_l_fwd_pos,exist,,,,0,,

out=WHeatRSide,integer,,0.000000,,,laminar/B738/ice/window_heat_r_side_pos,exist,,,,0,,

out=WHeatRFwd,integer,,0.000000,,,laminar/B738/ice/window_heat_r_fwd_pos,exist,,,,0,,

out=AltFlap,integer,,0.000000,,,laminar/B738/switches/alt_flaps_pos,exist,,,,0,,

out=AltFlapCover,integer,,0.000000,,,laminar/B738/switches/alt_flaps_cover_pos,exist,0,,,0,,

out=WiperL,integer,,0.000000,,,laminar/B738/switches/left_wiper_pos,exist,,,,0,,

out=WiperR,integer,,0.000000,,,laminar/B738/switches/right_wiper_pos,exist,,,,0,,

out=FltContrA,double,,0.000000,,,laminar/B738/switches/flt_ctr_A_cover_pos,exist,,,,0,,

out=FltContrB,double,,0.000000,,,laminar/B738/switches/flt_ctr_B_cover_pos,exist,,,,0,,

out=SpoilerA,double,,0.000000,,,laminar/B738/switches/spoiler_A_cover_pos,exist,,,,0,,

out=SpoilerB,double,,0.000000,,,laminar/B738/switches/spoiler_B_cover_pos,exist,,,,0,,

out=YawDamper,integer,,0.000000,,,laminar/B738/toggle_switch/yaw_dumper_pos,exist,,,,0,,

out=EquipCool_S,integer,,0.000000,,,laminar/B738/toggle_switch/eq_cool_supply,exist,,,,0,,

out=EquipCool_E,integer,,0.000000,,,laminar/B738/toggle_switch/eq_cool_exhaust,exist,,,,0,,



dev=OVHDUP

out=IRS_L,integer,,0.000000,,,laminar/B738/toggle_switch/irs_left,exist,,,,0,,

out=IRS_R,integer,,0.000000,,,laminar/B738/toggle_switch/irs_right,exist,,,,0,,

out=IrsL_Alig,double,,0.000000,,,laminar/B738/irs/alignment_left_remain,exist,,,,0,,

out=IrsR_Alig,double,,0.000000,,,laminar/B738/irs/alignment_right_remain,exist,,,,0,,

out=IrsAlignment,integer,,0.000000,,,,,,,,0,,

logic:

calc=[SYSTEMS.OVHDUP.IrsL_Alig]+[SYSTEMS.OVHDUP.IrsR_Alig]

out=EltSW,integer,,0.000000,,,laminar/B738/toggle_switch/elt,exist,,,,0,,

out=EltCover,double,,0.000000,,,laminar/B738/button_switch/cover_position[8],exist,,,,0,,

out=ServiceInter,integer,,0.000000,,,laminar/B738/toggle_switch/service_interphone,exist,,,,0,,

out=PassOxyCover,integer,,0.000000,,,laminar/B738/button_switch/cover_position[7],exist,,,,0,,

out=FlightRecor,integer,,0.000000,,,laminar/B738/switches/fdr_pos,exist,,,,0,,

out=FlightRecorCover,double,,0.000000,,,laminar/B738/switches/fdr_cover_pos,exist,,,,0,,



dev=OVHDSIDER

out=WiperRSW,integer,,0.000000,,,AirbusFBW/RightWiperSwitch,exist,,,,0,,

out=PressModeSel,integer,,0.000000,,,laminar/B738/pressurization_mode,exist,,,,0,,

out=VoiceRecorder,integer,,0.000000,,,laminar/B738/toggle_switch/vcr,exist,,,,0,,

